MPlayer - Odtwarzacz filmów dla LINUKSA

Table of Contents

MPlayer - Odtwarzacz filmów dla LINUKSA................................................................................................1 http://www.mplayerhq.hu........................................................................................................................1 Jak czytaæ tê dokumentacjê.....................................................................................................................5 Rozdzia³ 1. Wprowadzenie......................................................................................................................5 WA¯NE..............................................................................................................................................6 1.1. History..............................................................................................................................................7 1.2. Installation........................................................................................................................................8 1.2.1. Software requirements.............................................................................................................9 1.2.2. Codecs.....................................................................................................................................9 Notatka............................................................................................................................................10 1.2.3. Video cards............................................................................................................................10 1.2.4. Sound cards...........................................................................................................................12 1.2.5. Features.................................................................................................................................12 1.3. What about the GUI?......................................................................................................................13 1.4. Subtitles and OSD...........................................................................................................................13 1.4.1. MPlayer's own subtitle format (MPsub)................................................................................14 1.4.2. Installing OSD and subtitles..................................................................................................15 1.4.3. OSD menu.............................................................................................................................16 Notatka............................................................................................................................................16 1.5. RTC.................................................................................................................................................16 Notatka............................................................................................................................................17 Rozdzia³ 2. Mo¿liwo¶ci.........................................................................................................................17 2.1. Obs³ugiwane formaty......................................................................................................................19 2.1.1. Formaty video........................................................................................................................19 Notatka............................................................................................................................................20 Notatka............................................................................................................................................21 2.1.2. Formaty audio........................................................................................................................23 2.2. Supported codecs............................................................................................................................24 2.2.1. Video codecs.........................................................................................................................24 Notatka............................................................................................................................................25 Notatka............................................................................................................................................26 Notatka............................................................................................................................................27 Notatka............................................................................................................................................28 Notatka............................................................................................................................................29 2.2.2. Audio codecs.........................................................................................................................29 2.2.3. Win32 codecs importing HOWTO........................................................................................31 Notatka............................................................................................................................................32 Notatka............................................................................................................................................32 Notatka............................................................................................................................................33 2.3. Urz±dzenia wyj¶ciowe...................................................................................................................33 2.3.1. Video output devices.............................................................................................................33 Notatka............................................................................................................................................34 Notatka............................................................................................................................................35 Security risk.....................................................................................................................................37 Notatka............................................................................................................................................40 Notatka............................................................................................................................................40 Notatka............................................................................................................................................41 Ostrze¿enie......................................................................................................................................41

MPlayer - Odtwarzacz filmów dla LINUKSA

Table of Contents

MPlayer - Odtwarzacz filmów dla LINUKSA Notatka............................................................................................................................................44 WA¯NE............................................................................................................................................45 Notatka............................................................................................................................................49 WA¯NE............................................................................................................................................54 2.3.2. Urz±dzenia wyj¶ciowe audio................................................................................................57 Notatka............................................................................................................................................66 Notatka............................................................................................................................................67 2.4. Wej¶cie TV.....................................................................................................................................68 2.4.1. Kompilacja............................................................................................................................69 2.4.2. Wskazówki u¿ytkowania.......................................................................................................69 2.4.3. Przyk³ady...............................................................................................................................70 2.5. Edit Decision Lists (EDL)..............................................................................................................71 2.5.1. Using an EDL file..................................................................................................................71 2.5.2. Making an EDL file...............................................................................................................71 Rozdzia³ 3. Sposób u¿ycia.....................................................................................................................71 3.1. Linia poleceñ...................................................................................................................................72 3.2. Sterowanie.......................................................................................................................................73 3.2.1. Konfiguracja sterowania........................................................................................................73 3.2.2. Sterowanie poprzez LIRC.....................................................................................................76 3.2.3. Tryb s³ugi..............................................................................................................................77 3.3. Strumieniowanie z sieci i potoków.................................................................................................77 Notatka............................................................................................................................................77 3.4. Strumienie zdalne............................................................................................................................77 3.4.1. Kompilacja serwera...............................................................................................................77 3.4.2. U¿ywanie strumieni zdalnych...............................................................................................77 Rozdzia³ 4. Frequently Asked Questions...............................................................................................78 4.1. Development............................................................................................................................81 4.2. Compilation..............................................................................................................................81 4.3. General questions.....................................................................................................................83 4.4. Playback problems...................................................................................................................85 4.5. Video/audio driver problems (vo/ao).......................................................................................87 Ostrze¿enie......................................................................................................................................87 4.6. DVD playback..........................................................................................................................88 4.7. Feature requests........................................................................................................................88 4.8. Encoding...................................................................................................................................88 Rozdzia³ 5. U¿ywanie CD/DVD............................................................................................................89 5.1. Napêdy CD/DVD............................................................................................................................89 5.2. Odtwarzanie DVD..........................................................................................................................90 Notatka............................................................................................................................................91 5.3. Odtwarzanie VCD...........................................................................................................................93 Notatka............................................................................................................................................93 Rozdzia³ 6. Porty....................................................................................................................................94 6.1. Linux...............................................................................................................................................94 6.1.1. Pakiety Debiana.....................................................................................................................94 6.1.2. Pakiety RPM..........................................................................................................................94 6.1.3. ARM......................................................................................................................................95 6.2. *BSD...............................................................................................................................................95

MPlayer - Odtwarzacz filmów dla LINUKSA

Table of Contents

MPlayer - Odtwarzacz filmów dla LINUKSA 6.2.1. FreeBSD................................................................................................................................95 6.2.2. OpenBSD...............................................................................................................................95 6.2.3. Darwin...................................................................................................................................95 6.3. Sun Solaris......................................................................................................................................95 6.4. Silicon Graphics Irix.......................................................................................................................97 6.5. QNX................................................................................................................................................97 6.6. Windows.........................................................................................................................................97 6.6.1. Cygwin..................................................................................................................................98 6.6.2. MinGW..................................................................................................................................98 6.7. Mac OS...........................................................................................................................................99 6.8. HP UX.............................................................................................................................................99 6.9. Amiga/MorphOS (zabawki dla zapaleñców)..................................................................................99 Rozdzia³ 7. Encoding with MEncoder...................................................................................................99 7.1. Encoding 2 or 3-pass MPEG-4 ("DivX")....................................................................................100 7.2. Encoding to MPEG format...........................................................................................................101 7.3. Rescaling movies..........................................................................................................................101 7.4. Stream copying.............................................................................................................................101 7.5. Fixing AVIs with broken index or interleaving............................................................................102 7.5.1. Appending multiple AVI files.............................................................................................102 Notatka..........................................................................................................................................102 7.6. Encoding with the libavcodec codec family.................................................................................102 7.7. Encoding from multiple input image files (JPEGs,PNGs or TGAs)............................................103 Notatka..........................................................................................................................................103 7.8. Extracting DVD subtitles to Vobsub file......................................................................................104 7.9. Preserving aspect ratio..................................................................................................................104 7.10. Custom inter/intra matrices.........................................................................................................105 Dodatek A. Listy mailingowe..............................................................................................................105 Notatka..........................................................................................................................................106 Dodatek B. Jak zg³aszaæ b³êdy...........................................................................................................107 B.1. Jak poprawiaæ b³êdy....................................................................................................................107 B.2. Jak zg³aszaæ b³êdy.......................................................................................................................107 B.3. Gdzie zg³aszaæ b³êdy...................................................................................................................108 B.4. Co zg³aszaæ..................................................................................................................................108 B.4.1. Informacja o systemie operacyjnym...................................................................................108 B.4.2. Sprzêt i sterowniki..............................................................................................................109 B.4.3. Problemy z konfiguracj±....................................................................................................109 B.4.4. Problemy z kompilacj±.......................................................................................................109 B.4.5. Problemy z odtwarzaniem..................................................................................................110 B.4.6. Awarie programu (ang. Crashes)........................................................................................110 B.5. Wiem co robiê..............................................................................................................................111 Dodatek C. Znane b³êdy......................................................................................................................111 C.1. Specjalne systemowe/specyficzne dla procesora b³êdy/problemy...............................................112 C.2. Ró¿ne problemy z synchronizacj± A-V i d¼wiêkiem................................................................112 C.2.1. Ogólne opó¼nienie audio lub "d³awi±cy siê" d¼wiêk (wystêpuje przy wszystkich lub wielu plikach)........................................................................................................................112 C.2.2. Opó¼nienia/desynchronizacja d¼wiêku specyficzne dla jednego lub kilku plików.........113 C.2.3. Zupe³ny brak d¼wiêku.......................................................................................................113

MPlayer - Odtwarzacz filmów dla LINUKSA

Table of Contents

MPlayer - Odtwarzacz filmów dla LINUKSA C.2.4. Zupe³ny brak obrazu (jedynie puste, szare lub zielone okno)............................................113 C.2.5. Problemy z wyj¶ciem video...............................................................................................114 Dodatek D. Format skórki MPlayera...................................................................................................114 D.1. Wstêp...........................................................................................................................................115 D.1.1. Katalogi..............................................................................................................................115 D.1.2. Formaty obrazków..............................................................................................................115 D.1.3. Sk³adniki skórki..................................................................................................................115 Notatka..........................................................................................................................................116 D.1.4. Pliki.....................................................................................................................................116 D.2. Plik skin.......................................................................................................................................117 D.2.1. Okno g³ówne i panel odtwarzania......................................................................................118 Notatka..........................................................................................................................................118 Ostrze¿enie....................................................................................................................................118 Notatka..........................................................................................................................................119 Notatka..........................................................................................................................................121 D.2.2. Okno ekranu.......................................................................................................................121 D.2.3. Menu skórki........................................................................................................................121 D.3. Czcionki.......................................................................................................................................121 D.3.1. Znaki specjalne (symbole)..................................................................................................122 D.4. Sygna³y GUI................................................................................................................................122 Notatka..........................................................................................................................................122 Dodatek E. Developer cries.................................................................................................................125 E.1. GCC 2.96......................................................................................................................................125 E.2. Binary distribution........................................................................................................................126 E.3. nVidia...........................................................................................................................................126 E.4. Joe Barr.........................................................................................................................................126 Dodatek F. Jak przesy³aæ poprawki (patche)......................................................................................127

MPlayer - Odtwarzacz filmów dla LINUKSA

MPlayer - Odtwarzacz filmów dla LINUKSA

http://www.mplayerhq.hu

Copyright © 2000-2003 Arpad Gereoffy (A'rpi/ESP-team)

Spis tre¶ci

Jak czytaæ tê dokumentacjê 1. Wprowadzenie

1.1. History 1.2. Installation

1.2.1. Software requirements 1.2.2. Codecs 1.2.3. Video cards

1.2.3.1. YUV cards 1.2.3.2. Non-YUV cards 1.2.3.3. Cirrus-Logic cards 1.2.4. Sound cards 1.2.5. Features 1.3. What about the GUI? 1.4. Subtitles and OSD 1.4.1. MPlayer's own subtitle format (MPsub) 1.4.2. Installing OSD and subtitles 1.4.3. OSD menu 1.5. RTC 2. Mo¿liwo¶ci

2.1. Obs³ugiwane formaty 2.1.1. Formaty video

2.1.1.1. Pliki MPEG 2.1.1.2. Pliki AVI 2.1.1.3. Pliki ASF/WMV 2.1.1.4. Pliki QuickTime/MOV 2.1.1.5. Pliki VIVO 2.1.1.6. Pliki FLI 2.1.1.7. Pliki RealMedia (RM) 2.1.1.8. Pliki NuppelVideo 2.1.1.9. pliki yuv4mpeg 2.1.1.10. Pliki FILM 2.1.1.11. Pliki RoQ 2.1.1.12. Pliki OGG/OGM 2.1.1.13. Pliki SDP 2.1.1.14. Pliki PVA 2.1.1.15. Pliki GIF 2.1.2. Formaty audio

2.1.2.1. Pliki MP3 2.1.2.2. Pliki WAV 2.1.2.3. Pliki OGG/OGM (Vorbis) 2.1.2.4. Pliki WMA/ASF

2.1.2.5. Pliki MP4 2.1.2.6. CD audio 2.1.2.7. XMMS 2.2. Supported codecs 2.2.1. Video codecs

2.2.1.1. DivX4/DivX5 2.2.1.2. FFmpeg/libavcodec 2.2.1.3. XAnim codecs 2.2.1.4. VIVO video 2.2.1.5. MPEG 1/2 video 2.2.1.6. MS Video1 2.2.1.7. Cinepak CVID 2.2.1.8. RealVideo 2.2.1.9. XviD 2.2.1.10. Sorenson 2.2.2. Audio codecs

2.2.2.1. Software AC3 decoding 2.2.2.2. Hardware AC3 decoding 2.2.2.3. libmad support 2.2.2.4. VIVO audio 2.2.2.5. RealAudio 2.2.2.6. QDesign codecs 2.2.2.7. Qualcomm codecs 2.2.2.8. AAC codec 2.2.3. Win32 codecs importing HOWTO 2.2.3.1. VFW codecs 2.2.3.2. DirectShow codecs 2.3. Urz±dzenia wyj¶ciowe 2.3.1. Video output devices

2.3.1.1. Setting up MTRR 2.3.1.2. Video outputs for traditional video cards 2.3.1.2.1. Xv 2.3.1.2.2. DGA 2.3.1.2.3. SDL 2.3.1.2.4. SVGAlib 2.3.1.2.5. Framebuffer output (FBdev) 2.3.1.2.6. Matrox framebuffer (mga_vid) 2.3.1.2.7. 3Dfx YUV support 2.3.1.2.8. OpenGL output 2.3.1.2.9. AAlib - text mode displaying 2.3.1.2.10. VESA - output to VESA BIOS 2.3.1.2.11. X11 2.3.1.2.12. VIDIX 2.3.1.2.13. DirectFB 2.3.1.2.14. DirectFB/Matrox (dfbmga) 2.3.1.3. MPEG decoders

2.3.1.3.1. DVB output and input 2.3.1.3.2. DXR2 2.3.1.3.3. DXR3/Hollywood+ 2.3.1.4. Other visualization hardware

2.3.1.4.1. Zr

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1.4.2. Blinkenlights 2.3.1.5. TV-out support

2.3.1.5.1. Matrox G400 cards 2.3.1.5.2. Matrox G450/G550 cards 2.3.1.5.3. ATI cards 2.3.1.5.4. Voodoo 3 2.3.1.5.5. nVidia 2.3.1.5.6. Neomagic 2.3.2. Urz±dzenia wyj¶ciowe audio 2.3.2.1. Synchronizacja Audio/Video 2.3.2.2. Do¶wiadczenia zwi±zane z u¿ytkowaniem kart d¼wiêkowych i zalecenia 2.3.2.3. Filtry audio

2.3.2.3.1. Zmniejszenie/Zwiêkszenie czêstotliwo¶ci próbkowania (Up/Downsampling) 2.3.2.3.2. Zmiana liczby kana³ów 2.3.2.3.3. Konwerter formatu próbek (sample format converter) 2.3.2.3.4. Opó¼nienie (delay) 2.3.2.3.5. Programowa regulacja g³o¶no¶ci (software volume control) 2.3.2.3.6. Korektor (equalizer) 2.3.2.3.7. Filtr pan (panning filter) 2.3.2.3.8. Subwoofer 2.3.2.3.9. Dekoder d¼wiêku przestrzennego (Surround-sound decoder) 2.3.2.3.10. Audio Exporter 2.3.2.4. Wtyczki Audio (odradzane)

2.3.2.4.1. Zwiêkszanie/Zmniejszanie czêstotliwo¶ci próbkowania (up/downsampling) 2.3.2.4.2. Dekodowanie d¼wiêku przestrzennego 2.3.2.4.3. Konwerter formatu próbek (sample format converter) 2.3.2.4.4. Opó¼nianie 2.3.2.4.5. Programowa regulacja g³o¶no¶ci± (software volume control) 2.3.2.4.6. Extrastereo 2.3.2.4.7. Normalizator g³o¶no¶ci (volume normalizer) 2.4. Wej¶cie TV

2.4.1. Kompilacja 2.4.2. Wskazówki u¿ytkowania 2.4.3. Przyk³ady 2.5. Edit Decision Lists (EDL)

2.5.1. Using an EDL file 2.5.2. Making an EDL file 3. Sposób u¿ycia 3.1. Linia poleceñ 3.2. Sterowanie

3.2.1. Konfiguracja sterowania 3.2.1.1. Nazwy klawiszy 3.2.1.2. Komendy 3.2.2. Sterowanie poprzez LIRC 3.2.3. Tryb s³ugi 3.3. Strumieniowanie z sieci i potoków 3.4. Strumienie zdalne

3.4.1. Kompilacja serwera 3.4.2. U¿ywanie strumieni zdalnych

MPlayer - Odtwarzacz filmów dla LINUKSA

4. Frequently Asked Questions 5. U¿ywanie CD/DVD

5.1. Napêdy CD/DVD 5.2. Odtwarzanie DVD 5.3. Odtwarzanie VCD 6. Porty

6.1. Linux

6.1.1. Pakiety Debiana 6.1.2. Pakiety RPM 6.1.3. ARM 6.2. *BSD

6.2.1. FreeBSD 6.2.2. OpenBSD 6.2.3. Darwin 6.3. Sun Solaris 6.4. Silicon Graphics Irix 6.5. QNX 6.6. Windows

6.6.1. Cygwin 6.6.2. MinGW 6.7. Mac OS 6.8. HP UX 6.9. Amiga/MorphOS (zabawki dla zapaleñców) 7. Encoding with MEncoder 7.1. Encoding 2 or 3-pass MPEG-4 ("DivX") 7.2. Encoding to MPEG format 7.3. Rescaling movies 7.4. Stream copying 7.5. Fixing AVIs with broken index or interleaving

7.5.1. Appending multiple AVI files 7.6. Encoding with the libavcodec codec family 7.7. Encoding from multiple input image files (JPEGs,PNGs or TGAs) 7.8. Extracting DVD subtitles to Vobsub file 7.9. Preserving aspect ratio 7.10. Custom inter/intra matrices A. Listy mailingowe B. Jak zg³aszaæ b³êdy

B.1. Jak poprawiaæ b³êdy B.2. Jak zg³aszaæ b³êdy B.3. Gdzie zg³aszaæ b³êdy B.4. Co zg³aszaæ

B.4.1. Informacja o systemie operacyjnym B.4.2. Sprzêt i sterowniki B.4.3. Problemy z konfiguracj± B.4.4. Problemy z kompilacj± B.4.5. Problemy z odtwarzaniem B.4.6. Awarie programu (ang. Crashes) B.4.6.1. Jak otrzymaæ informacjê o awarii B.4.6.2. Jak wyci±gn±æ sensowne informacjê ze zrzutu core (ang. core dump) B.5. Wiem co robiê...

C. Znane b³êdy

MPlayer - Odtwarzacz filmów dla LINUKSA

C.1. Specjalne systemowe/specyficzne dla procesora b³êdy/problemy C.2. Ró¿ne problemy z synchronizacj± A-V i d¼wiêkiem C.2.1. Ogólne opó¼nienie audio lub "d³awi±cy siê" d¼wiêk (wystêpuje przy wszystkich lub wielu plikach) C.2.2. Opó¼nienia/desynchronizacja d¼wiêku specyficzne dla jednego lub kilku plików C.2.3. Zupe³ny brak d¼wiêku C.2.4. Zupe³ny brak obrazu (jedynie puste, szare lub zielone okno) C.2.5. Problemy z wyj¶ciem video D. Format skórki MPlayera

D.1. Wstêp

D.1.1. Katalogi D.1.2. Formaty obrazków D.1.3. Sk³adniki skórki D.1.4. Pliki D.2. Plik skin

D.2.1. Okno g³ówne i panel odtwarzania D.2.2. Okno ekranu D.2.3. Menu skórki D.3. Czcionki

D.3.1. Znaki specjalne (symbole) D.4. Sygna³y GUI E. Developer cries

E.1. GCC 2.96 E.2. Binary distribution E.3. nVidia E.4. Joe Barr F. Jak przesy³aæ poprawki (patche)

Jak czytaæ tê dokumentacjê

Przy pierwszej instalacji powiniene¶ przeczytaæ wszystko od tego miejsca do koñca rozdzia³u Instalacja, ³±cznie z tekstami, do których s± tam odno¶niki. Je¶li masz jeszcze jakie¶ pytania, wróæ do Spisu tre¶ci i w nim poszukaj odpowiedniego tematu, przeczytaj FAQ albo spróbuj przegrepowaæ zbiory. Odpowied¼ na wiêkszo¶æ pytañ powinna byæ zawarta w niniejszej dokumentacji, a pozosta³e prawdopodobnie zosta³y ju¿ zadane na naszych listach mailingowych. Sprawd¼ archiwa, mo¿na tam znale¼æ wiele interesuj±cych informacji.

Rozdzia³ 1. Wprowadzenie

Spis tre¶ci

1.1. History 1.2. Installation

1.2.1. Software requirements 1.2.2. Codecs 1.2.3. Video cards

1.2.3.1. YUV cards 1.2.3.2. Non-YUV cards 1.2.3.3. Cirrus-Logic cards 1.2.4. Sound cards

MPlayer - Odtwarzacz filmów dla LINUKSA

Jak czytaæ tê dokumentacjê 5

1.2.5. Features 1.3. What about the GUI? 1.4. Subtitles and OSD

1.4.1. MPlayer's own subtitle format (MPsub) 1.4.2. Installing OSD and subtitles 1.4.3. OSD menu 1.5. RTC

MPlayer jest odtwarzaczem filmów dla Linuksa (dzia³a te¿ na wielu innych Uniksach i na procesorach nie-x86, patrz porty). Odtwarza wiêkszo¶æ zbiorów w formatach MPEG, VOB, AVI, OGG/OGM, VIVO, ASF/WMA/WMV, QT/MOV/MP4, FLI, RM, NuppelVideo, yuv4mpeg, FILM, RoQ, PVA, zbiory Matroska, obs³ugiwanych przez wiele rdzennych kodeków, XAnim, RealPlayer, i Win32 DLL. Mo¿esz w nim tak¿e ogl±daæ filmy VideoCD, SVCD, DVD, 3ivx, RealMedia, Sorenson, Theora i DivX (i wcale nie trzeba do tego biblioteki avifile!). Inn± wielk± zalet± MPlayera jest szeroki zakres obs³ugiwanych sterowników wyj¶ciowych. Dzia³a on z X11, Xv, DGA, OpenGL, SVGAlib, fbdev, AAlib, DirectFB, ale mo¿esz te¿ u¿ywaæ GGI i SDL (i dziêki temu wszystkich ich sterowników) i niektórych specyficznych dla kart graficznych sterowników niskiego poziomu (dla Matroxa, 3Dfxa, Radeona, Mach64, Permedia3)! Wiêkszo¶æ z nich obs³uguje skalowanie sprzêtowe lub programowe, wiêc filmy mo¿na ogl±daæ na pe³nym ekranie. MPlayer obs³uguje wy¶wietlanie przy u¿yciu niektórych sprzêtowych dekoderów MPEG, takich jak DVB i DXR3/Hollywood+. Nie mo¿na te¿ zapomnieæ o ³adnych, du¿ych, antyaliasowanych i cieniowanych napisach (10 obs³ugiwanych typów) z czcionkami europejskimi/ISO 8859-1,2 (polskimi, wêgierskimi, angielskimi, czeskimi, itp.), cyrylic±, koreañskimi i wy¶wietlaniem na ekranie (OSD)!

MPlayer jest doskona³y do odczytywania uszkodzonych plików MPEG (przydatne przy niektórych VCD), odtwarza równie¿ b³êdne pliki AVI, których nie mo¿na odczytaæ za pomoc± znanego odtwarzacza multimedialnego pod Windows. Nawet zbiory AVI bez bloku indeksowego mo¿na odtworzyæ i mo¿na zrekonstruowaæ ich indeks tymczasowo, u¿ywaj±c opcji -idx, albo trwale dziêki MEncoderowi, w ten sposób umo¿liwiaj±c sobie przeszukiwanie! Jak widaæ najwa¿niejsza jest tu stabilno¶æ i jako¶æ, ale szybko¶æ równie¿ jest zadziwiaj±ca.

MEncoder (Enkoder filmów MPlayera) jest to prosty enkoder filmów, zaprojektowany do kodowania odczytywalnych przez MPlayera filmów (AVI/ASF/OGG/DVD/VCD/VOB/MPG/MOV/VIV/FLI/RM/NUV/NET/PVA) na inne odczytywalne formaty (patrz ni¿ej). Mo¿e kodowaæ rozmaitymi kodekami video, takimi jak DivX4 (1 i 2 przebiegowy), libavcodec oraz audio PCM/MP3/VBR MP3. Ma te¿ potê¿ny system wtyczek do manipulacji obrazem.

Mo¿liwo¶ci MEncodera

Kodowanie z szerokiego zakresu formatów i dekoderów MPlayer • Kodowanie na wszystkie kodeki libavcodec z ffmpeg. • Kodowanie obrazu z tunerów kompatybilnych z V4L • Kodowanie/multipleksowanie przeplatanych zbiorów AVI z prawid³owymi indeksami • Tworzenie zbiorów z zewnêtrznego strumienia audio • Kodowanie 1, 2 lub 3-przej¶ciowe • D¼wiêk MP3 VBR

WA¯NE

D¼wiêk MP3 VBR w odtwarzaczach pod Windows nie zawsze brzmi przyjemnie!

•

D¼wiêk PCM • Kopiowanie strumieniowe •

MPlayer - Odtwarzacz filmów dla LINUKSA

Synchronizacja wej¶cia A/V (oparta na PTS, mo¿e byæ wy³±czona opcj± -mc 0) • Korekta FPS opcj± -ofps (przydatne gdy kodujesz 29.97 fps VOB na 24 fps AVI) • Mo¿liwo¶æ zastosowania naszego potê¿nego systemu wtyczek (kadrowanie, powiêkszanie, obracanie, postproces, skalowanie, konwersja rgb/yuv) • Mo¿liwo¶æ wkodowania DVD/VOBsub ORAZ napisów w zbiór wyj¶ciowy • Mo¿liwo¶æ zapisu napisów DVD do formatu Vobsub • Planowane mo¿liwo¶ci

Zwiêkszenie zakresu dostêpnych formatów/kodeków do (de)kodowania (tworzenie zbiorów VOB ze strumieniami DivX4/Indeo5/VIVO :). •

MPlayer i MEncoder mog± byæ rozprowadzane zgodnie z warunkami GNU General Public License Version 2. 1.1. History

This began a year ago... I have tried lots of players under linux (mtv, xmps, dvdview, livid/oms, videolan, xine, xanim, avifile, xmmp) but they all have some problem. Mostly with special files or with audio/video sync. Most of them are unable to play both MPEG1, MPEG2 and AVI (DivX) files. Many players have image quality or speed problems too. So I've decided to write/modify one...

A'rpi, 2001

mpg12play v0.1-v0.3: Sep 22-25, 2000

The first try, hacked together in a half hour! I've used libmpeg3 from http://www.heroinewarrior.com up to the version 0.3, but there were image quality and speed problems with it.

•

mpg12play v0.5-v0.87: Sep 28-Oct 20, 2000

Mpeg codec replaced with DVDview by Dirk Farin, it was a great stuff, but it was slow and was written in C++ (A'rpi hates C++!!!)

•

mpg12play v0.9-v0.95pre5: Oct 21-Nov 2, 2000

Mpeg codec was libmpeg2 (mpeg2dec) by Aaron Holtzman and Michel Lespinasse. It's great, optimized very fast C code with perfect image quality and 100% MPEG standard conformance.

•

MPlayer v0.3-v0.9: Nov 18-Dec 4, 2000

It was a pack of two programs: mpg12play v0.95pre6 and my new simple AVI player 'avip' based on avifile's Win32 DLL loader.

•

MPlayer v0.10: Jan 1, 2001

The MPEG and AVI player in a single binary! •

MPlayer v0.11pre series:

Some new developers joined and since 0.11 the MPlayer project is a team-work! Added ASF file support, and OpenDivX (see http://www.projectmayo.com) en/decoding.

•

MPlayer v0.17a "The IdegCounter" Apr 27, 2001 •

MPlayer - Odtwarzacz filmów dla LINUKSA

1.1. History 7

The release version of the 0.11pre after 4 months of heavy development! Try it, and be amazed! Thousands of new features added... and of course old code was improved too, bugs removed etc. MPlayer 0.18 "The BugCounter" Jul 9, 2001

2 months since 0.17 and here's a new release.. Completed ASF support, more subtitle formats, introduced libao (similar to libvo but to audio), even more stable than ever, and so on. It's a MUST!

•

MPlayer 0.50 "The Faszom(C)ounter" Oct 8, 2001

Hmm. Release again. Tons of new features, beta GUI version, bugs fixed, new vo and ao drivers, ported to many systems, including opensource DivX codecs and much more. Try it!

•

MPlayer 0.60 "The RTFMCounter" Jan 3, 2002

MOV/VIVO/RM/FLI/NUV fileformats support, native CRAM, Cinepak, ADPCM codecs, and support for XAnim's binary codecs; DVD subtitles support, first release of MEncoder, TV grabbing, cache, liba52, countless fixes.

•

MPlayer 0.90pre10 "The BirthdayCounter" Nov 11, 2002

Although this is not a release, I am going to mention it because it came out 2 years after MPlayer v0.01. Happy birthday, MPlayer!

•

MPlayer 0.90rc1 "The CodecCounter" Dec 7, 2002

Again not a release, but after adding Sorenson 3 (QuickTime) and Windows Media 9 support, MPlayer is the world's first movie player with support for all known video formats!

•

MPlayer 0.90 "The CounterCounter" Apr 6, 2003

After more than 1 year, we finally concluded that the code was indeed stable again, and ready to be published as a release. Unfortunately we forgot even to increase the version number, and other annoying bugs went in, so get ready for...

•

MPlayer 0.91 Aug 13, 2003

The above mentioned and lot of other bugs have been fixed. This is the latest stable version. •

MPlayer 1.0pre1 "Development on the beach" Sep 1, 2003

Although this is not a stable release, I am going to mention it because it is the first pre version of the 1.0 series of MPlayer and it is intended to help the big bug hunting party. This is a huge step forward!

•

MPlayer 1.0 date yet unknown • 1.2. Installation

A quick installation guide can be found in the README file. Please read it first and then come back here for the rest of the gory details.

In this section I'll try to guide you through the compiling and configuring process of MPlayer. It's not easy, but it won't necessarily be hard. If you experience a different behavior than what I explain, please search through this documentation and you'll find your answers. If you see links, please follow them and read carefully what they contain. It will take some time, but it IS worth it.

You need a fairly recent system. On Linux, 2.4.x kernels are recommended.

MPlayer - Odtwarzacz filmów dla LINUKSA

1.2. Installation 8

1.2.1. Software requirements

binutils - suggested version is 2.11.x. This program is responsible for generating MMX/ 3DNow!/etc instructions, thus very important. • gcc - suggested versions are: 2.95.3 (maybe 2.95.4) and 3.2+. Never use 2.96 or 3.0.x! They generate faulty code for MPlayer. If you decide to change gcc from 2.96, then don't decide in favor of 3.x just because it's newer! Early releases of 3.x were even more buggy than 2.96. So downgrade to 2.95.x (downgrade libstdc++ too, other programs may need it) or don't up/downgrade at all (but in this case, be prepared for runtime problems). If you vote for 3.x, try to use the latest version, early releases had various bugs, so be sure you use at least 3.1, it's tested and working. For detailed information about gcc 2.96's bugs (that are still NOT fixed, they have been WORKED AROUND in MPlayer!),see the gcc 2.96 section and the FAQ.

•

XFree86 - suggested version is always the newest (4.3). Normally, everyone wants this, as starting with XFree86 4.0.2, it contains the XVideo extension (somewhere referred to as Xv) which is needed to enable the hardware YUV acceleration (fast image display) on cards that support it. Make sure its development package is installed, too, otherwise it won't work. For some video cards you don't need XFree86. See list below.

•

make - suggested version is always the newest (at least 3.79.x). This usually isn't important. • SDL - it's not mandatory, but can help in some cases (bad audio, video cards that lag strangely with the xv driver). Always use the newest (beginning from 1.2.x). • libjpeg - optional JPEG decoder, used by the -mf option and some QT MOV files. Useful for both MPlayer and MEncoder if you plan to work with jpeg files. • libpng - recommended and default (M)PNG decoder. Required for GUI. Useful for both MPlayer and MEncoder. • lame - recommended, needed for encoding MP3 audio with MEncoder, suggested version is always the newest (at least 3.90). • zlib - recommended, necessary for compressed MOV header and PNG support. • libogg - optional, needed for playing OGG file format. • libvorbis - optional, needed for playing OGG Vorbis audio. • LIVE.COM Streaming Media - optional, needed for playing RTSP/RTP streams. • directfb - optional, from http://www.directfb.org • cdparanoia - optional, for CDDA support • libfreetype - optional, for TTF fonts support. At least 2.0.9 is required. • libxmms - optional, for XMMS input plugin support. At least 1.2.7 is required. • libsmb - optional, for Samba support. • 1.2.2. Codecs

libavcodec: This codec package is capable of decoding H263/MJPEG/RV10/DivX3/DivX4/DivX5/MP41/MP42/WMV1/WMV2/SVQ1/SVQ3 encoded video streams and WMA (Windows Media Audio) v1/v2 audio streams, on multiple platforms. It is also known to be the fastest for this task. See FFmpeg section for details. Features:

gain decoding of videos mentioned above, on non-x86 machines ♦ encoding with most of the mentioned codecs ♦ this codec is the fastest codec available for DivX/3/4/5 and other MPEG4 types. Recommended! ♦

•

Win32 codecs: If you plan to use MPlayer on x86 architecture, you will possibly need them. Download the Win32 codecs from our codecs page and install them to /usr/local/lib/codecs BEFORE compiling MPlayer, otherwise no Win32 support will be compiled! •

MPlayer - Odtwarzacz filmów dla LINUKSA

1.2.1. Software requirements 9

Notatka

The avifile project has similar codecs package, but it differs from ours, so if you want to use all supported codecs, then use our package (do not worry, avifile works with it without problems).

Features:

you need this if you want to play or encode for example movies recorded with various hardware compressors, like tuner cards, digital cameras (example: DV, ATI VCR, MJPEG) ♦ needed if you want to play WMV9/WMA9 movies. ♦ Not needed for old ASF's with MP41 or MP42 video (though VoxWare audio is frequent for these files - it's done by the Win32 codec), or WMV7. Also not needed for WMA (Windows Media Audio), libavcodec has opensource decoder for that. ♦

QuickTime codecs: on x86 platforms these codecs can be used to decode RPZA, and other QuickTime video, and QDesign audio streams. Installation instructions can be found in the Sorenson video codec section. •

DivX4/DivX5: information about this codec is available in the DivX4/DivX5 section. You possibly don't want this codec as libavcodec (see above) is much faster and has better quality than this, for both decoding and encoding. Features:

1 pass or 2 pass encoding with MEncoder ♦ can play old DivX3 movies much faster than the Win32 DLL but slower than libavcodec! ♦ it's closed-source, and only a x86 version is available. ♦

•

XviD: Open source encoding alternative to Divx4Linux. Features:

1 pass or 2 pass encoding with MEncoder ♦ it's open-source, so it's multiplatform. ♦ it's about 2 times faster than divx4 when encoding - about the same quality ♦

•

The XAnim codecs are the best (full screen, hardware YUV zoom) for decoding 3ivx and Indeo 3/4/5 movies, and some old formats. And they are multiplatform, so this is the only way to play Indeo on non-x86 platforms (well, apart from using XAnim:). But for example Cinepak movies are best played with MPlayer's own Cinepak decoder!

•

For Ogg Vorbis audio decoding you need to install libvorbis properly. Use deb/rpm packages if available, or compile from source (this is a nightly updated tarball of Vorbis CVS). • MPlayer can use the libraries of RealPlayer 8 or RealONE to play files with RealVideo 2.0-4.0 video, and Sipro/Cook audio. See RealMedia file format section for installation instructions and more information. •

1.2.3. Video cards

There are generally two kind of video cards. One kind (the newer cards) has hardware scaling and YUV acceleration support, the other cards don't.

1.2.3.1. YUV cards

They can display and scale (zoom) the picture to any size that fits in their memory, with small CPU usage (even when zooming), thus fullscreen is nice and very fast.

Matrox G200/G400/G450/G550 cards: although a Vidix driver is provided, it is recommended to use the mga_vid module instead, for it works much better. Please see the mga_vid section about its installation and usage. It is important to do these steps before compiling MPlayer, otherwise no mga_vid support will be built. Also check out the Matrox TV-out section. If you don't use Linux,

•

MPlayer - Odtwarzacz filmów dla LINUKSA your only possibility is the VIDIX driver: read the VIDIX section. 3Dfx Voodoo3/Banshee cards: please see tdfxfb section in order to gain big speedup. It is important to do these steps before compiling MPlayer, otherwise no 3Dfx support will be built. Also see the 3dfx TV-out section. If you use X, use at least 4.2.0, as 3dfx Xv driver was broken in 4.1.0, and earlier releases.

•

ATI cards: VIDIX driver is provided for the following cards: Radeon, Rage128, Mach64 (Rage XL/Mobility, Xpert98). Also see the ATI cards section of the TV-out documentation, to know if you card's TV-out is supported under Linux/MPlayer. •

S3 cards: the Savage and Virge/DX chips have hardware acceleration. Use as new XFree86 version as possible, older drivers are buggy. Savage chips have problems with YV12 display, see S3 Xv section for details. Older, Trio cards have no, or slow hardware support. •

nVidia cards: may or may not be good choice for video playing. If you do not have a GeForce2 (or newer) card, it's not likely to work without bugs. the built-in nVidia driver in XFree86 does not support hardware YUV acceleration on all nVidia cards. You have to download nVidia's closed-source drivers from nVidia.com. See the nVidia Xv driver section for details. Please also check the nVidia TV-out section if you wish to use a TV.

•

3DLabs GLINT R3 and Permedia3: a VIDIX driver is provided (pm3_vid). Please see the VIDIX section for details. • Other cards: none of the above?

Try if the XFree86 driver (and your card) supports hardware acceleration. See the Xv section for details. ♦ If it doesn't, then your card's video features aren't supported under your operating system :( If hardware scaling works under Windows, it doesn't mean it will work under Linux or other operating system, it depends on the drivers. Most manufacturers neither make Linux drivers nor release specifications of their chips - so you are unlucky if using their cards. See Non-YUV cards.

♦

•

1.2.3.2. Non-YUV cards

Fullscreen playing can be achieved by either enabling software scaling (use the -zoom or -vf option, but I warn you: this is slow), or switching to a smaller video mode, for example 352x288. If you don't have YUV acceleration, this latter method is recommended. Video mode switching can be enabled by using the -vm option and it works with the following drivers:

using XFree86: see details in DGA driver and X11 driver sections. DGA is recommended! Also try DGA via SDL, sometimes it's better. • not using XFree86: try the drivers in the following order: vesa, fbdev, svgalib, aalib. • 1.2.3.3. Cirrus-Logic cards

GD 7548: present on-board and tested in Compaq Armada 41xx notebook series.

XFree86 3: works in 8/16bpp modes. However, the driver is dramatically slow and buggy in 800x600@16bpp. Recommended: 640x480@16bpp ♦ XFree86 4: the Xserver freezes soon after start unless acceleration is disabled, but then the whole thing gets slower than XFree86 3. No XVideo. ♦ FBdev: framebuffer can be turned on with the clgenfb driver in the kernel, though for me it worked only in 8bpp, thus unusable. The clgenfb source had to be extended with the 7548 ID before compilation. ♦

VESA: the card is only VBE 1.2 capable, so VESA output can't be used. Can't be workarounded with UniVBE. ♦ SVGAlib: detects an older Cirrus chip. Usable but slow with -bpp 8. ♦

•

MPlayer - Odtwarzacz filmów dla LINUKSA

1.2.3. Video cards 11

1.2.4. Sound cards

Soundblaster Live!: with this card you can use 4 or 6 (5.1) channels AC3 decoding instead of 2. Read the Software AC3 decoding section. For hardware AC3 passthrough you must use ALSA 0.9 with OSS emulation! •

C-Media with SP/DIF out: hardware AC3 passthrough is possible with these cards, see Hardware AC3 decoding section. • Features of other cards aren't supported by MPlayer. It's very recommended to read the sound card section! • 1.2.5. Features

Decide if you need GUI. If you do, see the GUI section before compiling. • If you want to install MEncoder (our great all-purpose encoder), see the MEncoder section. • If you have a V4L compatible TV tuner card, and wish to watch/grab and encode movies with MPlayer, read the TV input section. • There is a neat OSD Menu support ready to be used. Check the OSD menu section. • Then build MPlayer:

./configure
make
make install

At this point, MPlayer is ready to use. The directory $PREFIX/share/mplayer contains the

codecs.conf file, which is used to tell the program all the codecs and their capabilities. This file is needed

only when you want to change its properties, as the main binary contains an internal copy of it. Check if you have codecs.conf in your home directory (~/.mplayer/codecs.conf) left from old MPlayer versions, and remove it.

Note that if you have a codecs.conf in ~/.mplayer/, the builtin and system codecs.conf will be ignored completely. Do not do this unless you want to fiddle with MPlayer internals as this can can cause many problems. If you want to change the codecs search order, use the -vc, -ac, -vfm, or -afm options either on the command line or in your config file (see the manual page).

Debian users can build a .deb package for themselves, it's very simple. Just exec

fakeroot debian/rules binary

in MPlayer's root directory. See Debian packaging for detailed instructions.

Always browse the output of ./configure, and the configure.log file, they contain information about what will be built, and what will not. You may also want to view config.h and config.mak files. If you have some libraries installed, but not detected by ./configure, then check if you also have the proper header files (usually the -dev packages) and their version matches. The configure.log file usually tells you what is missing.

Though not mandatory, the fonts should be installed in order to gain OSD, and subtitle functionality. The recommended method is installing a TTF font file and telling MPlayer to use it. See the Subtitles and OSD section for details.

MPlayer - Odtwarzacz filmów dla LINUKSA

1.2.4. Sound cards 12

1.3. What about the GUI?

The GUI needs GTK 1.2.x (it isn't fully GTK, but the panels are). The skins are stored in PNG format, so GTK, libpng (and their devel stuff, usually called gtk-dev and libpng-dev) has to be installed. You can build it by specifying --enable-gui during ./configure. Then, to turn on GUI mode, you have to execute the gmplayer binary.

Currently you can't use the -gui option on the command line, due to technical reasons.

As MPlayer doesn't have a skin included, you have to download them if you want to use the GUI. See the download page. They should be extracted to the usual system-wide directory ($PREFIX/share/mplayer/Skin), or to $HOME/.mplayer/Skin. MPlayer by default looks in these directories for a directory named default, but you can use the -skin newskin option, or the

skin=newskin config file directive to use the skin in */Skin/newskin directory.

1.4. Subtitles and OSD

MPlayer can display subtitles along with movie files. Currently the following formats are supported:

VobSub • OGM • CC (closed caption) • MicroDVD • SubRip • SubViewer • Sami • VPlayer • RT • SSA • MPsub • AQTitle • JACOsub • MPlayer can dump the previously listed subtitle formats (except the three first) into the following destination formats, with the given options:

MPsub: -dumpmpsub • SubRip: -dumpsrtsub • MicroDVD: -dumpmicrodvdsub • JACOsub: -dumpjacosub • Sami: -dumpsami • MEncoder can dump DVD subtitles into VobSub format.

The command line options differ slightly for the different formats:

VobSub subtitles. VobSub subtitles consist of a big (some megabytes) .SUB file, and optional .IDX and/or

.IFO files. If you have files like sample.sub, sample.ifo (optional), sample.idx - you have to

pass MPlayer the -vobsub sample [-vobsubid id] options (full path optional). The -vobsubid option is like -sid for DVDs, you can choose between subtitle tracks (languages) with it. In case that

MPlayer - Odtwarzacz filmów dla LINUKSA

1.3. What about the GUI? 13

-vobsubid is omitted, MPLayer will try to use the languages given by the -slang option and fall back to

the langidx in the .IDX file to set the subtitle language. If it fails, there will be no subtitles.

Other subtitles. The other formats consist of a single text file containing timing, placement and text information. Usage: If you have a file like sample.txt, you have to pass the option -sub sample.txt (full path optional).

Adjusting subtitle timing and placement:

-subdelay sec

Delays subtitles by sec seconds. Can be negative.

-subfps RATE

Specify frame/sec rate of subtitle file (float number).

-subpos 0-100

Specify the position of subtitles.

If you experience a growing delay between the movie and the subtitles when using a MicroDVD subtitle file, most likely the frame rate of the movie and the subtitle file are different. Please note that the MicroDVD subtitle format uses absolute frame numbers for its timing, and therefore the -subfps option cannot be used with this format. As MPlayer has no way to guess the frame rate of the subtitle file, you have to manually convert the frame rate. There is a little perl script in the contrib directory of the MPlayer FTP site to do this conversion for you.

About DVD subtitles, read the DVD section.

1.4.1. MPlayer's own subtitle format (MPsub)

MPlayer introduces a new subtitle format called MPsub. It was designed by Gabucino. Basically its main feature is being dynamically time-based (although it has frame-based mode too). Example (from DOCS/tech/mpsub.sub):

FORMAT=TIME
# first number  : wait this much after previous subtitle disappeared
# second number : display the current subtitle for this many seconds

15 3
A long long, time ago...

0 3
in a galaxy far away...

0 3
Naboo was under an attack.

So you see, the main goal was to make subtitle editing/timing/joining/cutting easy. And, if you - say - get an SSA subtitle but it's badly timed/delayed to your version of the movie, you simply do a

mplayer dummy.avi -sub source.ssa -dumpmpsub

A dump.mpsub file will be created in the current directory, which will contain the source subtitle's text, but in MPsub format. Then you can freely add/subtract seconds to/from the subtitle.

MPlayer - Odtwarzacz filmów dla LINUKSA

1.4.1. MPlayer's own subtitle format (MPsub) 14

Subtitles are displayed with a technique called 'OSD', On Screen Display.OSD is used to display current time, volume bar, seek bar etc.

1.4.2. Installing OSD and subtitles

You need an MPlayer font package to be able to use OSD/SUB feature. There are many ways to get it:

Use the font generator tool at TOOLS/subfont-c. It's a complete tool to convert from TTF/Type1/etc font to mplayer font pkg (read TOOLS/subfont-c/README for details). • Use the font generator GIMP plugin at TOOLS/subfont-GIMP (note: you must have HSI RAW plugin too, see http://realtime.ssu.ac.kr/~lethean/mplayer/). • using a TrueType (TTF) font, by the means of the freetype library. Version 2.0.9 or greater is mandatory! Then you have two methods:

use the -font /path/to/sample_font.ttf option to specify a TrueType font file on every occasion ♦ create a symlink:

ln -s /path/to/sample_font.ttf ~/.mplayer/subfont.ttf

♦

•

If MPlayer was compiled with fontconfig support, the above methods won't work, instead the -font expects a fontconfig font name and defaults to the sans-serif font. To get a list of fonts known to

fontconfig, use fc-list. Example: -font 'Bitstream Vera Sans'

Download ready-to-use font packages from MPlayer site. Note: currently available fonts are limited for ISO 8859-1/2 support, but there are some other (including Korean, Russian, ISO 8859-8 etc) fonts at contrib/font section of FTP, made by users.

Font should have appropriate font.desc file which maps unicode font positions to the actual code page of the subtitles text. Other solution is to have subtitles encoded in UTF8 encoding and use -utf8 option or just name the subtitles file <video_name>.utf and have it in the same dir as the video file. Recoding from different codepages to UTF8 could be done by using konwert or iconv programs.

Tabela 1.1. Some URLs

URL Comment ftp://ftp.mplayerhq.hu/MPlayer/releases/fonts/ ISO fonts ftp://ftp.mplayerhq.hu/MPlayer/contrib/fonts/ various fonts by users

http://realtime.ssu.ac.kr/~lethean/mplayer/ Korean fonts and RAW plugin

•

If you chose non-TTF fonts, UNZIP the file you downloaded to ~/.mplayer or

$PREFIX/share/mplayer. Then rename or symlink one of the extracted directories to font, for

example:

ln -s ~/.mplayer/arial-24 ~/.mplayer/font

Now you have to see a timer at the upper left corner of the movie (switch it off with the o key).

(subtitles are always enabled, for disabling them please read the man page)

OSD has 4 states (switch with o):

MPlayer - Odtwarzacz filmów dla LINUKSA

1.4.2. Installing OSD and subtitles 15 volume bar + seek bar (default) 1. volume bar + seek bar + timer + file position percentage on seeking 2. volume bar + seek bar + timer + total duration of the media 3. subtitles only 4. You can change default behaviour by setting osdlevel variable in config file, or the -osdlevel command line option.

1.4.3. OSD menu

MPlayer has a completely user definiable OSD Menu interface.

Notatka

the Preferences menu is currently UNIMPLEMENTED!

Installation

compile MPlayer by passing the --enable-menu to ./configure 1. make sure you have an OSD font installed 2. copy etc/menu.conf to your .mplayer directory 3. copy etc/input.conf to your .mplayer directory, or to the system-wide MPlayer config dir (default: /usr/local/etc/mplayer) 4. check and edit input.conf to enable menu movement keys (it is described there). 5. start MPlayer by the following example:

$ mplayer -menu file.avi

6.

push any menu key you defined 7. 1.5. RTC

There are three timing methods in MPlayer.

To use the old method, you don't have to do anything. It uses usleep() to tune A/V sync, with +/- 10ms accuracy. However sometimes the sync has to be tuned even finer. • The new timer code uses PC's RTC (Real Time Clock) for this task, because it has precise 1ms timers. It is automagically enabled when available, but requires root privileges, a setuid root MPlayer binary or a properly set up kernel. If you are running kernel 2.4.19pre8 or later you can adjust the maximum RTC frequency for normal users through the /proc filesystem. Use this command to enable RTC for normal users:

echo 1024 > /proc/sys/dev/rtc/max-user-freq

If you do not have such a new kernel, you can also change one line in drivers/char/rtc.c and recompile your kernel. Find the section that reads

       * We don't really want Joe User enabling more
       * than 64Hz of interrupts on a multi-user machine.
       */
      if ((rtc_freq > 64) && (!capable(CAP_SYS_RESOURCE)))

•

MPlayer - Odtwarzacz filmów dla LINUKSA

1.4.3. OSD menu 16 and change the 64 to 1024. You should really know what you are doing, though. You can see the new timer's efficiency in the status line. The power management functions of some notebook BIOSes with speedstep CPUs interact badly with RTC. Audio and video may get out of sync. Plugging the external power connector in before you power up your notebook seems to help. You can always turn off RTC support with the -nortc option. In some hardware combinations (confirmed during usage of non-DMA DVD drive on an ALi1541 board) usage of the RTC timer causes skippy playback. It's recommended to use the third method in these cases.

The third timer code is turned on with the -softsleep option. It has the efficiency of the RTC, but it doesn't use RTC. On the other hand, it requires more CPU. • Notatka

NEVER install a setuid root MPlayer binary on a multiuser system! It's a clear way for everyone to become root.

Rozdzia³ 2. Mo¿liwo¶ci

Spis tre¶ci

2.1. Obs³ugiwane formaty

2.1.1. Formaty video

2.1.1.1. Pliki MPEG 2.1.1.2. Pliki AVI 2.1.1.3. Pliki ASF/WMV 2.1.1.4. Pliki QuickTime/MOV 2.1.1.5. Pliki VIVO 2.1.1.6. Pliki FLI 2.1.1.7. Pliki RealMedia (RM) 2.1.1.8. Pliki NuppelVideo 2.1.1.9. pliki yuv4mpeg 2.1.1.10. Pliki FILM 2.1.1.11. Pliki RoQ 2.1.1.12. Pliki OGG/OGM 2.1.1.13. Pliki SDP 2.1.1.14. Pliki PVA 2.1.1.15. Pliki GIF 2.1.2. Formaty audio

2.1.2.1. Pliki MP3 2.1.2.2. Pliki WAV 2.1.2.3. Pliki OGG/OGM (Vorbis) 2.1.2.4. Pliki WMA/ASF 2.1.2.5. Pliki MP4 2.1.2.6. CD audio 2.1.2.7. XMMS 2.2. Supported codecs

2.2.1. Video codecs

2.2.1.1. DivX4/DivX5 2.2.1.2. FFmpeg/libavcodec 2.2.1.3. XAnim codecs 2.2.1.4. VIVO video

MPlayer - Odtwarzacz filmów dla LINUKSA

2.2.1.5. MPEG 1/2 video 2.2.1.6. MS Video1 2.2.1.7. Cinepak CVID 2.2.1.8. RealVideo 2.2.1.9. XviD 2.2.1.10. Sorenson 2.2.2. Audio codecs

2.2.2.1. Software AC3 decoding 2.2.2.2. Hardware AC3 decoding 2.2.2.3. libmad support 2.2.2.4. VIVO audio 2.2.2.5. RealAudio 2.2.2.6. QDesign codecs 2.2.2.7. Qualcomm codecs 2.2.2.8. AAC codec 2.2.3. Win32 codecs importing HOWTO 2.2.3.1. VFW codecs 2.2.3.2. DirectShow codecs 2.3. Urz±dzenia wyj¶ciowe 2.3.1. Video output devices

2.3.1.1. Setting up MTRR 2.3.1.2. Video outputs for traditional video cards 2.3.1.2.1. Xv 2.3.1.2.2. DGA 2.3.1.2.3. SDL 2.3.1.2.4. SVGAlib 2.3.1.2.5. Framebuffer output (FBdev) 2.3.1.2.6. Matrox framebuffer (mga_vid) 2.3.1.2.7. 3Dfx YUV support 2.3.1.2.8. OpenGL output 2.3.1.2.9. AAlib - text mode displaying 2.3.1.2.10. VESA - output to VESA BIOS 2.3.1.2.11. X11 2.3.1.2.12. VIDIX 2.3.1.2.13. DirectFB 2.3.1.2.14. DirectFB/Matrox (dfbmga) 2.3.1.3. MPEG decoders

2.3.1.3.1. DVB output and input 2.3.1.3.2. DXR2 2.3.1.3.3. DXR3/Hollywood+ 2.3.1.4. Other visualization hardware

2.3.1.4.1. Zr 2.3.1.4.2. Blinkenlights 2.3.1.5. TV-out support

2.3.1.5.1. Matrox G400 cards 2.3.1.5.2. Matrox G450/G550 cards 2.3.1.5.3. ATI cards 2.3.1.5.4. Voodoo 3 2.3.1.5.5. nVidia 2.3.1.5.6. Neomagic 2.3.2. Urz±dzenia wyj¶ciowe audio

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.2.1. Synchronizacja Audio/Video 2.3.2.2. Do¶wiadczenia zwi±zane z u¿ytkowaniem kart d¼wiêkowych i zalecenia 2.3.2.3. Filtry audio

2.3.2.3.1. Zmniejszenie/Zwiêkszenie czêstotliwo¶ci próbkowania (Up/Downsampling) 2.3.2.3.2. Zmiana liczby kana³ów 2.3.2.3.3. Konwerter formatu próbek (sample format converter) 2.3.2.3.4. Opó¼nienie (delay) 2.3.2.3.5. Programowa regulacja g³o¶no¶ci (software volume control) 2.3.2.3.6. Korektor (equalizer) 2.3.2.3.7. Filtr pan (panning filter) 2.3.2.3.8. Subwoofer 2.3.2.3.9. Dekoder d¼wiêku przestrzennego (Surround-sound decoder) 2.3.2.3.10. Audio Exporter 2.3.2.4. Wtyczki Audio (odradzane)

2.3.2.4.1. Zwiêkszanie/Zmniejszanie czêstotliwo¶ci próbkowania (up/downsampling) 2.3.2.4.2. Dekodowanie d¼wiêku przestrzennego 2.3.2.4.3. Konwerter formatu próbek (sample format converter) 2.3.2.4.4. Opó¼nianie 2.3.2.4.5. Programowa regulacja g³o¶no¶ci± (software volume control) 2.3.2.4.6. Extrastereo 2.3.2.4.7. Normalizator g³o¶no¶ci (volume normalizer) 2.4. Wej¶cie TV

2.4.1. Kompilacja 2.4.2. Wskazówki u¿ytkowania 2.4.3. Przyk³ady 2.5. Edit Decision Lists (EDL)

2.5.1. Using an EDL file 2.5.2. Making an EDL file

2.1. Obs³ugiwane formaty

Na pocz±tek wa¿ne jest wyja¶nienie pewnego czêsto pope³nianego b³êdu. Kiedy ludzie widz± plik o rozszerzeniu .AVI, automatycznie stwierdzaj±, ¿e to nie jest plik MPEG. Nie jest to prawda. Przynajmniej niezupe³nie. W przeciwieñstwie do popularnego stwierdzenia, plik taki mo¿e zawieraæ video MPEG1.

Widzisz, kodek to nie to samo, co format pliku. Przyk³ady kodeków video: MPEG1, MPEG2, DivX, Indeo5, 3vix. Przyk³ady formatów plików: MPG, AVI, ASF.

W teorii, mo¿esz umie¶ciæ video OpenDivX i d¼wiêk MP3 w pliku MPG. Wiêkszo¶æ odtwarzaczy nie bêdzie jednak w stanie go odtworzyæ, gdy¿ spodziewaj± siê obrazu MPEG1 i d¼wiêku MP2 (w przeciwieñstwie do AVI, MPG nie ma odpowiednich pól do opisu jego strumieni audio i video). Mo¿esz równie¿ umie¶ciæ video MPEG1 w pliku AVI. FFmpeg i MEncoder potrafi± tworzyæ takie pliki.

2.1.1. Formaty video

2.1.1.1. Pliki MPEG

Pliki MPEG spotykamy w ró¿nych kszta³tach:

MPlayer - Odtwarzacz filmów dla LINUKSA

2.1. Obs³ugiwane formaty 19

MPG: To jest najbardziej podstawowa forma plików MPEG. Zawiera video MPEG1 i audio MP2 (MPEG-1 warstwa 2) lub rzadziej MP1. • DAT: To dok³adnie ten sam format, co MPG, tylko z innym rozszerzeniem. Jest on u¿ywany na p³ytach Video CD. W zwi±zku ze sposobem tworzenia p³yt VCD i struktury Linuksa, pliki DAT nie mog± byæ odtwarzane ani kopiowane z VCD jak zwyk³e pliki. Musisz u¿yæ opcji vcd:// by odtworzyæ Video CD.

•

VOB: To format pliku MPEG na p³ytach DVD. Jest to to samo, co MPG, plus mo¿liwo¶æ umieszczenia w nim napisów lub d¼wiêku nie-MPEG (AC3). Zawiera zakodowany strumieñ obrazu MPEG2 i przewa¿nie d¼wiêk AC3, lecz dozwolone s± tak¿e DTS, MP2 i nieskompresowane LPCM. Przejrzyj sekcjê DVD!

•

Serie klatek tworz± niezale¿ne grupy w plikach MPEG. To oznacza, ¿e mo¿esz ci±æ/³±czyæ plik MPEG za pomoc± zwyk³ych narzêdzi plikowych (typu dd, cut) i pozostaje on ca³kowicie funkcjonalny.

Jedn± wa¿n± cech± plików MPG jest to, ¿e zawieraj± pole opisuj±ce stosunek szeroko¶ci do wysoko¶ci obrazu. Na przyk³ad pliki SVCD zawieraj± obraz o rozdzielczo¶ci 480x480, a w nag³ówku pole to jest ustawione na 4:3, wiêc odtwarzane s± w 640x480. Pliki AVI nie zawieraj± tego pola, wiêc musz± byæ skalowane w trakcie kodowania lub odtwarzane z opcj± -aspect

2.1.1.2. Pliki AVI

Zaprojektowane przez Microsoft pliki AVI (Audio Video Interleaved) to szeroko stosowany wielofunkcyjny format aktualnie u¿ywany g³ównie dla video DivX i DivX4. Posiada wiele wad i niedoci±gniêæ (np. przy strumieniowaniu). Obs³uguje jeden strumieñ video i od 0 do 99 strumieni audio i mo¿e mieæ co najwy¿ej 2 GB, lecz istnieje rozszerzenie, które pozwala na osi±gniêcie wiêkszych plików, zwane OpenDML. Aktualnie Microsoft usilnie zniechêca do stosowania AVI i zaleca ASF/WMV. Nie ¿eby to kogo¶ obchodzi³o...

Istnieje hack, który pozwala plikom AVI zawieraæ strumieñ audio Ogg Vorbis, ale powoduje to ich niekompatybilno¶æ ze zwyk³ymi AVI. MPlayer obs³uguje odtwarzanie takich plików. Skoki s± równie¿ zaimplementowane, lecz powa¿nie ograniczone poprzez ¼le zakodowane pliki z pomieszanymi nag³ówkami tworzonymi przez zepsute programy. Niestety jedyny program, który potrafi tworzyæ takie pliki - NanDub ma z tym problem.

Notatka

Kamery DV tworz± surowe strumienie DV, które s± konwertowane przez narzêdzia do zgrywania DV do dwóch ró¿nych typów plików AVI. Pliki te zawieraj± wtedy albo osobne strumienie audio i video, które MPlayer potrafi odtwarzaæ lub surowy strumieñ DV, którego obs³uga jest w trakcie rozwoju.

Istniej± dwa typy plików AVI:

Z przeplotem: Zawarto¶æ audio i video jest przepleciona. Jest to standardowy typ - zalecany i przewa¿nie u¿ywany. Niektóre narzêdzia tworz± przeplatane pliki AVI ze z³± synchronizacj±. MPlayer wykrywa je jako przeplatane, ale powoduje to utratê synchronizacji A/V (najczê¶ciej przy skokach). Pliki te powinny byæ odtwarzane jako bez przeplotu (opcja -ni).

•

Bez przeplotu: Najpierw umieszczony jest ca³y strumieñ video, a potem ca³y strumieñ audio. Wymaga to wiêc du¿o "chodzenia" po pliku, co powoduje, ¿e trudno jest je odtwarzaæ z sieci lub z CD-ROMów. •

MPlayer obs³uguje dwie metody synchronizacji dla plików AVI:

MPlayer - Odtwarzacz filmów dla LINUKSA

2.1.1. Formaty video 20 oparte na bps (bitach na sekundê): Oparta jest na liczbie bitów/próbek na sekundê strumieni audio/video. Metoda ta jest stosowana przez wiêkszo¶æ odtwarzaczy, w³±czaj±c w to avifile oraz Windows Media Player. Pliki z uszkodzonymi nag³ówkami i pliki z d¼wiêkiem VBR (Variable Bitrate - zmienne tempo bitowe) utworzone za pomoc± niekompatybilnego z VBR programu koduj±cego spowoduj± desynchronizacjê A/V przy tej metodzie (g³ównie przy skokach).

•

oparte na przeplocie: Nie korzysta z informacji o tempie bitowym z nag³ówka, lecz zamiast tego u¿ywa wzglêdnej pozycji przeplecionych fragmentów audio i video, dziêki czemu ¼le zakodowane pliki z d¼wiêkiem VBR mo¿na normalnie odtwarzaæ. •

Ka¿dy kodek video i audio jest dozwolony, lecz nale¿y zauwa¿yæ, ¿e d¼wiêk VBR nie jest zbyt dobrze obs³ugiwany przez wiêkszo¶æ odtwarzaczy. Format pliku co prawda pozwala na u¿ycie d¼wiêku VBR, lecz wiêkszo¶æ odtwarzaczy spodziewa siê d¼wiêku CBR (Constant Bitrate - sta³e tempo bitowe), przez co zawiod± przy VBR. VBR nie jest powszechny i specyfikacja AVI Microsoftu opisuje jedynie CBR. Zauwa¿y³em równie¿, ¿e wiêkszo¶æ enkoderów/multiplekserów AVI tworzy z³e pliki z d¼wiêkiem VBR. Istniej± jedynie dwa wyj±tki potwierdzaj±ce tê regu³ê: NanDub oraz MEncoder.

2.1.1.3. Pliki ASF/WMV

ASF (Active Streaming Format - Aktywny Format Strumieniowania) pochodzi z Microsoftu. Rozwinê³y siê dwa warianty ASF: v1.0 i v2.0. v1.0 jest u¿ywana przez ich narzêdzia medialne (Windows Media Player oraz Windows Media Encoder) i jest bardzo tajna. v2.0 jest opublikowana i opatentowana :). Oczywi¶cie ró¿ni± siê one znacz±co i nie ma pomiêdzy nimi ¿adnej kompatybilno¶ci (kolejna zagrywka legalistyczna). MPlayer obs³uguje jedynie v1.0, gdy¿ nikt jeszcze nie widzia³ ¿adnego pliku v2.0 :). Zauwa¿, ¿e dzisiejsze pliki ASF maj± rozszerzenia .WMA lub .WMV.

2.1.1.4. Pliki QuickTime/MOV

Formaty te zosta³y zaprojektowane przez Apple i mog± zawieraæ dowolny kodek, CBR lub VBR. Maj± przewa¿nie rozszerzenie .QT lub .MOV. Warto zauwa¿yæ, ¿e grupa MPEG4 wybra³a QuickTime jako zalecany format pliku dla MPEG4, a ich pliki MOV maj± rozszerzenie .MPG lub .MP4 (interesuj±ce jest to, ¿e strumienie w tych plikach to w rzeczywisto¶ci pliki MPG i AAC. Mo¿esz nawet je wyci±gn±æ za pomoc± opcji -dumpvideo oraz -dumpaudio).

Notatka

Wiêkszo¶æ nowych plików QuickTime u¿ywa kodeka video Sorenson i d¼wiêku QDesign Music. Zobacz nasz± sekcjê po¶wiêcon± kodekowi Sorenson.

2.1.1.5. Pliki VIVO

MPlayer szczê¶liwie demultipleksuje pliki VIVO. Najwiêksz± niedogodno¶ci± formatu jest to, ¿e nie ma on bloku indeksu ani sta³ego rozmiaru pakietu czy bajtów synchronizacji, a wiêkszo¶æ plików nie ma nawet klatek kluczowych, wiêc zapomnij o skakaniu po filmie!

Kodek video plików VIVO/1.0 to standardowy h.263. Kodek video plików VIVO/2.0 to zmodyfikowany, niestandardowy h.263v2. D¼wiêk jest ten sam i mo¿e to byæ g.723 (standardowy) lub Vivo Siren.

Zobacz sekcje Kodeka video VIVO i Kodeka audio VIVO by uzyskaæ informacje na temat instalacji.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.1.1.6. Pliki FLI FLI jest bardzo starym formatem u¿ywanym przez Autodesk Animator, lecz jest to powszechny w sieci format dla krótkich animacji. MPlayer demultipleksuje i dekoduje pliki FLI i potrafi nawet po nich skakaæ (u¿yteczne przy zapêtlaniu za pomoc± opcji -loop). Pliki FLI nie zawieraj± klatek kluczowych, wiêc obraz bêdzie trochê za¶miecony przez krótk± chwilê po skoku. 2.1.1.7. Pliki RealMedia (RM) Tak, MPlayer potrafi czytaæ (demultipleksowaæ) pliki RealMedia (.rm). Skoki dzia³aj±, ale musisz dodatkowo podaæ opcjê -forceidx (format obs³uguje klatki kluczowe). Tu znajdziesz listê obs³ugiwanych kodeków RealVideo i RealAudio. 2.1.1.8. Pliki NuppelVideo NuppelVideo jest narzêdziem do zgrywania TV (AFAIK :). MPlayer potrafi czytaæ jego pliki .NUV (tylko NuppelVideo 5.0). Pliki te mog± zawieraæ klatki: nieskompresowane YV12, skompresowane YV12+RTJpeg, skompresowane YV12 RTJpeg+lzo i skompresowane YV12+lzo. MPlayer dekoduje je (a nawet koduje za pomoc± MEncodera) wszystkie. Dzia³aj± równie¿ skoki. 2.1.1.9. pliki yuv4mpeg yuv4mpeg / yuv4mpeg2 to format plików stosowany przez programy mjpegtools. Mo¿esz zgrywaæ, produkowaæ, filtrowaæ lub kodowaæ video w tym formacie za pomoc± tych narzêdzi. Format ten jest w rzeczywisto¶ci sekwencj± nieskompresowanych obrazów YUV 4:2:0. 2.1.1.10. Pliki FILM Format ten jest u¿ywany przez stare gry CD-ROM na Sega Saturn. 2.1.1.11. Pliki RoQ Pliki RoQ to pliki multimedialne u¿ywane w niektórych grach ID, np. Quake III czy Return to Castle Wolfenstein. 2.1.1.12. Pliki OGG/OGM Jest to nowy format plików z Xiphophorus. Mo¿e zawieraæ dowolne kodeki audio i video, CBR lub VBR. Bêdziesz potrzebowa³ zainstalowanych bibliotek libogg oraz libvorbis zanim skompilujesz MPlayera by móc go odtwarzaæ. 2.1.1.13. Pliki SDP SDP to standardowy format IETF dla opisu strumieni RTP audio i/lub video. (Wymagane jest "LIVE.COM Streaming Media".) 2.1.1.14. Pliki PVA PVA to format MPEGo-podobny u¿ywany przez oprogramowanie kart DVB (np.: MultiDec lub WinTV pod Windows).

MPlayer - Odtwarzacz filmów dla LINUKSA

Specyfikacje PVA s± do pobrania pod nastêpuj±cym adresem: http://www.technotrend.de/download/av_format_v1.pdf

2.1.1.15. Pliki GIF

Format GIF jest powszechnym formatem zapisu grafiki sieciowej. Istniej± dwie wersje specyfikacji GIF: GIF87a oraz GIF89a. G³ówn± ró¿nic± jest to, ¿e GIF89a pozwala na animacjê. MPlayer obs³uguje oba formaty plików za pomoc± biblioteki libungif lub innej, kompatybilnej z libgif biblioteki. Nieanimowane GIFy s± wy¶wietlane jako filmy o pojedynczej klatce. (U¿yj opcji -loop oraz -fixed-vo by wy¶wietliæ je d³u¿ej)

MPlayer obecnie nie pozwala na skoki w plikach GIF. Pliki GIF bowiem niekoniecznie musz± mieæ sta³ego rozmiaru klatki, ani sta³ej prêdko¶ci odtwarzania. Raczej ka¿da klatka jest niezale¿nego rozmiaru i ma zostaæ umiejscowiona w odpowiednim miejscu na polu o ustalonym rozmiarze. Prêdko¶æ odtwarzania jest kontrolowana za pomoc± opcjonalnego bloku przed ka¿d± klatk±, która ustala opó¼nienie kolejnej klatki w setnych sekundy.

Standardowe pliki GIF zawieraj± 24-bitowe klatki RGB z co najwy¿ej 8-bitow± indeksowan± palet±. Klatki te s± przewa¿nie kompresowane za pomoc± LZW, lecz niektóre kodery produkuj± nieskompresowane klatki by unikn±æ problemów patentowych w zwi±zku z kompresj± LZW.

Je¶li Twoja dystrybucja nie zawiera biblioteki libungif, pobierz j± ze strony domowej libungif. By uzyskaæ szczegó³owe informacje techniczne, zajrzyj do specyfikacji GIF89a.

2.1.2. Formaty audio

MPlayer jest odtwarzaczem filmów, a nie mediów. Potrafi jednak odtwarzaæ niektóre pliki audio (s± one wymienione w sekcjach poni¿ej). Nie jest to jednak zalecane zastosowanie MPlayera. Powiniene¶ raczej u¿yæ XMMSa.

2.1.2.1. Pliki MP3

Mo¿esz mieæ pewne problemy przy odtwarzaniu niektórych plików MP3, które MPlayer b³êdnie rozpozna jako MPEG i odtworzy je nieprawid³owo lub nie odtworzy ich wcale. Nie da siê tego naprawiæ bez porzucenia wsparcia obs³ugi uszkodzonych plików MPEG i tak prawdopodobnie zostanie przez najbli¿sz± przysz³o¶æ. Opcja -demuxer opisana na stronie man mo¿e pomóc Ci w takich przypadkach.

2.1.2.2. Pliki WAV

2.1.2.3. Pliki OGG/OGM (Vorbis)

Wymaga poprawnie zainstalowanych bibliotek libogg i libvorbis.

2.1.2.4. Pliki WMA/ASF

2.1.2.5. Pliki MP4

MPlayer - Odtwarzacz filmów dla LINUKSA

2.1.2.6. CD audio

MPlayer potrafi korzystaæ z programu cdparanoia do odtwarzania CDDA (Audio CD). Sekcja ta nie zawiera spisu mo¿liwo¶ci programu cdparanoia.

Zajrzyj do strony man i przeczytaj opis opcji -cdda, która mo¿e zostaæ wykorzystana do przekazania opcji do programu cdparanoia.

2.1.2.7. XMMS

MPlayer potrafi korzystaæ z wtyczek wej¶cia z programu XMMS do odtwarzania wielu formatów. Istniej± wtyczki do muzyczek z gier na SNES, muzyczek SID (z Commodore 64), wielu formatów Amigi, .xm, .it, VQF, musepack, Bonk, shorten i wielu innych. Mo¿esz znale¼æ je na Stronie wtyczek wej¶ciowych do XMMS.

Do obs³ugi tej mo¿liwo¶ci musisz mieæ XMMSa i skompilowaæ MPlayera za pomoc± ./configure

--enable-xmms. Je¶li to nie zadzia³a, byæ mo¿e musisz ustawiæ ¶cie¿ki do wtyczek i bibliotek XMMSa

rêcznie za pomoc± opcji konfiguracji --with-xmmsplugindir i --with-xmmslibdir

2.2. Supported codecs

2.2.1. Video codecs

See the codec status table for the complete, daily generated list. Quite a few codecs are available for download from our homepage. Grab them from our codecs page.

The most important ones above all:

MPEG1 (VCD) and MPEG2 (DVD) video • native decoders for DivX ;-), OpenDivX (DivX4), DivX 5.01, 3ivX, M$ MPEG4 v1, v2 and other MPEG4 variants • native decoder for Windows Media Video 7/8 (WMV1/WMV2), and Win32 DLL decoder for Windows Media Video 9 (WMV3), both used in .wmv files • native Sorenson 1 (SVQ1) decoder • native Sorenson 3 (SVQ3) decoder • 3ivx v1, v2 decoder • Cinepak and Intel Indeo codecs (3.1,3.2,4.1,5.0) • MJPEG, AVID, VCR2, ASV2 and other hardware formats • VIVO 1.0, 2.0, I263 and other h263(+) variants • FLI/FLC • RealVideo 1.0 & 2.0 from libavcodec, and RealVideo 3.0 & 4.0 codecs using RealPlayer libraries • native decoder for HuffYUV • Various old simple RLE-like formats • If you have a Win32 codec not listed here which is not supported yet, please read the codec importing HOWTO and help us add support for it.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.1.2. Formaty audio 24

2.2.1.1. DivX4/DivX5

This section contains information about the DivX4 and DivX5 codecs of Project Mayo. Their first available alpha version was OpenDivX 4.0 alpha 47 and 48. Support for this was included in MPlayer in the past, and built by default. We also used its postprocessing code to optionally enhance visual quality of MPEG1/2 movies. Now we use our own, for all file types.

The new generation of this codec is called DivX4 and can even decode movies made with the infamous DivX codec! In addition it is much faster than the native Win32 DivX DLLs but slower than libavcodec. Hence its usage as a decoder is DISCOURAGED. However, it is useful for encoding. One disadvantage of this codec is that it is not available under an Open Source license.

DivX4 works in two modes:

-vc odivx

Uses the codec in OpenDivX fashion. In this case it produces YV12 images in its own buffer, and MPlayer does colorspace conversion via libvo. (Fast, recommended!)

-vc divx4

Uses the colorspace conversion of the codec. In this mode you can use YUY2/UYVY, too. (SLOW)

The -vc odivx method is usually faster, due to the fact that it transfers image data in YV12 (planar YUV 4:2:0) format, thus requiring much less bandwidth on the bus. For packed YUV modes (YUY2, UYVY) use the -vc divx4 method. For RGB modes the speed is the same, differing at best according to your current color depth.

Notatka

If your -vo driver supports direct rendering, then -vc divx4 may be faster, or even the fastest solution.

The Divx4/5 binary codec library can be downloaded from avifile or divx.com Unpack it, run

./install.sh as root and do not forget adding /usr/local/lib to your /etc/ld.so.conf and

running ldconfig.

Get the CVS version of the OLD OpenDivx core library like this:

cvs -d:pserver:anonymous@cvs.projectmayo.com:/cvsroot login

1.

cvs -d:pserver:anonymous@cvs.projectmayo.com:/cvsroot co divxcore

• This core library is split into a decore and encore library that have to be compiled separately. For the decore Library, simply type

cd divxcore/decore/build/linux
make
cp libdivxdecore.so /usr/local/lib
ln -s libdivxdecore.so /usr/local/lib/libdivxdecore.so.0
cp ../../src/decore.h /usr/local/include

•

Alas, for the encore library there is no Linux Makefile available, and the MMX optimized code only works on Windows. You can still compile it, though, by using this Makefile.

cd ../../../encore/build

•

MPlayer - Odtwarzacz filmów dla LINUKSA

2.2.1. Video codecs 25

mkdir linux
cd linux
cp path/Makefile .
make
cp libdivxencore.so /usr/local/lib
ln -s libdivxencore.so /usr/local/lib/libdivxencore.so.0
cp ../../src/encore.h /usr/local/include

MPlayer autodetects DivX4/DivX5 if it is properly installed, just compile as usual. If it does not detect it, you did not install or configure it correctly.

2.2.1.2. FFmpeg/libavcodec

FFmpeg contains an open source codec package, which is capable of decoding streams with various audio and video codecs. It also offers an impressing encoding facility and higher speed than the Win32 codecs or the DivX.com DivX4/5 libraries!

It contains a lot of nice codecs, especially important are the MPEG4 variants: DivX3, DivX4, DivX5, Windows Media Video 7/8 (WMV1/WMV2). Also a very interesting one is the WMA decoder.

The most recent codec deserving credit is the Sorenson 3 (SVQ3) codec. This is the first, completely opensource implementation. It's even faster than the original. Be sure to prefer this instead of the binary codec!

For a complete list of supported codecs please visit the FFmpeg homepage. Supported video and audio codecs.

If you use an MPlayer release you have libavcodec right in the package, just build as usual. If you use MPlayer from CVS you have to extract libavcodec from the FFmpeg CVS tree as FFmpeg releases are very rare. The CVS is mostly stable and offers the most features. In order to achieve this do:

cvs -d:pserver:anonymous@mplayerhq.hu:/cvsroot/ffmpeg login

1.

cvs -d:pserver:anonymous@mplayerhq.hu:/cvsroot/ffmpeg co ffmpeg

2. Move the libavcodec directory from the FFmpeg sources to the root of the MPlayer CVS tree. It should look like this: main/libavcodec

Symlinking is not enough, you have to copy/move it!

3.

If you prefer having libavcodec updated at the same time you update MPlayer CVS, put the following line into the main/CVS/Entries file:

D/libavcodec////

4.

Compile. configure should detect problems before compilation. 5. Notatka

MPlayer from CVS does contain a libavcodec subdirectory, but it does not contain the source for libavcodec! You must follow the steps above to obtain the source for this library.

With FFmpeg and my Matrox G400, I can view even the highest resolution DivX movies without dropped frames on my K6-2 500.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.2.1.3. XAnim codecs

Notatka

Be advised that the XAnim binary codecs are packaged with a piece of text claiming to be a legally binding software license which, besides other restrictions, forbids the user to use the codecs in conjunction with any program other than XAnim. However, the XAnim author has yet to bring legal action against anyone for codec-related issues.

INSTALLATION AND USAGE. MPlayer is capable of employing the XAnim codecs for decoding. Follow the instructions to enable them:

Download the codecs you wish to use from the XAnim site. The 3ivx codec is not there, but at the 3ivx site. 1. OR download the codecs pack from our codecs page 2. Use the --with-xanimlibdir option to tell configure where to find the XAnim codecs. By default, it looks for them at /usr/local/lib/codecs, /usr/local/lib/xanim/mods,

/usr/lib/xanim/mods and /usr/lib/xanim. Alternatively you can set the environment

variable XANIM_MOD_DIR to the directory of the XAnim codecs.

3.

Rename/symlink the files, cutting out the architecture stuff, so they will have filenames like these:

vid_cvid.xa, vid_h263.xa, vid_iv50.xa

4.

XAnim is video codec family xanim, so you may want to use the -vfm xanim option to tell MPlayer to use them if possible.

Tested codecs include: Indeo 3.2, 4.1, 5.0, CVID, 3ivX, h263.

2.2.1.4. VIVO video

MPlayer can play Vivo (1.0 and 2.0) videos. The most suitable codec for 1.0 files is FFmpeg's H263 decoder, you can use it with the -vc ffh263 option. For 2.0 files, use the Win32 DLL through the -vc vivo option. If you do not supply command line options MPlayer selects the best codec automatically.

2.2.1.5. MPEG 1/2 video

MPEG1 and MPEG2 are decoded by the multiplatform native libmpeg2 library, whose source code is included in MPlayer. We handle buggy MPEG 1/2 video files by catching Signal 11 (segmentation

fault), and quickly reinitializing the codec, continuing exactly from where the failure occurred. This

recovery technique has no measurable speed penalty.

2.2.1.6. MS Video1

This is a very old and very bad codec from Microsoft. In the past it was decoded with the msvidc32.dll Win32 codec, now we have our own open source implementation (by Mike Melanson).

2.2.1.7. Cinepak CVID

MPlayer uses its own open source, multiplatform Cinepak decoder (by Dr. Tim Ferguson) by default. It supports YUV outputs, so that hardware scaling is possible if the video output driver permits it.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.2.1.8. RealVideo

MPlayer supports decoding all versions of RealVideo:

RealVideo 1.0, 2.0 (fourcc RV10, RV20) - en/decoding supported by libavcodec • RealVideo 3.0, 4.0 (fourcc RV30, RV40) - decoding supported by RealPlayer libraries • It is recommended to download and install RealPlayer8 or RealONE, because MPlayer can use their libraries to decode files with RealVideo 2.0 - 4.0 video. The MPlayer configure script should detect the RealPlayer libraries in the standard locations of a full installation. If it does not, tell configure where to look with the

--with-reallibdir option.

As a second chance you can download the codecs from http://www.mplayerhq.hu/MPlayer/releases/codecs/. After downloading the Real codecs package, extract it to the /usr/local/lib/codecs directory, or you can specify a unique path with the --with-reallibdir option.

Notatka

RealPlayer libraries currently only work with Linux, FreeBSD, NetBSD and Cygwin on the x86, Alpha and PowerPC (Linux/Alpha and Linux/PowerPC have been tested) platforms.

2.2.1.9. XviD

XviD is a forked development of the OpenDivX codec. It happened when ProjectMayo changed OpenDivX to closed source DivX4 (now DivX5), and the non-ProjectMayo people working on OpenDivX got angry, then started XviD. So both projects have the same origin.

ADVANTAGES

open source • its API is compatible with DivX4 so adding support for it is easy • 2-pass encoding support • nice encoding quality, higher speed than DivX4 (you can optimize it for your box while compiling) • DISADVANTAGES

currently it does not properly decode all DivX/DivX4 files (no problem as libavcodec can play them) • under development • INSTALLING XVID CVS

It is currently available only from CVS. Here are download and installation instructions (you need at least autoconf 2.50, automake and libtool):

cvs -z3 -d:pserver:anonymous@cvs.xvid.org:/xvid login

1.

cvs -z3 -d:pserver:anonymous@cvs.xvid.org:/xvid co xvidcore

2.

cd xvidcore/build/generic

3.

MPlayer - Odtwarzacz filmów dla LINUKSA

./bootstrap.sh

4.

./configure

You may have to add some options (examine the output of

./configure --help

).

5.

make && make install

6. If you specified --enable-divxcompat, copy ../../src/divx4.h to

/usr/local/include/.

7. Recompile MPlayer with --with-xvidcore=/path/to/libxvidcore.a. 8. 2.2.1.10. Sorenson

Sorenson is a video codec developed by Sorenson Media and licensed to Apple who distribute it with their QuickTime Player. We are currently able to decode all version of Sorenson video files with the following decoders:

Sorenson Video v1 (fourcc SVQ1) - decoding supported by native codec (libavcodec) • Sorenson Video v3 (fourcc SVQ3) - decoding supported by native codec (libavcodec) • COMPILING MPLAYER WITH QUICKTIME LIBRARIES SUPPORT

Notatka

currently only 32bit Intel platforms are supported.

download MPlayer CVS 1. download QuickTime DLL pack from http://www.mplayerhq.hu/MPlayer/releases/codecs/ 2. extract QuickTime DLL pack to your Win32 codecs directory (default:

/usr/local/lib/codecs/)

3. compile MPlayer 4. 2.2.2. Audio codecs

The most important audio codecs above all:

MPEG layer 1/2/3 (MP1/2/3) audio (native code, with MMX/SSE/3DNow! optimization) • Windows Media Audio 7 and 8 (aka WMAv1 and WMAv2) (native code, with libavcodec) • Windows Media Audio 9 (WMAv3) (using DMO DLL) • AC3 Dolby audio (native code, with MMX/SSE/3DNow! optimization) • AC3 passing through soundcard hardware • AAC • Ogg Vorbis audio codec (native library) • RealAudio: DNET (low bitrate AC3), Cook, Sipro and ATRAC3 • QuickTime: Qualcomm and QDesign audio codecs • VIVO audio (g723, Vivo Siren) • Voxware audio (using DirectShow DLL) •

MPlayer - Odtwarzacz filmów dla LINUKSA alaw and ulaw, various gsm, adpcm and pcm formats and other simple old audio codecs • 2.2.2.1. Software AC3 decoding This is the default decoder used for files with AC3 audio.

The AC3 decoder can create audio output mixes for 2, 4, or 6 speakers. When configured for 6 speakers, this decoder provides separate output of all the AC3 channels to the sound driver, allowing for full "surround sound" experience without the external AC3 decoder required to use the hwac3 codec. Use the -channels option to select the number of output channels. Use -channels 2 for a stereo downmix. For a 4 channel downmix (Left Front, Right Front, Left Surround and Right Surround outputs), use

-channels 4. In this case, any center channel will be mixed equally to the front channels. -channels 6

will output all the AC3 channels as they are encoded - in the order Left, Right, Left Surround, Right Surround, Center and LFE.

The default number of output channels is 2.

To use more than 2 output channels, you will need to use OSS, and have a sound card that supports the appropriate number of output channels via the SNDCTL_DSP_CHANNELS ioctl. An example of a suitable driver is emu10k1 (used by Soundblaster Live! cards) from August 2001 or newer (ALSA CVS is also supposed to work). 2.2.2.2. Hardware AC3 decoding You need an AC3 capable sound card, with digital out (SP/DIF). The card's driver must properly support the AFMT_AC3 format (C-Media does). Connect your AC3 decoder to the SP/DIF output, and use the -ac

hwac3 option. It is experimental but known to work with C-Media cards and Soundblaster Live! + ALSA

(but not OSS) drivers and DXR3/Hollywood+ MPEG decoder cards. 2.2.2.3. libmad support libmad is a multiplatform, integer (internally 24bit PCM) only MPEG audio decoding library. It does not handle broken files well, and it sometimes has problems with seeking, but it may perform better on FPU-less (such as ARM) platform than mp3lib. To enable support, compile with the --enable-mad configure option. 2.2.2.4. VIVO audio The audio codec used in VIVO files depends on whether it is a VIVO/1.0 or VIVO/2.0 file. VIVO/1.0 files have g.723 audio, and VIVO/2.0 files have Vivo Siren audio. Both are supported. 2.2.2.5. RealAudio MPlayer supports decoding nearly all versions of RealAudio:

RealAudio DNET - decoding supported by liba52 • RealAudio Cook/Sipro/ATRAC3 - decoding supported by RealPlayer libraries • On how to install RealPlayer libraries, see the RealMedia file format section.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.2.2.6. QDesign codecs

QDesign audio streams (fourcc:QDMC, QDM2) are found in MOV/QT files. Both versions of this codec can be decoded with QuickTime libraries. For installation instructions please see the Sorenson video codec section.

2.2.2.7. Qualcomm codecs

Qualcomm audio streams (fourcc:Qclp) is found in MOV/QT files. It can be decoded with QuickTime libraries. For installation instructions please see the Sorenson video codec section.

2.2.2.8. AAC codec

AAC (Advanced Audio Coding) is an audio codec sometimes found in MOV and MP4 files. An open source decoder called FAAD is available from http://www.audiocoding.com. MPlayer includes libfaad 2.0RC1, so you do not need to get it separately.

If you use gcc 3.2 which fails to compile our internal FAAD or want to use the external library for some other reason, download the library from the download page and pass --with-externalfaad to configure. You do not need all of faad2 to decode AAC files, libfaad is enough. Build it like this:

cd faad2/
chmod +x bootstrap
./bootstrap
./configure
cd libfaad
make
make install

Binaries are not available from audiocoding.com, but you can (apt-)get Debian packages from Christian Marillat's homepage, Mandrake RPMs from the P.L.F and RedHat RPMs from Dominik Mierzejewski's homepage.

2.2.3. Win32 codecs importing HOWTO

2.2.3.1. VFW codecs

VFW (Video for Windows) is the old Video API for Windows. Its codecs have the .DLL or (rarely) .DRV extension. If MPlayer fails at playing your AVI with this kind of message:

UNKNOWN video codec: HFYU (0x55594648)

It means your AVI is encoded with a codec which has the HFYU fourcc (HFYU = HuffYUV codec, DIV3 = DivX Low Motion, etc.). Now that you know this, you have to find out which DLL Windows loads in order to play this file. In our case, the system.ini contains this information in a line that reads:

VIDC.HFYU=huffyuv.dll

So you need the huffyuv.dll file. Note that the audio codecs are specified by the MSACM prefix:

msacm.l3acm=L3codeca.acm

This is the MP3 codec. Now that you have all the necessary information (fourcc, codec file, sample AVI),

MPlayer - Odtwarzacz filmów dla LINUKSA submit your codec support request by mail, and upload these files to the FTP site:

ftp://ftp.mplayerhq.hu/MPlayer/incoming/[codecname]/

Notatka

On Windows NT/2000/XP search for this info in the registry, e.g. search for "VIDC.HFYU". To find out how to do this, look at the old DirectShow method below.

2.2.3.2. DirectShow codecs

DirectShow is the newer Video API, which is even worse than its predecessor. Things are harder with DirectShow, since

system.ini does not contain the needed information, instead it is stored in the registry and

• we need the GUID of the codec. • New Method:

Using Microsoft GraphEdit (fast)

Get GraphEdit from either DirectX SDK or doom9 1. Start graphedit.exe. 2. From the menu select Graph -> Insert Filters. 3. Expand item DirectShow Filters 4. Select the right codec name and expand item. 5. In the entry DisplayName look at the text in winged brackets after the backslash and write it down (five dash-delimited blocks, the GUID). 6. The codec binary is the file specified in the Filename entry. 7. Notatka

If there is no Filename and DisplayName contains something like device:dmo, then it is a DMO-Codec.

Old Method:

Take a deep breath and start searching the registry...

Start regedit. 1. Press Ctrl+F, disable the first two checkboxes, and enable the third. Type in the fourcc of the codec (e.g. TM20). 2. You should see a field which contains the path and the filename (e.g.

C:\WINDOWS\SYSTEM\TM20DEC.AX).

3. Now that you have the file, we need the GUID. Try searching again, but now search for the codec's name, not the fourcc. Its name can be acquired when Media Player is playing the file, by checking File -> Properties -> Advanced. If not, you are out of luck. Try guessing (e.g. search for TrueMotion).

4.

If the GUID is found you should see a FriendlyName and a CLSID field. Write down the 16 byte CLSID, this is the GUID we need. 5.

MPlayer - Odtwarzacz filmów dla LINUKSA

Notatka

If searching fails, try enabling all the checkboxes. You may have false hits, but you may get lucky...

Now that you have all the necessary information (fourcc, GUID, codec file, sample AVI), submit your codec support request by mail, and upload these files to the FTP site:

ftp://ftp.mplayerhq.hu/MPlayer/incoming/[codecname]/

2.3. Urz±dzenia wyj¶ciowe

2.3.1. Video output devices

2.3.1.1. Setting up MTRR

It is VERY recommended to check if the MTRR registers are set up properly, because they can give a big performance boost.

Do a cat /proc/mtrr:

--($:~)-- cat /proc/mtrr
reg00: base=0xe4000000 (3648MB), size=  16MB: write-combining, count=9
reg01: base=0xd8000000 (3456MB), size= 128MB: write-combining, count=1

It's right, shows my Matrox G400 with 16MB memory. I did this from XFree 4.x.x , which sets up MTRR registers automatically.

If nothing worked, you have to do it manually. First, you have to find the base address. You have 3 ways to find it:

from X11 startup messages, for example:

(--) SVGA: PCI: Matrox MGA G400 AGP rev 4, Memory @ 0xd8000000, 0xd4000000
(--) SVGA: Linear framebuffer at 0xD8000000

1.

from /proc/pci (use lspci -v command):

01:00.0 VGA compatible controller: Matrox Graphics, Inc.: Unknown device 0525
Memory at d8000000 (32-bit, prefetchable)

•

from mga_vid kernel driver messages (use dmesg):

mga_mem_base = d8000000

•

Then let's find the memory size. This is very easy, just convert video RAM size to hexadecimal, or use this table:

1 MB 0x100000 2 MB 0x200000 4 MB 0x400000 8 MB 0x800000 16 MB 0x1000000 32 MB 0x2000000

MPlayer - Odtwarzacz filmów dla LINUKSA

You know base address and memory size, let's setup MTRR registers! For example, for the Matrox card above (base=0xd8000000) with 32MB ram (size=0x2000000) just execute:

echo "base=0xd8000000 size=0x2000000 type=write-combining" >| /proc/mtrr

Not all CPUs support MTRRs. For example older K6-2's (around 266MHz, stepping 0) doesn't support MTRR, but stepping 12's do (cat /proc/cpuinfo to check it).

2.3.1.2. Video outputs for traditional video cards

2.3.1.2.1. Xv

Under XFree86 4.0.2 or newer, you can use your card's hardware YUV routines using the XVideo extension. This is what the option '-vo xv' uses. Also, this driver supports adjusting brightness/contrast/hue/etc (unless you use the old, slow DirectShow DivX codec, which supports it everywhere), see the man page.

In order to make this work, be sure to check the following:

You have to use XFree86 4.0.2 or newer (former versions don't have XVideo) 1. Your card actually supports hardware acceleration (modern cards do) 2. X loads the XVideo extension, it's something like this:

(II) Loading extension XVideo

in /var/log/XFree86.0.log

Notatka

This loads only the XFree86's extension. In a good install, this is always loaded, and doesn't mean that the card's XVideo support is loaded!

3.

Your card has Xv support under Linux. To check, try xvinfo, it is the part of the XFree86 distribution. It should display a long text, similar to this:

X-Video Extension version 2.2
screen #0
  Adaptor #0: "Savage Streams Engine"
    number of ports: 1
    port base: 43
    operations supported: PutImage
    supported visuals:
      depth 16, visualID 0x22
      depth 16, visualID 0x23
    number of attributes: 5
(...)
    Number of image formats: 7
      id: 0x32595559 (YUY2)
        guid: 59555932-0000-0010-8000-00aa00389b71
        bits per pixel: 16
        number of planes: 1
        type: YUV (packed)
      id: 0x32315659 (YV12)
        guid: 59563132-0000-0010-8000-00aa00389b71
        bits per pixel: 12
        number of planes: 3

•

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1. Video output devices 34

        type: YUV (planar)
(...etc...)

It must support YUY2 packed, and YV12 planar pixel formats to be usable with MPlayer. And finally, check if MPlayer was compiled with 'xv' support. Do a mplayer -vo help | grep xv If 'xv' support was built a line similar to this should appear:

  xv      X11/Xv

•

2.3.1.2.1.1. 3dfx cards

Older 3dfx drivers were known to have problems with XVideo acceleration, it didn't support either YUY2 or YV12, and so. Verify that you have XFree86 version 4.2.0 or greater, it works OK with YV12 and YUY2. Previous versions, including 4.1.0, crashes with YV12. If you experience strange effects using -vo xv, try SDL (it has XVideo, too) and see if it helps. Check the SDL section for details.

OR, try the NEW -vo tdfxfb driver! See the tdfxfb section.

2.3.1.2.1.2. S3 cards

S3 Savage3D's should work fine, but for Savage4, use XFree86 version 4.0.3 or greater (in case of image problems, try 16bpp). As for S3 Virge: there is xv support, but the card itself is very slow, so you better sell it.

Notatka

It's currently unclear which Savage models lack YV12 support, and convert by driver (slow). If you suspect your card, get a newer driver, or ask politely on the mplayer-users mailing list for an MMX/3DNow enabled driver.

2.3.1.2.1.3. nVidia cards

nVidia isn't always a very good choice under Linux (according to nVidia, this is not true)... XFree86's open-source driver supports most of these cards, but for some cases, you'll have to use the binary closed-source nVidia driver, available at nVidia's web site. You'll always need this driver if you want 3D acceleration, too.

Riva128 cards don't have XVideo support with XFree86's nVidia driver :( Complain to nVidia.

However, MPlayer contains a VIDIX driver for most nVidia cards. Currently it is in beta stage, and has some drawbacks. For more information, see nVidia VIDIX section.

2.3.1.2.1.4. ATI cards

The GATOS driver (which you should use, unless you have Rage128 or Radeon) has VSYNC enabled by default. It means that decoding speed (!) is synced to the monitor's refresh rate. If playing seems to be slow, try disabling VSYNC somehow, or set refresh rate to a n*(fps of the movie) Hz.

Radeon VE - if you need X, use XFree86 4.2.0 or greater for this card. No TV out support. Of course with MPlayer you can happily get accelerated display, with or without TV output, and no libraries or X are needed. Read the VIDIX section.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1.2.1.5. NeoMagic cards

These cards can be found in many laptops. You must use XFree86 4.3.0 or above, or else use Stefan Seyfried's Xv-capable drivers. Just choose the one that applies to your version of XFree86.

XFree86 4.3.0 includes Xv support, yet Bohdan Horst sent a small patch against the XFree86 sources that speeds up framebuffer operations (so XVideo) up to four times. The patch has been included in XFree86 CVS and should be in the next release after 4.3.0.

To allow playback of DVD sized content change your XF86Config like this:

Section "Device"
    [...]
    Driver "neomagic"
    Option "OverlayMem" "829440"
    [...]
EndSection

2.3.1.2.1.6. Trident cards

If you want to use xv with a trident card, provided that it doesn't work with 4.1.0, install XFree 4.2.0. 4.2.0 adds support for fullscreen Xv support with the Cyberblade XP card.

Alternatively, MPlayer contains a VIDIX driver for the Cyberblade/i1 card.

2.3.1.2.1.7. Kyro/PowerVR cards

If you want to use Xv with a Kyro based card (for example Hercules Prophet 4000XT), you should download the drivers from the PowerVR site

2.3.1.2.2. DGA

PREAMBLE. This document tries to explain in some words what DGA is in general and what the DGA video output driver for MPlayer can do (and what it can't).

WHAT IS DGA. DGA is short for Direct Graphics Access and is a means for a program to bypass the X server and directly modifying the framebuffer memory. Technically spoken this happens by mapping the framebuffer memory into the memory range of your process. This is allowed by the kernel only if you have superuser privileges. You can get these either by logging in as root or by setting the SUID bit on the MPlayer executable (not recommended).

There are two versions of DGA: DGA1 is used by XFree 3.x.x and DGA2 was introduced with XFree 4.0.1.

DGA1 provides only direct framebuffer access as described above. For switching the resolution of the video signal you have to rely on the XVidMode extension.

DGA2 incorporates the features of XVidMode extension and also allows switching the depth of the display. So you may, although basically running a 32 bit depth X server, switch to a depth of 15 bits and vice versa.

However DGA has some drawbacks. It seems it is somewhat dependent on the graphics chip you use and on the implementation of the X server's video driver that controls this chip. So it does not work on every system...

MPlayer - Odtwarzacz filmów dla LINUKSA

INSTALLING DGA SUPPORT FOR MPLAYER. First make sure X loads the DGA extension, see in

/var/log/XFree86.0.log:

(II) Loading extension XFree86-DGA

See, XFree86 4.0.x or greater is highly recommended! MPlayer's DGA driver is autodetected by

./configure, or you can force it with --enable-dga.

If the driver couldn't switch to a smaller resolution, experiment with options -vm (only with X 3.3.x), -fs,

-bpp, -zoom to find a video mode that the movie fits in. There is no converter right now :(

Become root. DGA needs root access to be able to write directly video memory. If you want to run it as user, then install MPlayer SUID root:

chown root /usr/local/bin/mplayer
chmod 750 /usr/local/bin/mplayer
chmod +s /usr/local/bin/mplayer

Now it works as a simple user, too.

Security risk

This is a big security risk! Never do this on a server or on a computer that can be accessed by other people because they can gain root privileges through SUID root MPlayer.

Now use -vo dga option, and there you go! (hope so:) You should also try if the -vo sdl:dga option works for you! It's much faster!

RESOLUTION SWITCHING. The DGA driver allows for switching the resolution of the output signal. This avoids the need for doing (slow) software scaling and at the same time provides a fullscreen image. Ideally it would switch to the exact resolution (except for honoring aspect ratio) of the video data, but the X server only allows switching to resolutions predefined in /etc/X11/XF86Config (/etc/X11/XF86Config-4 for XFree 4.X.X respectively). Those are defined by so-called modelines and depend on the capabilities of your video hardware. The X server scans this config file on startup and disables the modelines not suitable for your hardware. You can find out which modes survive with the X11 log file. It can be found at: /var/log/XFree86.0.log.

These entries are known to work fine with a Riva128 chip, using the nv.o X server driver module.

Section "Modes"
  Identifier "Modes[0]"
  Modeline "800x600"  40     800 840 968 1056  600 601 605 628
  Modeline "712x600"  35.0   712 740 850 900   400 410 412 425
  Modeline "640x480"  25.175 640 664 760 800   480 491 493 525
  Modeline "400x300"  20     400 416 480 528   300 301 303 314 Doublescan
  Modeline "352x288"  25.10  352 368 416 432   288 296 290 310
  Modeline "352x240"  15.750 352 368 416 432   240 244 246 262 Doublescan
  Modeline "320x240"  12.588 320 336 384 400   240 245 246 262 Doublescan
EndSection

DGA & MPLAYER. DGA is used in two places with MPlayer: The SDL driver can be made to make use of it (-vo sdl:dga) and within the DGA driver (-vo dga). The above said is true for both; in the following sections I'll explain how the DGA driver for MPlayer works.

MPlayer - Odtwarzacz filmów dla LINUKSA

FEATURES. The DGA driver is invoked by specifying -vo dga at the command line. The default behavior is to switch to a resolution matching the original resolution of the video as close as possible. It deliberately ignores the -vm and -fs options (enabling of video mode switching and fullscreen) - it always tries to cover as much area of your screen as possible by switching the video mode, thus refraining to use a single additional cycle of your CPU to scale the image. If you don't like the mode it chooses you may force it to choose the mode matching closest the resolution you specify by -x and -y. By providing the -v option, the DGA driver will print, among a lot of other things, a list of all resolutions supported by your current

XF86Config file. Having DGA2 you may also force it to use a certain depth by using the -bpp option.

Valid depths are 15, 16, 24 and 32. It depends on your hardware whether these depths are natively supported or if a (possibly slow) conversion has to be done.

If you should be lucky enough to have enough offscreen memory left to put a whole image there, the DGA driver will use doublebuffering, which results in much smoother movie replaying. It will tell you whether double-buffering is enabled or not.

Doublebuffering means that the next frame of your video is being drawn in some offscreen memory while the current frame is being displayed. When the next frame is ready, the graphics chip is just told the location in memory of the new frame and simply fetches the data to be displayed from there. In the meantime the other buffer in memory will be filled again with new video data.

Doublebuffering may be switched on by using the option -double and may be disabled with -nodouble. Current default option is to disable doublebuffering. When using the DGA driver, onscreen display (OSD) only works with doublebuffering enabled. However, enabling doublebuffering may result in a big speed penalty (on my K6-II+ 525 it used an additional 20% of CPU time!) depending on the implementation of DGA for your hardware.

SPEED ISSUES. Generally spoken, DGA framebuffer access should be at least as fast as using the X11 driver with the additional benefit of getting a fullscreen image. The percentage speed values printed by MPlayer have to be interpreted with some care, as for example, with the X11 driver they do not include the time used by the X server needed for the actual drawing. Hook a terminal to a serial line of your box and start top to see what is really going on in your box.

Generally spoken, the speedup done by using DGA against 'normal' use of X11 highly depends on your graphics card and how well the X server module for it is optimized.

If you have a slow system, better use 15 or 16 bit depth since they require only half the memory bandwidth of a 32 bit display.

Using a depth of 24 bit is even a good idea if your card natively just supports 32 bit depth since it transfers 25% less data compared to the 32/32 mode.

I've seen some AVI files already be replayed on a Pentium MMX 266. AMD K6-2 CPUs might work at 400 MHZ and above.

KNOWN BUGS. Well, according to some developers of XFree, DGA is quite a beast. They tell you better not to use it. Its implementation is not always flawless with every chipset driver for XFree out there.

With XFree 4.0.3 and nv.o there is a bug resulting in strange colors. • ATI driver requires to switch mode back more than once after finishing using of DGA. • Some drivers simply fail to switch back to normal resolution (use Ctrl+Alt+Keypad + and Ctrl+Alt+Keypad - to switch back manually). •

MPlayer - Odtwarzacz filmów dla LINUKSA

Some drivers simply display strange colors. • Some drivers lie about the amount of memory they map into the process's address space, thus vo_dga won't use doublebuffering (SIS?). • Some drivers seem to fail to report even a single valid mode. In this case the DGA driver will crash telling you about a nonsense mode of 100000x100000 or something like that. • OSD only works with doublebuffering enabled (else it flickers). • 2.3.1.2.3. SDL

SDL (Simple Directmedia Layer) is basically a unified video/audio interface. Programs that use it know only about SDL, and not about what video or audio driver does SDL actually use. For example a Doom port using SDL can run on svgalib, aalib, X, fbdev, and others, you only have to specify the (for example) video driver to use with the SDL_VIDEODRIVER environment variable. Well, in theory.

With MPlayer, we used its X11 driver's software scaler ability for cards/drivers that doesn't support XVideo, until we made our own (faster, nicer) software scaler. Also we used its aalib output, but now we have ours which is more comfortable. Its DGA mode was better than ours, until recently. Get it now? :)

It also helps with some buggy drivers/cards if the video is jerky (not slow system problem), or audio is lagging.

SDL video output supports displaying subtitles under the movie, on the (if present) black bar.

There are several command line switches for SDL:

-vo sdl:name

specifies SDL video driver to use (i.e. aalib, dga, x11)

-ao sdl:name

specifies SDL audio driver to use (i.e. dsp, esd, arts)

-noxv

disables XVideo hardware acceleration

-forcexv

tries to force XVideo acceleration

Tabela 2.1. SDL only keys

Key Action c cycles available fullscreen modes n changes back to normal mode

Known bugs:

Keys pressed under sdl:aalib console driver repeat forever. (use -vo aa!) It's bug in SDL, I can't change it (tested with SDL 1.2.1). • DO NOT USE SDL with GUI! It won't work as it should. • 2.3.1.2.4. SVGAlib

INSTALLATION. You'll have to install svgalib and its development package in order for MPlayer build its SVGAlib driver (autodetected, but can be forced), and don't forget to edit /etc/vga/libvga.config to

MPlayer - Odtwarzacz filmów dla LINUKSA suit your card and monitor.

Notatka

Be sure not to use the -fs switch, since it toggles the usage of the software scaler, and it's slow. If you really need it, use the -sws 4 option which will produce bad quality, but is somewhat faster. EGA (4BPP) SUPPORT. SVGAlib incorporates EGAlib, and MPlayer has the possibility to display any movie in 16 colors, thus usable in the following sets:

EGA card with EGA monitor: 320x200x4bpp, 640x200x4bpp, 640x350x4bpp • EGA card with CGA monitor: 320x200x4bpp, 640x200x4bpp • The bpp (bits per pixel) value must be set to 4 by hand: -bpp 4 The movie probably must be scaled down to fit in EGA mode:

-vf scale=640:350

or

-vf scale=320:200

For that we need fast but bad quality scaling routine:

-sws 4

Maybe automatic aspect correction has to be shut off:

-noaspect

Notatka

According to my experience the best image quality on EGA screens can be achieved by decreasing the brightness a bit: -vf eq=-20:0. I also needed to lower the audio samplerate on my box, because the sound was broken on 44kHz: -srate 22050. You can turn on OSD and subtitles only with the expand filter, see the man page for exact parameters.

2.3.1.2.5. Framebuffer output (FBdev)

Whether to build the FBdev target is autodetected during ./configure. Read the framebuffer documentation in the kernel sources (Documentation/fb/*) for more information. If your card doesn't support VBE 2.0 standard (older ISA/PCI cards, such as S3 Trio64), only VBE 1.2 (or older?): Well, VESAfb is still available, but you'll have to load SciTech Display Doctor (formerly UniVBE) before booting Linux. Use a DOS boot disk or whatever. And don't forget to register your UniVBE ;)) The FBdev output takes some additional parameters above the others:

-fb

MPlayer - Odtwarzacz filmów dla LINUKSA specify the framebuffer device to use (/dev/fb0)

-fbmode

mode name to use (according to /etc/fb.modes)

-fbmodeconfig

config file of modes (default /etc/fb.modes)

-monitor-hfreq, -monitor-vfreq, -monitor-dotclock

important values, see example.conf

If you want to change to a specific mode, then use

mplayer -vm -fbmode name_of_mode filename

     -vm alone will choose the most suitable mode from /etc/fb.modes. Can be used together with
     -x and -y options too. The -flip option is supported only if the movie's pixel format matches the

video mode's pixel format. Pay attention to the bpp value, fbdev driver tries to use the current, or if you specify the -bpp option, then that.

•

-zoom option isn't supported (use -vf scale). You can't use 8bpp (or less) modes.

• You possibly want to turn the cursor off:

echo -e '\033[?25l'

or

setterm -cursor off

and the screen saver:

setterm -blank 0

To turn the cursor back on:

echo -e '\033[?25h'

or

setterm -cursor on

•

Notatka

FBdev video mode changing does not work with the VESA framebuffer, and don't ask for it, since it's not an MPlayer limitation.

2.3.1.2.6. Matrox framebuffer (mga_vid)

This section is about the Matrox G200/G400/G450/G550 BES (Back-End Scaler) support, the mga_vid kernel driver. It's actively developed by A'rpi, and it has hardware VSYNC support with triple buffering. It works on both framebuffer console and under X.

Ostrze¿enie

This is Linux only! On non-Linux (tested on FreeBSD) systems, you can use VIDIX instead!

MPlayer - Odtwarzacz filmów dla LINUKSA

Installation:

To use it, you first have to compile mga_vid.o:

cd drivers
make

1.

Then create /dev/mga_vid device:

mknod /dev/mga_vid c 178 0

and load the driver with

insmod mga_vid.o

2.

You should verify the memory size detection using the dmesg command. If it's bad, use the

mga_ram_size option (rmmod mga_vid first), specify card's memory size in MB:

insmod mga_vid.o mga_ram_size=16

3.

To make it load/unload automatically when needed, first insert the following line at the end of

/etc/modules.conf:

alias char-major-178 mga_vid

Then copy the mga_vid.o module to the appropriate place under /lib/modules/kernel

version/somewhere.

Then run

depmod -a

4.

Now you have to (re)compile MPlayer, ./configure will detect /dev/mga_vid and build the 'mga' driver. Using it from MPlayer goes by -vo mga if you have matroxfb console, or -vo xmga under XFree86 3.x.x or 4.x.x. 5.

The mga_vid driver cooperates with Xv.

The /dev/mga_vid device file can be read for some info, for example by

cat /dev/mga_vid

and can be written for brightness change:

echo "brightness=120" > /dev/mga_vid

2.3.1.2.7. 3Dfx YUV support

This driver uses the kernel's tdfx framebuffer driver to play movies with YUV acceleration. You'll need a kernel with tdfxfb support, and recompile with

./configure --enable-tdfxfb

2.3.1.2.8. OpenGL output

MPlayer supports displaying movies using OpenGL, but if your platform/driver supports xv as should be the case on a PC with Linux, use xv instead, OpenGL performance is considerably worse. If you have an X11

MPlayer - Odtwarzacz filmów dla LINUKSA implementation without xv support, OpenGL is a viable alternative.

Unfortunately not all drivers support this feature. The Utah-GLX drivers (for XFree86 3.3.6) support it for all cards. See http://utah-glx.sourceforge.net for details about how to install it.

XFree86(DRI) 4.0.3 or later supports OpenGL with Matrox and Radeon cards, 4.2.0 or later supports Rage128. See http://dri.sourceforge.net for download and installation instructions.

A hint from one of our users: the GL video output can be used to get vsynced TV output. You'll have to set an environment variable (at least on nVidia):

export $__GL_SYNC_TO_VBLANK=1

2.3.1.2.9. AAlib - text mode displaying

AAlib is a library for displaying graphics in text mode, using powerful ASCII renderer. There are lots of programs already supporting it, like Doom, Quake, etc. MPlayer contains a very usable driver for it. If

./configure detects aalib installed, the aalib libvo driver will be built.

You can use some keys in the AA Window to change rendering options:

Key Action 1 decrease contrast 2 increase contrast 3 decrease brightness 4 increase brightness 5 switch fast rendering on/off 6 set dithering mode (none, error distribution, Floyd Steinberg) 7 invert image 8 toggles between aa and MPlayer control The following command line options can be used:

-aaosdcolor=V

change OSD color

-aasubcolor=V

change subtitle color

where V can be: 0 (normal), 1 (dark), 2 (bold), 3 (bold font), 4 (reverse), 5 (special).

AAlib itself provides a large sum of options. Here are some important:

-aadriver

set recommended aa driver (X11, curses, Linux)

-aaextended

use all 256 characters

-aaeight

use eight bit ASCII

-aahelp

prints out all aalib options

MPlayer - Odtwarzacz filmów dla LINUKSA

Notatka

The rendering is very CPU intensive, especially when using AA-on-X (using aalib on X), and it's least CPU intensive on standard, non-framebuffer console. Use SVGATextMode to set up a big textmode, then enjoy! (secondary head Hercules cards rock :)) (but imho you can use -vf 1bpp option to get graphics on hgafb:)

Use the -framedrop option if your computer isn't fast enough to render all frames!

Playing on terminal you'll get better speed and quality using the Linux driver, not curses (-aadriver

linux). But therefore you need write access on /dev/vcsa<terminal>! That isn't autodetected by

aalib, but vo_aa tries to find the best mode. See http://aa-project.sourceforge.net/tune for further tuning issues.

2.3.1.2.10. VESA - output to VESA BIOS

This driver was designed and introduced as a generic driver for any video card which has VESA VBE 2.0 compatible BIOS. Another advantage of this driver is that it tries to force TV output on. VESA BIOS EXTENSION (VBE) Version 3.0 Date: September 16, 1998 (Page 70) says:

Dual-Controller Designs. VBE 3.0 supports the dual-controller design by assuming that since both controllers are typically provided by the same OEM, under control of a single BIOS ROM on the same graphics card, it is possible to hide the fact that two controllers are indeed present from the application. This has the limitation of preventing simultaneous use of the independent controllers, but allows applications released before VBE 3.0 to operate normally. The VBE Function 00h (Return Controller Information) returns the combined information of both controllers, including the combined list of available modes. When the application selects a mode, the appropriate controller is activated. Each of the remaining VBE functions then operates on the active controller.

So you have chances to get working TV-out by using this driver. (I guess that TV-out frequently is standalone head or standalone output at least.)

ADVANTAGES

You have chances to watch movies if Linux even doesn't know your video hardware. • You don't need to have installed any graphics' related things on your Linux (like X11 (aka XFree86), fbdev and so on). This driver can be run from text-mode. • You have chances to get working TV-out. (It's known at least for ATI's cards). • This driver calls int 10h handler thus it's not an emulator - it calls real things of real BIOS in real-mode (actually in vm86 mode). • You can use VIDIX with it, thus getting accelerated video display and TV output at the same time! (Recommended for ATI cards.) • If you have VESA VBE 3.0+, and you had specified monitor-hfreq, monitor-vfreq,

monitor-dotclock somewhere (config file, or commandline) you will get the highest possible

refresh rate. (Using General Timing Formula). To enable this feature you have to specify all your monitor options.

•

DISADVANTAGES

It works only on x86 systems. • It can be used only by root. •

MPlayer - Odtwarzacz filmów dla LINUKSA

Currently it's available only for Linux. • WA¯NE

Don't use this driver with GCC 2.96! It won't work!

COMMAND LINE OPTIONS AVAILABLE FOR VESA

-vo vesa:opts

currently recognized: dga to force dga mode and nodga to disable dga mode. In dga mode you can enable double buffering via the -double option. Note: you may omit these parameters to enable autodetection of dga mode.

KNOWN PROBLEMS AND WORKAROUNDS

If you have installed NLS font on your Linux box and run VESA driver from text-mode then after terminating MPlayer you will have ROM font loaded instead of national. You can load national font again by using setsysfont utility from the Mandrake distribution for example. (Hint: The same utility is used for localization of fbdev).

•

Some Linux graphics drivers don't update active BIOS mode in DOS memory. So if you have such problem - always use VESA driver only from text-mode. Otherwise text-mode (#03) will be activated anyway and you will need restart your computer. •

Often after terminating VESA driver you get black screen. To return your screen to original state - simply switch to other console (by pressing Alt+F<x>) then switch to your previous console by the same way. •

To get working TV-out you need have plugged TV-connector in before booting your PC since video BIOS initializes itself only once during POST procedure. •

2.3.1.2.11. X11

Avoid if possible. Outputs to X11 (uses shared memory extension), with no hardware acceleration at all. Supports (MMX/3DNow/SSE accelerated, but still slow) software scaling, use the options -fs -zoom. Most cards have hardware scaling support, use the -vo xv output for them, or -vo xmga for Matroxes.

The problem is that most cards' driver doesn't support hardware acceleration on the second head/TV. In those cases, you see green/blue colored window instead of the movie. This is where this driver comes in handy, but you need powerful CPU to use software scaling. Don't use the SDL driver's software output+scaler, it has worse image quality!

Software scaling is very slow, you better try changing video modes instead. It's very simple. See the DGA section's modelines, and insert them into your XF86Config.

If you have XFree86 4.x.x: use the -vm option. It will change to a resolution your movie fits in. If it doesn't: • With XFree86 3.x.x: you have to cycle through available resolutions with the Ctrl+Alt+plus and Ctrl+Alt+minus keys. •

If you can't find the modes you inserted, browse XFree86's output. Some drivers can't use low pixelclocks that are needed for low resolution video modes.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1.2.12. VIDIX

PREAMBLE. VIDIX is the abbreviation for VIDeo Interface for *niX. VIDIX was designed and introduced as an interface for fast user-space drivers providing such video performance as mga_vid does for Matrox cards. It's also very portable.

This interface was designed as an attempt to fit existing video acceleration interfaces (known as mga_vid, rage128_vid, radeon_vid, pm3_vid) into a fixed scheme. It provides highlevel interface to chips which are known as BES (BackEnd scalers) or OV (Video Overlays). It doesn't provide lowlevel interface to things which are known as graphics servers. (I don't want to compete with X11 team in graphics mode switching). I.e. main goal of this interface is to maximize the speed of video playback.

USAGE

You can use standalone video output driver: -vo xvidix. This driver was developed as X11's front end to VIDIX technology. It requires X server and can work only under X server. Note that, as it directly accesses the hardware and circumvents the X driver, pixmaps cached in the graphics card's memory may be corrupted. You can prevent this by limiting the amount of video memory used by X with the XF86Config option "VideoRam" in the device section. You should set this to the amount of memory installed on your card minus 4MB. If you have less than 8MB of video ram, you can use the option "XaaNoPixmapCache" in the screen section instead.

•

There is a console VIDIX driver: -vo cvidix. This requires a working and initialized framebuffer for most cards (or else you'll just mess up the screen), and you'll have a similar effect as with -vo

mga or -vo fbdev. nVidia cards however are able to output truly graphical video on a real text

console. See the nvidia_vid section for more information.

•

You can use VIDIX subdevice which was applied to several video output drivers, such as: -vo

vesa:vidix (Linux only) and -vo fbdev:vidix.

•

Indeed it doesn't matter which video output driver is used with VIDIX.

REQUIREMENTS

Video card should be in graphics mode (except nVidia cards with the -vo cvidix output driver). • MPlayer's video output driver should know active video mode and be able to tell to VIDIX subdevice some video characteristics of server. •

USAGE METHODS. When VIDIX is used as subdevice (-vo vesa:vidix) then video mode configuration is performed by video output device (vo_server in short). Therefore you can pass into command line of MPlayer the same keys as for vo_server. In addition it understands -double key as globally visible parameter. (I recommend using this key with VIDIX at least for ATI's card). As for -vo xvidix, currently it recognizes the following options: -fs -zoom -x -y -double.

Also you can specify VIDIX's driver directly as third subargument in command line:

mplayer -vo xvidix:mga_vid.so -fs -zoom -double file.avi

or

mplayer -vo vesa:vidix:radeon_vid.so -fs -zoom -double -bpp 32 file.avi

But it's dangerous, and you shouldn't do that. In this case given driver will be forced and result is

MPlayer - Odtwarzacz filmów dla LINUKSA unpredictable (it may freeze your computer). You should do that ONLY if you are absolutely sure it will work, and MPlayer doesn't do it automatically. Please tell about it to the developers. The right way is to use VIDIX without arguments to enable driver autodetection.

VIDIX is new technology and it's extremely possible that on your system it won't work. In this case only solution for you it's port it (mainly libdha). But there is hope that it will work on those systems where X11 does.

Since VIDIX requires direct hardware access you can either run it as root or set the SUID bit on the MPlayer binary (Warning: This is a security risk!). Alternatively, you can use a special kernel module, like this:

Download the development version of svgalib (for example 1.9.17), OR download a version made by Alex especially for usage with MPlayer (it doesn't need the svgalib source to compile) from here. 1. Compile the module in the svgalib_helper directory (it can be found inside the

svgalib-1.9.17/kernel/ directory if you've downloaded the source from the svgalib site) and

insmod it. 2.

To create the neccessary devices in the /dev directory, do a

make device

in the svgalib_helper dir, as root.

3.

Move the svgalib_helper directory to mplayer/main/libdha/svgalib_helper. 4. Required if you download the source from the svgalib site: Remove the comment before the CFLAGS line containing "svgalib_helper" string from the libdha/Makefile. 5. Recompile and install libdha. 6. 2.3.1.2.12.1. ATI cards

Currently most ATI cards are supported natively, from Mach64 to the newest Radeons.

There are two compiled binaries: radeon_vid for Radeon and rage128_vid for Rage 128 cards. You may force one or let the VIDIX system autoprobe all available drivers.

2.3.1.2.12.2. Matrox cards

Matrox G200, G400, G450 and G550 have been reported to work.

The driver supports video equalizers and should be nearly as fast as the Matrox framebuffer

2.3.1.2.12.3. Trident cards

There is a driver available for the Trident Cyberblade/i1 chipset, which can be found on VIA Epia motherboards.

The driver was written and is maintained by Alastair M. Robinson

2.3.1.2.12.4. 3DLabs cards

Although there is a driver for the 3DLabs GLINT R3 and Permedia3 chips, no one has tested it, so reports are welcome.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1.2.12.5. nVidia cards

There's a relatively new nVidia driver out there, it's known to work on Riva 128, TNT and GeForce2 chipsets, also others have been reported working.

LIMITATIONS

It's recommended to use the binary nVidia drivers for X before using this VIDIX driver, because some of the registers which need to be initialized haven't been discovered yet, so it will probably fail with the Open Source XFree86 nv.o driver. •

Currently only codecs capable of UYVY colorspace output can work in conjunction with this driver. Unfortunately, this excludes every single decoder from the libavcodec family. This leaves us with the following usable popular codecs: cvid, divxds, xvid, divx4, wmv7, wmv8 and some others. Please note that this is only a temporal inconvenience. The usage syntax is as follows:

    mplayer -vf format=uyvy -vc divxds divx3file.avi

•

An unique feature of the nvidia_vid driver is its ability to display video on plain, pure, text-only console - with no framebuffer or X magic whatsoever. For this purpose, we'll have to use the cvidix video output, as the following example shows:

    mplayer -vf format=uyvy -vc divxds -vo cvidix example.avi

Reports awaited!

2.3.1.2.12.6. SiS cards

This is very experimental code, just like nvidia_vid.

It's been tested on SiS 650/651/740 (the most common chipsets used in the SiS versions of the "Shuttle XPC" barebones boxes out there)

Reports awaited!

2.3.1.2.13. DirectFB

"DirectFB is a graphics library which was designed with embedded systems in mind. It offers maximum hardware accelerated performance at a minimum of resource usage and overhead." - quoted from http://www.directfb.org

I'll exclude DirectFB features from this section.

Though MPlayer is not supported as a "video provider" in DirectFB, this output driver will enable video playback through DirectFB. It will - of course - be accelerated, on my Matrox G400 DirectFB's speed was the same as XVideo.

Always try to use the newest version of DirectFB. You can use DirectFB options on the command line, using the -dfbopts option. Layer selection can be done by the subdevice method, e.g.: -vo directfb:2 (layer -1 is default: autodetect)

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1.2.14. DirectFB/Matrox (dfbmga)

Please read the main DirectFB section or general informations.

This video output driver will enable CRTC2 (on the second head) on the Matrox G400/G450/G550 card, displaying video independently of the first head.

Instructions on how to make it work can be found in the tech section or directly on Ville Syrjala's home page.

Notatka

the first DirectFB version with which we could kick this working was 0.9.17 (it's buggy, needs that

surfacemanager patch from the URL above). Anyway, porting of the CRTC2 code to mga_vid is

underway.

2.3.1.3. MPEG decoders

2.3.1.3.1. DVB output and input

MPlayer supports cards with the Siemens DVB chipset from vendors like Siemens, Technotrend, Galaxis or Hauppauge. The latest DVB drivers are available from the Linux TV site. If you want to do software transcoding you should have at least a 1GHz CPU.

Configure should detect your DVB card. If it did not, force detection with

./configure --enable-dvb

If you have ost headers at a non-standard path, set the path with

./configure --with-extraincdir=DVB source directory/ost/include

Then compile and install as usual.

USAGE. Hardware decoding (playing standard MPEG1/2 files) can be done with this command:

mplayer -ao mpegpes -vo mpegpes file.mpg|vob

Software decoding or transcoding different formats to MPEG1 can be achieved using a command like this:

mplayer -ao mpegpes -vo mpegpes yourfile.ext
mplayer -ao mpegpes -vo mpegpes -vf expand yourfile.ext

Note that DVB cards only support heights 288 and 576 for PAL or 240 and 480 for NTSC. You must rescale for other heights by adding scale=width:height with the width and height you want to the -vf option. DVB cards accept various widths, like 720, 704, 640, 512, 480, 352 etc and do hardware scaling in horizontal direction, so you do not need to scale horizontally in most cases. For a 512x384 (aspect 4:3) DivX try:

mplayer -ao mpegpes -vo mpegpes -vf scale=512:576

If you have a widescreen movie and you do not want to scale it to full height, you can use the expand=w:h filter to add black bands. To view a 640x384 DivX, try:

MPlayer - Odtwarzacz filmów dla LINUKSA

mplayer -ao mpegpes -vo mpegpes -vf expand=640:576 file.avi

If your CPU is too slow for a full size 720x576 DivX, try downscaling:

mplayer -ao mpegpes -vo mpegpes -vf scale=352:576 file.avi

If speed does not improve, try vertical downscaling, too:

mplayer -ao mpegpes -vo mpegpes -vf scale=352:288 file.avi

For OSD and subtitles use the OSD feature of the expand filter. So, instead of expand=w:h or

expand=w:h:x:y, use expand=w:h:x:y:1 (the 5th parameter :1 at the end will enable OSD

rendering). You may want to move the image up a bit to get a bigger black zone for subtitles. You may also want to move subtitles up, if they are outside your TV screen, use the -subpos <0-100> option to adjust this (-subpos 80 is a good choice).

In order to play non-25fps movies on a PAL TV or with a slow CPU, add the -framedrop option.

To keep the aspect ratio of DivX files and get the optimal scaling parameters (hardware horizontal scaling and software vertical scaling while keeping the right aspect ratio), use the new dvbscale filter:

for a  4:3 TV: -vf dvbscale,scale=-1:0,expand=-1:576:-1:-1:1
for a 16:9 TV: -vf dvbscale=1024,scale=-1:0,expand=-1:576:-1:-1:1

Using your DVB card for watching Digital TV (DVB input module). First you need to pass the

dvb_shutdown_timeout=0 parameter to the kernel module dvb-core, or MPlayer will die after 10

seconds.

You should also have the programs scan and szap/tzap/czap installed; they are all included in the drivers package.

Verify that your drivers are working properly with a program such as dvbstream (that is the base of the DVB input module).

Now you should compile a ~/.mplayer/channels.conf file, with the syntax accepted by szap/tzap/czap, or have scan compile it for you.

Make sure that you have have only Free to Air channels in your channels.conf file, or MPlayer will hang on the others.

To show the first of the channels present in your list, run

  mplayer dvb://

If you want to watch a specific channel, such as R1, run

  mplayer dvb://R1

To change channels press the h (next) and k (previous) keys, or use the OSD menu (requires a working OSD subsystem).

MPlayer - Odtwarzacz filmów dla LINUKSA

If your ~/.mplayer/menu.conf contains a <dvbsel> entry, such as the one in the example file

etc/dvb-menu.conf (that you can use to overwrite ~/.mplayer/menu.conf), the main menu will

show a sub-menu entry that will permit you to choose one of the channels present in your

channels.conf.

If you want to save a program to disk you can use

  mplayer -dumpfile r1.ts -dumpstream dvb://R1

If you want to record it in a different format (re-encoding it) instead you can run a command such as

  mencoder -o r1.avi -ovc xvid -xvidencopts bitrate=800 -oac mp3lame -lameopts cbr:br=128 -pp=ci dvb://R1

Read the man page for a list of options that you can pass to the DVB input module.

FUTURE. If you have questions or want to hear feature announcements and take part in discussions on this subject, join our MPlayer-DVB mailing list. Please remember that the list language is English.

In the future you may expect the ability to display OSD and subtitles using the native OSD feature of DVB cards, as well as more fluent playback of non-25fps movies and realtime transcoding between MPEG2 and MPEG4 (partial decompression).

2.3.1.3.2. DXR2

MPlayer supports hardware accelerated playback with the Creative DXR2 card.

First of all you will need properly installed DXR2 drivers. You can find the drivers and installation instructions at the DXR2 Resource Center site.

USAGE

-vo dxr2

enable TV output

-vo dxr2:x11 or -vo dxr2:xv

enable Overlay output in X11

-dxr2 <option1:option2:...>

This option is used to control the DXR2 driver.

The overlay chipset used on the DXR2 is of pretty bad quality but the default settings should work for everybody. The OSD may be usable with the overlay (not on TV) by drawing it in the colorkey. With the default colorkey settings you may get variable results, usually you will see the colorkey around the characters or some other funny effect. But if you properly adjust the colorkey settings you should be able to get acceptable results.

Please see the manpage for available options.

2.3.1.3.3. DXR3/Hollywood+

MPlayer supports hardware accelerated playback with the Creative DXR3 and Sigma Designs Hollywood Plus cards. These cards both use the em8300 MPEG decoder chip from Sigma Designs.

MPlayer - Odtwarzacz filmów dla LINUKSA

First of all you will need properly installed DXR3/H+ drivers, version 0.12.0 or later. You can find the drivers and installation instructions at the DXR3 & Hollywood Plus for Linux site. configure should detect your card automatically, compilation should go without problems.

USAGE

-vo dxr3:prebuf:sync:norm=x:device
     overlay activates the overlay instead of TVOut. It requires that you have a properly configured

overlay setup to work right. The easiest way to configure the overlay is to first run autocal. Then run mplayer with dxr3 output and without overlay turned on, run dxr3view. In dxr3view you can tweak the overlay settings and see the effects in realtime, perhaps this feature will be supported by the MPlayer GUI in the future. When overlay is properly set up you will no longer need to use dxr3view.

prebuf turns on prebuffering. Prebuffering is a feature of the em8300 chip that enables it to hold

more than one frame of video at a time. This means that when you are running with prebuffering MPlayer will try to keep the video buffer filled with data at all times. If you are on a slow machine MPlayer will probably use close to, or precisely 100% of CPU. This is especially common if you play pure MPEG streams (like DVDs, SVCDs a.s.o.) since MPlayer will not have to reencode it to MPEG it will fill the buffer very fast. With prebuffering video playback is much less sensitive to other programs hogging the CPU, it will not drop frames unless applications hog the CPU for a long time. When running without prebuffering the em8300 is much more sensitive to CPU load, so it is highly suggested that you turn on MPlayer's -framedrop option to avoid further loss of sync. sync will turn on the new sync-engine. This is currently an experimental feature. With the sync feature turned on the em8300's internal clock will be monitored at all times, if it starts to deviate from MPlayer's clock it will be reset causing the em8300 to drop any frames that are lagging behind. norm=x will set the TV norm of the DXR3 card without the need for external tools like em8300setup. Valid norms are 5 = NTSC, 4 = PAL-60, 3 = PAL. Special norms are 2 (auto-adjust using PAL/PAL-60) and 1 (auto-adjust using PAL/NTSC) because they decide which norm to use by looking at the frame rate of the movie. norm = 0 (default) does not change the current norm. device = device number to use if you have more than one em8300 card. Any of these options may be left out. :prebuf:sync seems to work great when playing DivX movies. People have reported problems using the prebuf option when playing MPEG1/2 files. You might want to try running without any options first, if you have sync problems, or DVD subtitle problems, give :sync a try.

-ao oss:/dev/em8300_ma-X

For audio output, where X is the device number (0 if one card).

-aop list=resample:fout=xxxxx

The em8300 cannot play back samplerates lower than 44100Hz. If the sample rate is below 44100Hz select either 44100Hz or 48000Hz depending on which one matches closest. I.e. if the movie uses 22050Hz use 44100Hz as 44100 / 2 = 22050, if it is 24000Hz use 48000Hz as 48000 / 2 = 24000 and so on. This does not work with digital audio output (-ac hwac3).

-vf lavc/fame

To watch non-MPEG content on the em8300 (i.e. DivX or RealVideo) you have to specify an MPEG1 video filter such as libavcodec (lavc) or libfame (fame). At the moment lavc is both faster and gives better image quality, it is suggested that you use that unless you have problems with it. See the man page for further info about -vf lavc/fame. Using lavc is highly recommended. Currently there is no way of setting the fps of the em8300 which means that it is fixed to 29.97fps. Because of this it is highly recommended that you use -vf lavc=quality:25 especially if you are using prebuffering. Then why 25 and not 29.97? Well, the thing is that when you use 29.97 the picture becomes a bit jumpy. The reason for this is unknown to us. If you set it to somewhere between 25 and 27 the picture becomes stable. For now all we can do is accept this for a fact.

-vf expand=-1:-1:-1:-1:1

MPlayer - Odtwarzacz filmów dla LINUKSA

Although the DXR3 driver can put some OSD onto the MPEG1/2/4 video, it has much lower quality than MPlayer's traditional OSD, and has several refresh problems as well. The command line above will firstly convert the input video to MPEG4 (this is mandatory, sorry), then apply an expand filter which won't expand anything (-1: default), but apply the normal OSD onto the picture (that's what the "1" at the end does).

-ac hwac3

The em8300 supports playing back AC3 audio (surround sound) through the digital audio output of the card. See the -ao oss option above, it must be used to specify the DXR3's output instead of a soundcard.

2.3.1.4. Other visualization hardware

2.3.1.4.1. Zr

This is a display-driver (-vo zr) for a number of MJPEG capture/playback cards (tested for DC10+ and Buz, and it should work for the LML33, the DC10). The driver works by encoding the frame to JPEG and then sending it to the card. For the JPEG encoding libavcodec is used, and required. With the special cinerama mode, you can watch movies in true wide screen provided that you have two beamers and two MJPEG cards. Depending on resolution and quality settings, this driver may require a lot of CPU power, remember to specify -framedrop if your machine is too slow. Note: My AMD K6-2 350MHz is (with

-framedrop) quite adequate for watching VCD sized material and downscaled movies.

This driver talks to the kernel driver available at http://mjpeg.sourceforge.net, so you must get it working first. The presence of an MJPEG card is autodetected by the configure script, if autodetection fails, force detection with

./configure --enable-zr

The output can be controlled by several options, a long description of the options can be found in the man page, a short list of options can be viewed by running

mplayer -zrhelp

Things like scaling and the OSD (on screen display) are not handled by this driver but can be done using the video filters. For example, suppose that you have a movie with a resolution of 512x272 and you want to view it fullscreen on your DC10+. There are three main possibilities, you may scale the movie to a width of 768, 384 or 192. For performance and quality reasons, I would choose to scale the movie to 384x204 using the fast bilinear software scaler. The commandline is

mplayer -vo zr -sws 0 -vf scale=384:204 movie.avi

Cropping can be done by the crop filter and by this driver itself. Suppose that a movie is too wide for display on your Buz and that you want to use -zrcrop to make the movie less wide, then you would issue the following command

mplayer -vo zr -zrcrop 720x320+80+0 benhur.avi

if you want to use the crop filter, you would do

mplayer -vo zr -vf crop=720:320:80:0 benhur.avi

MPlayer - Odtwarzacz filmów dla LINUKSA

Extra occurrences of -zrcrop invoke cinerama mode, i.e. you can distribute the movie over several TV's or beamers to create a larger screen. Suppose you have two beamers. The left one is connected to your Buz at

/dev/video1 and the right one is connected to your DC10+ at /dev/video0. The movie has a

resolution of 704x288. Suppose also that you want the right beamer in black and white and that the left beamer should have JPEG frames at quality 10, then you would issue the following command

mplayer -vo zr -zrdev /dev/video0 -zrcrop 352x288+352+0 -zrxdoff 0 -zrbw \
          -zrcrop 352x288+0+0 -zrdev /dev/video1 -zrquality 10 movie.avi

You see that the options appearing before the second -zrcrop only apply to the DC10+ and that the options after the second -zrcrop apply to the Buz. The maximum number of MJPEG cards participating in cinerama is four, so you can build a 2x2 vidiwall.

Finally an important remark: Do not start or stop XawTV on the playback device during playback, it will crash your computer. It is, however, fine to FIRST start XawTV, THEN start MPlayer, wait for MPlayer to finish and THEN stop XawTV.

2.3.1.4.2. Blinkenlights

This driver is capable of playback using the Blinkenlights UDP protocol. If you don't know what Blinkenlights is, you don't need this driver.

2.3.1.5. TV-out support

2.3.1.5.1. Matrox G400 cards

Under Linux you have two methods to get G400 TV out working:

WA¯NE

for Matrox G450/G550 TV-out instructions, please see the next section!

XFree86

Using the driver and the HAL module, available from Matrox's site. This will give you X on the TV.

This method doesn't give you accelerated playback as under Windows! The second head has only YUV framebuffer, the BES (Back End Scaler, the YUV scaler on G200/G400/G450/G550 cards) doesn't work on it! The windows driver somehow workarounds this, probably by using the 3D engine to zoom, and the YUV framebuffer to display the zoomed image. If you really want to use X, use the

-vo x11 -fs -zoom options, but it will be SLOW, and has Macrovision copy protection

enabled (you can "workaround" Macrovision using this perl script). Framebuffer

Using the matroxfb modules in the 2.4 kernels. 2.2 kernels don't have the TVout feature in them, thus unusable for this. You have to enable ALL matroxfb-specific feature during compilation (except MultiHead), and compile them into modules! You'll also need I2C enabled.

Enter TVout and type ./compile.sh. Install TVout/matroxset/matroxset somewhere into your PATH. 1. If you don't have fbset installed, put TVout/fbset/fbset somewhere into your PATH. 2. If you don't have con2fb installed, put TVout/con2fb/con2fb somewhere into your

PATH.

3.

MPlayer - Odtwarzacz filmów dla LINUKSA

Then enter into the TVout/ directory in the MPlayer source, and execute ./modules as root. Your text-mode console will enter into framebuffer mode (no way back!). 4. Next, EDIT and run the ./matroxtv script. This will present you to a very simple menu. Press 2 and Enter. Now you should have the same picture on your monitor, and TV. If the TV (PAL by default) picture has some weird stripes on it, the script wasn't able to set the resolution correctly (to 640x512 by default). Try other resolutions from the menu and/or experiment with fbset.

5.

Yoh. Next task is to make the cursor on tty1 (or whatever) to disappear, and turn off screen blanking. Execute the following commands:

echo -e '\033[?25l'
setterm -blank 0

or

setterm -cursor off
setterm -blank 0

You possibly want to put the above into a script, and also clear the screen. To turn the cursor back:

echo -e '\033[?25h'

or

setterm -cursor on

6.

Yeah kewl. Start movie playing with

mplayer -vo mga -fs -screenw 640 -screenh 512 filename

(If you use X, now change to matroxfb with for example Ctrl+Alt+F1.) Change 640 and

512 if you set the resolution to other...

7.

Enjoy the ultra-fast ultra-featured Matrox TV output (better than Xv)! 8. Building a Matrox TV-out cable. No one takes any responsibility, nor guarantee for any damage caused by this documentation.

Cable for G400. The CRTC2 connector's fourth pin is the composite video signal. The ground are the sixth, seventh and eighth pins. (info contributed from Balázs Rácz)

Cable for G450. The CRTC2 connector's first pin is the composite video signal. The ground are the fifth, sixth, seventh, and fifteenth (5, 6, 7, 15) pins. (info contributed from Balázs Kerekes)

2.3.1.5.2. Matrox G450/G550 cards

TV output support for these cards has only been recently introduced, and is not yet in the mainstream kernel. Currently the mga_vid module can't be used AFAIK, because the G450/G550 driver works only in one configuration: the first CRTC chip (with much more features) on the first display (on monitor), and the second CRTC (no BES - for explanation on BES, please see the G400 section above) on TV. So you can only use MPlayer's fbdev output driver at the present.

MPlayer - Odtwarzacz filmów dla LINUKSA

The first CRTC can't be routed to the second head currently. The author of the kernel matroxfb driver - Petr Vandrovec - will maybe make support for this, by displaying the first CRTC's output onto both of the heads at once, as currently recommended for G400, see the section above.

The necessary kernel patch and the detailed howto is downloadable from http://www.bglug.ca/matrox_tvout/

2.3.1.5.3. ATI cards

PREAMBLE. Currently ATI doesn't want to support any of its TV-out chips under Linux, because of their licensed Macrovision technology.

ATI CARDS TV-OUT STATUS ON LINUX

ATI Mach64: supported by gatos. • ASIC Radeon VIVO: supported by gatos. • Radeon and Rage128: supported by MPlayer! Check VESA driver and VIDIX sections. • Rage Mobility P/M, Radeon, Rage 128, Mobility M3/M4: supported by atitvout. • On other cards, just use the VESA driver, without VIDIX. Powerful CPU is needed, though.

Only thing you need to do - Have the TV connector plugged in before booting your PC since video BIOS initializes itself only once during POST procedure.

2.3.1.5.4. Voodoo 3

Check this URL.

2.3.1.5.5. nVidia

First, you MUST download the closed-source drivers from http://nvidia.com. I will not describe the installation and configuration process because it does not cover the scope of this documentation.

After XFree86, XVideo, and 3D acceleration is properly working, edit your card's Device section in the

XF86Config file, according to the following example (adapt for your card/TV):

Section "Device"
        Identifier      "GeForce"
        VendorName      "ASUS"
        BoardName       "nVidia GeForce2/MX 400"
        Driver          "nvidia"
        #Option         "NvAGP" "1"
        Option          "NoLogo"
        Option          "CursorShadow"  "on"

        Option          "TwinView"
        Option          "TwinViewOrientation" "Clone"
        Option          "MetaModes" "1024x768,640x480"
        Option          "ConnectedMonitor" "CRT, TV"
        Option          "TVStandard" "PAL-B"
        Option          "TVOutFormat" "Composite"

EndSection

Of course the important thing is the TwinView part.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.1.5.6. Neomagic

Tested on a Toshiba Tecra 8000. Its TV output chip is a miserable crap. Avoid if possible.

You must use -vo vesa. The tested chip was capable of 1.333333 aspect ratio only, so be sure to use the

-x, -y options and/or the -vf scale,crop,expand filters if the box doesn't let you enable TV output.

Maximum resolution was 720*576 at 16bpp.

Known issues: VESA-only, 1.33333 limitation, image isn't always centered, movie becomes 4bpp in every 10 minutes, and stays that way. Frequent hard freezes, LCD display problems.

2.3.2. Urz±dzenia wyj¶ciowe audio

2.3.2.1. Synchronizacja Audio/Video

Interfejs audio MPlayera nazywa siê libao2. Obecnie zawiera on nastêpuj±ce sterowniki:

Sterownik Komentarz oss sterownik OSS (ioctl, sprzêtowa obs³uga AC3) sdl sterownik SDL (obs³uguje takie demony d¼wiêku jak: ESD i ARTS) nas sterownik NAS (Network Audio System) alsa5 rdzenny sterownik ALSA 0.5 alsa9 rdzenny sterownik ALSA 0.9 (sprzêtowa obs³uga AC3) sun rdzenny sterownik d¼wiêku SUN (/dev/audio) dla u¿ytkowników BSD i Solarisa 8 macosx rdzenny sterownik MacOSX win32 rdzenny sterownik Win32 arts rdzenny sterownik ARTS (g³ównie dla u¿ytkowników KDE) esd rdzenny sterownik ESD (g³ównie dla u¿ytkowników GNOMEa) Sterowniki kart d¼wiêkowych przeznaczone dla Linuksa maj± problemy zwi±zane z kompatybilno¶ci±. Dzieje siê tak, poniewa¿ MPlayer korzysta z wbudowanych w³a¶ciwo¶ci poprawnie napisanych sterowników d¼wiêku, które prawid³owo obs³uguj± synchronizacjê audio/video. Niestety, niektórzy autorzy sterowników nie uwzglêdniaj± tej cechy, poniewa¿ nie jest ona potrzebna do odtwarzania efektów d¼wiêkowych i plików MP3.

Inne odtwarzacze, takie jak: aviplay czy xine prawdopodobnie dzia³aj± od razu z tymi sterownikami, poniewa¿ u¿ywaj± "prostych" metod synchronizacji korzystaj±cych z wewnêtrznego zegara. Testy pokaza³y, ¿e ich metody nie s± tak wydajne jak MPlayera.

U¿ywanie MPlayera z poprawnie napisanym sterownikiem d¼wiêku, nigdy nie zaowocuje desynchronizacj± A/V z powodu d¼wiêku, chyba ¿e odtwarzany plik zosta³ utworzony w niew³a¶ciwy sposób lub jest popsuty (na stronie man znajdziesz mo¿liwe rozwi±zania tego problemu).

Je¶li masz kiepski sterownik d¼wiêku, spróbuj u¿yæ opcji -autosync. Powinna ona rozwi±zaæ Twój problem. Dok³adniejsze informacje znajdziesz na stronie man.

Kilka uwag:

MPlayer - Odtwarzacz filmów dla LINUKSA

Je¶li posiadasz sterownik OSS, spróbuj najpierw opcji -ao oss (domy¶lna). Je¿eli zauwa¿ysz niestabilne dzia³anie systemu, jego ci±g³e zawieszanie siê lub inne dziwne zachowanie, wypróbuj

-ao sdl (UWAGA: potrzebujesz zainstalowanych bibliotek i plików nag³ówkowych SDL).

Sterownik SDL pomaga w wielu wypadkach, a dodatkowo obs³uguje ESD (GNOME) i ARTS (KDE).

•

Je¿eli posiadasz sterowniki ALSA w wersji 0.5, prawie zawsze konieczne bêdzie u¿ycie -ao

alsa5, poniewa¿ ich kod emulacji OSS jest wadliwy i spowoduje b³±d MPlayera wy¶wietlaj±c

komunikat o tre¶ci podobnej do tej:

    DEMUXER: Za du¿o (945 w 8390980 bajtach) pakietów video w buforze!
    (DEMUXER: Too many (945 in 8390980 bytes) video packets in the buffer!)

•

Na Solarisie konieczne jest u¿ycie sterownika SUN przy pomocy opcji -ao sun, w przeciwnym wypadku nie bêdzie dzia³aæ ani audio, ani video. • Je¶li d¼wiêk przerywany jest krótkimi trzaskami podczas odtwarzania z CD-ROMu, w³±cz odmaskowywanie przerwañ, wpisuj±c np. hdparm -u1 /dev/cdrom (man hdparm). Jest to bardzo przydatne i opisane bardziej szczegó³owo w sekcji dotycz±cej CD-ROMu. •

2.3.2.2. Do¶wiadczenia zwi±zane z u¿ytkowaniem kart d¼wiêkowych i zalecenia

Przy stosowaniu Linuksa, zalecamy j±dro z serii 2.4.x. J±dro w wersji 2.2 nie by³o testowane.

Sterowniki kart d¼wiêkowych w Linuksie s± dostarczane g³ównie przez woln± wersjê OSS. Sterowniki te zosta³y zast±pione w wersji rozwojowej j±dra 2.5 przez system ALSA (Advanced Linux Sound Architecture). Je¿eli Twoja dystrybucja nie u¿ywa jeszcze ALSA, mo¿esz chcieæ j± wypróbowaæ, je¿eli bêdziesz mia³ jakie¶ k³opoty z d¼wiêkiem. Sterowniki ALSA generalnie przewy¿szaj± OSS pod wzglêdem zgodno¶ci, wydajno¶ci i mo¿liwo¶ci, Jednak niektóre karty s± obs³ugiwane wy³±cznie przez komercyjn± wersjê OSS z witryny 4Front Technologies. Obs³uguje ona równie¿ kilka innych systemów poza Linuksem.

KARTA D¬WIÊKOWA

STEROWNIK

Maks. czêstotliwo¶æ

(kHz)

Maks. liczba kana³ów

Maks. liczba aplikacji_{[a]}

OSS/Free ALSA OSS/Pro inne

Zintegrowane karty VIA (686/A/B, 8233, 8235) via82cxxx_audio snd-via82xx

4-48 kHz lub wy³±cznie 48 kHz, w zale¿no¶ci od uk³adu

Aureal Vortex 2 brak brak OK

Sterowniki do Aureala dla Linuksa bufor zwiêkszony do 32k

48 4.1 5+

SB Live!

Wyj¶cie analogowe-OK, SP/DIF nie dzia³a

Oba dzia³aj± Oba dzia³aj±

Sterowniki OSS Creative'a (obs³uga SP/DIF)

192 4.0/5.1 32

SB 128 PCI (es1371) OK ? 48 stereo 2

SB AWE 64 max 44kHz

¼le brzmi na 48kHz 48

MPlayer - Odtwarzacz filmów dla LINUKSA

GUS PnP brak OK OK 48 Gravis UltraSound ACE Gravis UltraSound MAX OK OK (?) 48

ESS 688 OK OK (?) 48

Karty C-Media (CMI8338/8738) OK OK SP/DIF jest obs³ugiwane przez ALSA 0.9.x

? 44 stereo 1

Karty Yamaha (*ymf*) z³e (?) (mo¿e

-ao sdl)

Dzia³a poprawnie tylko z ALSA 0.5 z w³±czon± emulacj± OSS i-ao sdl (!) (?) Karty z uk³adem envy24 (np. Terratec EWS88MT)

? ? OK ?

PC Speaker lub DAC OK brak

Sterowniki do PC speakera dla Linuksa (OSS)

Sterownik emuluje 44.1, mo¿e wiêcej.

mono 1

[a] liczba aplikacji, które mog± jednocze¶nie u¿ywaæ urz±dzenia. Pomoc przy tworzeniu tego dokumentu jest mile widziana. Powiedz jak MPlayer i Twoja karta d¼wiêkowa (karty d¼wiêkowe) wspó³pracuj± razem.

2.3.2.3. Filtry audio

Stare wtyczki audio zosta³y wyparte przez now± warstwê filtrów d¼wiêkowych. Mo¿na ich u¿ywaæ do zmiany w³a¶ciwo¶ci danych audio zanim d¼wiêk dotrze do karty. Ich uruchamianie i wy³±czanie odbywa siê przewa¿nie automatycznie, mo¿na to jednak zmieniæ. Filtry w³±czane s± wtedy, gdy cechy d¼wiêku ró¿ni± siê od tych wymaganych przez urz±dzenie audio, w przeciwnym wypadku procedura ta jest pomijana. Opcja

-af filter1,filter2,... u¿ywana jest do nadpisania automatycznych ustawieñ lub do zastosowania

dodatkowych. Kolejno¶æ stosowania filtrów uzale¿niona jest od kolejno¶ci w ci±gu oddzielonych od siebie przecinkami warto¶ci.

Przyk³ad:

mplayer -af resample,pan film.avi

uruchomi d¼wiêk poprzez filtr zmieniaj±cy czêstotliwo¶æ próbkowania (resample filter) a nastêpnie poprzez filtr pan. Zauwa¿, ¿e lista nie mo¿e zawieraæ ¿adnych spacji, inaczej zostanie b³êdnie zinterpretowana przez program.

MPlayer - Odtwarzacz filmów dla LINUKSA

Filtry czêsto posiadaj± opcje zmieniaj±ce ich zachowanie. S± one dok³adniej opisane w sekcji poni¿ej. Je¿eli pominie siê parametry, to filtr uruchomi siê z ustawieniami domy¶lnymi. Poni¿ej przedstawiony jest przyk³ad, jak u¿ywaæ filtrów wraz z ich opcjami:

mplayer -af resample=11025,pan=1:0.5:0.5 -channels 1 -srate 11025 media.avi

ustawi czêstotliwo¶æ wyj¶ciow± filtru zmieniaj±cego próbkowanie (resample filter) na 11025Hz i zmiksuje d¼wiêk do jednego kana³u u¿ywaj±c filtru pan.

Ogóln± kontrolê nad warstw± filtrów daje opcja -af-adv. Zawiera ona dwie dodatkowe opcje:

force jest polem bitowym, które okre¶la jak filtry s± stosowane i jakiej optymalizacji

prêdko¶ci/dok³adno¶ci u¿ywaj±:

0

U¿yj automatycznego stosowania filtrów i optymalizuj wzglêdem szybko¶ci procesora.

1

U¿yj automatycznego stosowania filtrów i optymalizuj tak, aby osi±gn±æ najwiêksz± prêdko¶æ. Uwaga: Niektóre mo¿liwo¶ci filtrów audio mog± nie zadzia³aæ i jako¶æ d¼wiêku spadnie.

2

U¿yj automatycznego stosowania filtrów i optymalizuj pod k±tem jak najwiêkszej jako¶ci.

3

Nie u¿ywaj automatycznego stosowania filtrów i nie optymalizuj. Uwaga: Je¶li u¿ywasz tego ustawienia, mo¿liwe jest wyst±pienie b³êdów podczas dzia³ania MPlayera i jego zakoñczenie.

4

U¿yj automatycznego stosowania filtrów (tak jak dla 0), jednak u¿yj obliczeñ zmiennoprzecinkowych, je¶li to mo¿liwe.

5

U¿yj automatycznego stosowania filtrów (tak jak dla 1), jednak u¿yj obliczeñ zmiennoprzecinkowych, je¶li to mo¿liwe.

6

U¿yj automatycznego stosowania filtrów (tak jak dla 2), jednak u¿yj obliczeñ zmiennoprzecinkowych, je¶li to mo¿liwe.

7

U¿yj automatycznego stosowania filtrów (tak jak dla 3), jednak u¿yj obliczeñ zmiennoprzecinkowych, je¶li to mo¿liwe.

list jest aliasem dla opcji -af.

Na zachowanie warstwy filtrów wp³ywaj± równie¿ ni¿ej podane, standardowe opcje:

-v

Zwiêksza poziom "gadatliwo¶ci" i sprawia, ¿e wiêkszo¶æ filtrów drukuje dodatkowe komunikaty.

-channels

Ustawia liczbê kana³ów wyj¶ciowych, których ma u¿ywaæ Twoja karta. Ma ona równie¿ wp³yw na liczbê kana³ów, które s± dekodowane z no¶nika danych. Je¶li zawiera on mniej kana³ów, filtr kana³ów (channels filter) zostanie automatycznie u¿yty (zobacz poni¿ej). Przekierowywanie kana³ów bêdzie ustawione domy¶lnie.

-srate

Ustawia czêstotliwo¶æ próbkowania, której ma u¿ywaæ Twoja karta (oczywi¶cie karty maj± swoje ograniczenia). Je¿eli poziom próbkowania Twojej karty ró¿ni siê od tego stosowanego w no¶niku,

MPlayer - Odtwarzacz filmów dla LINUKSA zostanie w³±czony filtr zmieniaj±cy próbkowanie (resample filter, zobacz poni¿ej), aby zniwelowaæ ró¿nice.

-format

Ustawia format próbki pomiêdzy filtrem audio a kart± d¼wiêkow±. Je¿eli ¿±dany format próbki dla karty jest inny ni¿ format zawieraj±cy siê w no¶niku, zostanie zastosowany filtr formatu (format filter, zobacz poni¿ej), aby zniwelowaæ ró¿nice.

2.3.2.3.1. Zmniejszenie/Zwiêkszenie czêstotliwo¶ci próbkowania (Up/Downsampling)

MPlayer w pe³ni obs³uguje zmniejszanie/zwiêkszanie czêstotliwo¶ci (up/downsampling) poprzez filtr zmieniaj±cy czêstotliwo¶æ próbkowania - resample filter. Mo¿e on byæ u¿yty, je¿eli masz sta³± czêstotliwo¶æ na karcie, albo je¿eli nie jest ona w stanie obs³u¿yæ wiêcej ni¿ 44.1kHz. Filtr jest automatycznie uruchamiany, je¿eli jest to konieczne, ale mo¿e równie¿ zostaæ w³±czony z poziomu linii poleceñ. Ma on trzy opcje:

srate <8000-192000>

jest to liczba ca³kowita, u¿ywana do okre¶lenia wyj¶ciowej czêstotliwo¶ci próbkowania w Hz. Przyjmuje warto¶ci z zakresu od 8kHz do 192kHz. Je¿eli czêstotliwo¶æ wej¶ciowa i wyj¶ciowa s± takie same albo je¿eli ten parametr jest pominiêty, filtr jest wy³±czany. Wysoka czêstotliwo¶æ przewa¿nie zwiêksza jako¶æ d¼wiêku, szczególnie je¿eli filtr jest u¿yty wraz z innymi.

sloppy

jest dodatkowym parametrem binarnym, który pozwala na ma³± ró¿nicê miêdzy czêstotliwo¶ci± wyj¶ciow± a t± podan± przez srate. Opcja ta mo¿e zostaæ u¿yta je¿eli pocz±tek odtwarzania jest bardzo wolny. Jest standardowo uruchomiony.

type <0-2>

jest dodatkow± liczb± ca³kowit± z przedzia³u od 0 do 2, która wybiera metodê zmiany czêstotliwo¶ci próbkowania. Tutaj 0 przedstawia interpolacjê liniow± (linear interpolation), 1 reprezentuje metodê wielofazowego przetwarzania banku filtrów (poly-phase filter-bank processing) przy u¿yciu obliczeñ ca³kowitoliczbowych, 2 do zmiany czêstotliwo¶ci za pomoc± wielofazowego przetwarzania banku filtrów (poly-phase filter-bank processing) i obliczeñ zmiennoprzecinkowych. Interpolacja liniowa (linear interpolation) jest wyj±tkowo szybka, jednak pogarsza jako¶æ d¼wiêku szczególnie przy zwiêkszaniu czêstotliwo¶ci (upsampling). Najlepsz± jako¶æ daje 2, ale metoda ta wymaga najwiêkszej mocy obliczeniowej.

Przyk³ad:

mplayer -af resample=44100:0:0

ustawi czêstotliwo¶æ wyj¶ciow± filtru zmieniaj±cego czêstotliwo¶æ próbkowania (resample filter) na 44100Hz u¿ywaj±c przy tym dok³adnego skalowania czêstotliwo¶ci wyj¶ciowej oraz interpolacji liniowej (linear interpolation).

2.3.2.3.2. Zmiana liczby kana³ów

Filtr kana³ów (channels filter) mo¿na u¿yæ w celu dodania lub usuniêcia kana³ów, mo¿na go tak¿e u¿yæ do kopiowania lub przekierowywania kana³ów. Jest on automatycznie w³±czony, je¿eli wyj¶cie warstwy audio filtrów ró¿ni siê od wej¶ciowego lub je¶li za¿±dano jego uruchomienia. Filtr wy³±cza siê sam, je¿eli nie jest u¿ywany. Liczba parametrów jest dynamiczna:

nch <1-6>

jest to liczba ca³kowita z zakresu od 1 do 6, która ustawia liczbê kana³ów wyj¶ciowych. Ta opcja jest wymagana. Nie podanie jej spowoduje b³±d uruchamiania (runtime error) programu.

MPlayer - Odtwarzacz filmów dla LINUKSA nr <1-6>

jest to liczba ca³kowita z zakresu od 1 do 6, która u¿ywana jest do okre¶lenia liczby dróg przekierowania. Parametr ten jest opcjonalny. Je¿eli jest pominiêty, stosowane jest domy¶lne przekierowanie.

od1:do1:od2:do2:od3:do3...

to pary liczb pomiêdzy 0 a 5, które okre¶laj± gdzie poszczególne kana³y maj± byæ przekierowywane.

Je¿eli podana jest tylko opcja nch, filtr u¿ywa domy¶lnego przekierowywanie, które dzia³a nastêpuj±co: Je¶li liczba kana³ów wyj¶ciowych jest wiêksza ni¿ wej¶ciowych, tworzone s± puste kana³y (w przypadku miksowania z mono do stereo, kana³ mono jest powtarzany w obu kana³ach wyj¶ciowych). Je¿eli liczba kana³ów wyj¶ciowych jest mniejsza ni¿ wej¶ciowych, nadmiarowe kana³y s± usuwane.

Przyk³ad 1:

mplayer -af channels=4:4:0:1:1:0:2:2:3:3 media.avi

zmieni liczbê kana³ów na 4 i ustawi 4 drogi przekierowywania, które zamieniaj± kana³ 1 z 0, a 2 i 3 pozostawiaj± bez zmian. Zauwa¿, ¿e je¿eli odtwarzany by³ no¶nik zawieraj±ce 2 kana³y, to kana³y 2 i 3 bêd± puste, ale 0 i 1 nadal bêd± zamienione.

Przyk³ad 2:

mplayer -af channels=6:4:0:0:0:1:0:2:0:3 media.avi

zmieni liczbê kana³ów na 6 i ustawi 4 drogi przekierowywania, które skopiuj± kana³ 0 do 0 i 3. Kana³y 4 i 5 bêd± puste.

2.3.2.3.3. Konwerter formatu próbek (sample format converter)

Filtr formatu (format filter) przekszta³ca jedne formaty próbek w inne. Jest uruchamiany automatycznie, je¶li tylko jest wymagany przez kartê lub inny filtr d¼wiêkowy.

bps <numer>

mo¿e mieæ warto¶æ 1, 2 lub 4, okre¶la liczbê bajtów przypadaj±c± na próbkê. Parametr ten jest wymagany. Nie podanie go spowoduje b³±d uruchamiania (runtime error).

f <format>

jest ci±giem znaków okre¶laj±cym format próbki. Ci±g jest kombinacj±: alaw, mulaw lub

imaadpcm, float lub int, unsigned lub signed, le lub be (little lub big endian). Opcja ta

jest wymagana. Jej nie podanie, spowoduje b³±d podczas uruchamiania (runtime error).

Przyk³ad:

mplayer -af format=4:float media.avi

ustawi format wyj¶ciowy na 4 bajty danych zmiennoprzecinkowych przypadaj±cych na próbkê.

2.3.2.3.4. Opó¼nienie (delay)

Filtr opó¼niaj±cy (delay filter) opó¼nia d¼wiêk zmierzaj±cy do g³o¶ników, tak ¿eby strumienie d¼wiêkowe z ró¿nych kana³ów dotar³y do nich jednocze¶nie. Jest to u¿yteczne, je¿eli masz wiêcej ni¿ 2 g³o¶niki. Filtr ma kilka opcji:

d1:d2:d3...

MPlayer - Odtwarzacz filmów dla LINUKSA s± liczbami rzeczywistymi okre¶laj±cymi opó¼nienie w milisekundach, które powinno byæ zastosowane do ka¿dego kana³u. Minimalna warto¶æ to 0ms a maksymalna to 1000ms.

Aby obliczyæ opó¼nienie dla poszczególnych kana³ów, wykonaj nastêpuje czynno¶ci:

Oblicz odleg³o¶æ od g³o¶ników do pozycji s³uchacza (w metrach), to da Ci warto¶ci od s1 do s5 (dla systemu 5.1). Nie ma sensu braæ pod uwagê subwoofera (i tak nie us³yszysz ró¿nicy). 1. Odejmij odleg³o¶æ od s1 do s5 od odleg³o¶ci maksymalnej tzn. s[i] = max(s) - s[i]; i = 1...5 2. Oblicz opó¼nienia w nastêpuj±cy sposób d[i] = 1000*s[i]/342; i = 1...5 3. Przyk³ad:

mplayer -af delay=10.5:10.5:0:0:7:0 media.avi

opó¼ni lewy i prawy przedni g³o¶nik o 10.5ms, dwa tylne i subwoofer o 0ms a centralny o 7ms.

2.3.2.3.5. Programowa regulacja g³o¶no¶ci (software volume control)

Programowa regulacja g³o¶no¶ci (software volume control) jest obs³ugiwana poprzez filtr g³o¶no¶ci (volume filter). U¿ywaj go ostro¿nie, gdy¿ mo¿e obni¿yæ stosunek sygna³u do szumu. W wiêkszo¶ci wypadków najlepszym rozwi±zaniem jest ustawienie miksera PCM na maksymaln± warto¶æ, wy³±czenie filtru i regulacja g³o¶no¶ci poziomem g³o¶no¶ci ogólnej miksera. Je¿eli Twoja karta ma cyfrowy mikser PCM zamiast analogowego i zauwa¿ysz przek³amania, u¿yj miksera MASTER. Je¿eli do komputera pod³±czony jest zewnêtrzny wzmacniacz (co zazwyczaj ma miejsce), poziom ha³asu mo¿e zostaæ zredukowany poprzez dostrojenie g³ównego poziomu g³o¶no¶ci (master level) i pokrêt³a g³o¶no¶ci, dopóki syczenie w tle nie ustanie. Filtr ma dwie opcje:

v <-200 - +60>

jest liczb± rzeczywist± pomiêdzy -200 a +60, która przedstawia poziom g³o¶no¶ci w dB. Domy¶lny poziom to 0dB.

c

jest binarn± warto¶ci± która w³±cza lub wy³±cza miêkkie obcinanie (soft-clipping). Miêkkie obcinanie (soft-clipping) mo¿e sprawiæ, ¿e d¼wiêk bêdzie ³agodniejszy, je¿eli wysokie poziomy d¼wiêku s± u¿yte. Uaktywnij tê opcjê, je¿eli moc g³o¶ników jest zbyt niska. Zwróæ uwagê, ¿e ta metoda powoduje przek³amania i powinna byæ u¿ywana tylko w ostateczno¶ci.

Przyk³ad:

mplayer -af volume=10.1:0 media.avi

wzmocni d¼wiêk o 10.1dB i zastosuje metodê twardego obcinania (hard-clip), je¿eli poziom d¼wiêku jest za wysoki.

Ten filtr ma drug± w³a¶ciwo¶æ: Mierzy ogólny, maksymalny poziom d¼wiêku i wypisuje go po zakoñczeniu MPlayera. Oszacowana g³o¶no¶æ mo¿e byæ u¿yta do ustawienia poziomu d¼wiêku w MEncoderze tak, ¿eby maksymalny zasiêg dynamiczny by³ mo¿liwy do osi±gniêcia.

2.3.2.3.6. Korektor (equalizer)

Filtr korektora (equalizer filter) to 10 oktawowy korektor graficzny zaimplementowany przy pomocy 10 filtrów pasmowych IIR. Oznacza to, ¿e dzia³a bez wzglêdu na format odtwarzanego d¼wiêku. ¦rodkowe czêstotliwo¶ci dla tych 10 pasm to:

MPlayer - Odtwarzacz filmów dla LINUKSA

Numer pasma Czêstotliwo¶æ ¶rodkowa 0 31.25 Hz 1 62.50 Hz 2 125.0 Hz 3 250.0 Hz 4 500.0 Hz 5 1.000 kHz 6 2.000 kHz 7 4.000 kHz 8 8.000 kHz 9 16.00 kHz Je¿eli czêstotliwo¶æ próbkowania odtwarzanego d¼wiêku jest ni¿sza ni¿ ¶rodkowa czêstotliwo¶æ dla odpowiedniego pasma, to jest ono wy³±czane. Znanym b³êdem jest to, ¿e w³a¶ciwo¶ci dla najwy¿szego pasma nie s± ca³kowicie symetryczne, je¿eli czêstotliwo¶æ próbki jest zbli¿ona do czêstotliwo¶ci ¶rodkowej danego pasma. Mo¿na obej¶æ ten problem zwiêkszaj±c jej czêstotliwo¶æ (up-sampling), zanim ta dotrze do filtru korektora (equalizer filter).

Filtr ma 10 parametrów:

g1:g2:g3...g10

s± liczbami rzeczywistymi z przedzia³u od -12 do +12, okre¶laj±cymi przyrost dB dla ka¿dego pasma czêstotliwo¶ci.

Przyk³ad:

mplayer -af equalizer=11:11:10:5:0:-12:0:5:12:12 media.avi

wzmocni d¼wiêk w wy¿szych i ni¿szych zakresach czêstotliwo¶ci, wyciszaj±c go prawie ca³kowicie oko³o 1kHz.

2.3.2.3.7. Filtr pan (panning filter)

U¿yj filtru pan (pan filter), ¿eby dowolnie miksowaæ kana³y. Najpro¶ciej t³umacz±c jest to po³±czenie programowej regulacji g³o¶no¶ci (software volume control) i filtru kana³ów (channels filter). Istniej± dla niego 2 podstawowe zastosowania:

Miksowanie wielu kana³ów w mniejsz± liczbê, na przyk³ad stereo do mono. 1. Zmienianie "szeroko¶ci" centralnego g³o¶nika w systemie przestrzennym. 2. Filtr jest trudny w u¿yciu i bêdzie wymaga³ zastosowania ¿mudnej metody prób i b³êdów, zanim zostanie osi±gniêty oczekiwany rezultat. Liczba parametrów filtru zale¿y od liczby kana³ów:

nch <1-6>

jest liczb± ca³kowit± z przedzia³u od 1 do 6 i jest u¿ywana w celu okre¶lenia liczby kana³ów wyj¶ciowych. Opcja ta jest wymagana. Nie podanie jej spowoduje b³±d uruchamiania (runtime error).

l00:l01:l02:..l10:l11:l12:...ln0:ln1:ln2:...

s± liczbami rzeczywistymi z przedzia³u od 0 do 1. l[i][j] ustala ile procent kana³u wej¶ciowego j ma byæ zmiksowanych do kana³u wyj¶ciowego i.

Przyk³ad 1:

MPlayer - Odtwarzacz filmów dla LINUKSA

mplayer -af pan=1:0.5:0.5 -channels 1 media.avi

zmiksuje kana³y ze stereo do mono.

Przyk³ad 2:

mplayer -af pan=3:1:0:1:0.5:0.5 -channels 3 media.avi

da 3 kana³ wyj¶ciowy, zostawiaj±c 0 i 1 nietkniête i miksuj±c kana³y 0 i 1 do 2 kana³u wyj¶ciowego (który mo¿e byæ na przyk³ad wys³any do subwoofera).

2.3.2.3.8. Subwoofer

Filtr subwoofera (sub filter) dodaje kana³ subwoofera do strumienia audio. Dane audio u¿yte do stworzenia tego kana³u s± ¶redni± d¼wiêku w 0 i 1 kanale. D¼wiêk wynikowy zostanie poddany dzia³aniu dolnoprzepustowego filtru Butterwortha czwartego rzêdu (4th order Butterworth filter) z domy¶ln± czêstotliwo¶ci± graniczn± na poziomie 60Hz i dodany do oddzielnego kana³u w strumieniu audio. Uwaga: Wy³±cz ten filtr, je¿eli odtwarzasz DVD z d¼wiêkiem w systemie Dolby Digital 5.1, w przeciwnym wypadku, jego dzia³anie zak³óci d¼wiêk subwoofera. Filtr ma 2 parametry:

fc <20-300>

jest opcjonaln± liczb± rzeczywist±, u¿ywan± do okre¶lenia warto¶ci czêstotliwo¶ci granicznej w Hz. Prawid³owy zakres wynosi od 20Hz do 300Hz. Dla uzyskania najlepszego rezultatu, spróbuj ustawiæ j± na jak najni¿sz±. Wzbogaci to do¶wiadczenia p³yn±ce z u¿ywania d¼wiêku stereo i w systemie przestrzennym. Domy¶ln± warto¶ci± jest 60Hz.

ch <0-5>

jest opcjonaln± liczb± ca³kowit± pomiêdzy 0 a 5, która okre¶la numer kana³u, do którego ma zostaæ wys³any d¼wiêk subwoofera. Domy¶lnym jest 5. Zauwa¿, ¿e liczb± kana³ów zwiêkszy siê doch, je¿eli zajdzie taka potrzeba.

Przyk³ad:

mplayer -af sub=100:4 -channels 5 media.avi

doda kana³ subwoofera z czêstotliwo¶ci± graniczn± równ± 100Hz do 4 kana³u wyj¶ciowego.

2.3.2.3.9. Dekoder d¼wiêku przestrzennego (Surround-sound decoder)

Macierzowo zakodowany d¼wiêk przestrzenny, mo¿e byæ zdekodowany filtrem przestrzennym (surround filter). Dolby Surround jest przyk³adem formatu zakodowanego macierzowo. Wiele plików zawieraj±cych 2 kana³y audio, w rzeczywisto¶ci zawiera d¼wiêk przestrzenny zakodowany w tym systemie. Aby u¿yæ tego filtru potrzebujesz karty z obs³ug± przynajmniej 4 kana³ów. Filtr posiada jedn± opcjê:

d <0-1000>

jest opcjonaln± liczb± rzeczywist± pomiêdzy 0 a 1000, u¿ywan± do ustawienia opó¼nienia w ms dla tylnych g³o¶ników. Opó¼nienie powinno byæ ustawione w nastêpuj±cy sposób: je¶li d1 to odleg³o¶æ od pozycji s³uchacza do przednich g³o¶ników a d2 to odleg³o¶æ od tylnych g³o¶ników, to opó¼nienie d powinno byæ ustawione na 15ms, je¿eli d1 <= d2 i 15 + 5*(d1-d2) je¿eli d1 > d2. Domy¶lna warto¶æ dla d to 20ms.

Przyk³ad:

mplayer -af surround=15 -channels 4 media.avi

MPlayer - Odtwarzacz filmów dla LINUKSA doda d¼wiêk przestrzenny dekoduj±c d¼wiêk dla tylnych g³o¶ników z opó¼nieniem 15ms.

2.3.2.3.10. Audio Exporter

Ten filtr audio eksportuje nadchodz±cy sygna³ do innych procesów, u¿ywaj±c mapowania pamiêci (mmap()). Zmapowane obszary zawieraj± nag³ówek:

int nch                      /*ilo¶æ kana³ów*/
int size                     /*rozmiar bufora*/
unsigned long long counter   /*U¿ywany do zachowania synchronizacji,
                               aktualizowany za ka¿dym razem kiedy
                               eksportowane s± nowe dane.*/

Reszta to 16-bitowe dane (bez przeplotu).

mmapped_file

Plik, do którego chcesz eksportowaæ. Domy¶lnie jest to ~/.mplayer/mplayer-af_export.

nsamples

Ilo¶æ próbek przypadaj±cych na kana³. Domy¶lnie jest to 512.

Przyk³ad:

mplayer -af export=/tmp/mplayer-af_export:1024 media.avi

wyeksportuje 1024 próbek na kana³ do /tmp/mplayer-af_export. 2.3.2.4. Wtyczki Audio (odradzane)

Notatka

Wtyczki audio zosta³y zast±pione przez filtry audio i wkrótce zostan± usuniête.

MPlayer ma obs³ugê wtyczek audio. Mog± one byæ u¿yte do zmiany w³a¶ciwo¶ci danych audio, zanim d¼wiêk dotrze do karty. W³±cza je siê poprzez opcjê -aop, która przyjmuje argumenty w postaci

list=wtyczka1,wtyczka2,.... Argument list jest wymagany i okre¶la, które wtyczki powinny

zostaæ u¿yte i w jakiej kolejno¶ci. Przyk³ad:

mplayer media.avi -aop list=resample,format

przepu¶ci d¼wiêk przez wtyczkê zmieniaj±c± czêstotliwo¶æ próbkowania (resampling plugin) a nastêpnie wtyczkê formatu (format plugin).

Wtyczki równie¿ posiadaj± parametry, które zmieniaj± ich zachowanie. Opisane s± one dok³adniej w sekcji poni¿ej. Wtyczka uruchomi siê z domy¶lnymi warto¶ciami, je¿eli pominiemy jej opcje. Poni¿ej podany jest przyk³ad u¿ycia wtyczek i ich specyficznych ustawieñ:

mplayer media.avi -aop list=resample,format:fout=44100:format=0x8

ustawi czêstotliwo¶æ wyj¶ciow± dla wtyczki zmieniaj±cej czêstotliwo¶æ próbkowania (resample plugin) na 44100 Hz i format wyj¶ciowy wtyczki formatu (format plugin) na AFMT_U8.

Obecnie wtyczki audio nie mog± zostaæ u¿yte w MEncoderze.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.2.4.1. Zwiêkszanie/Zmniejszanie czêstotliwo¶ci próbkowania (up/downsampling)

MPlayer w pe³ni obs³uguje zmniejszanie/zwiêkszanie czêstotliwo¶ci próbkowania (up/downsampling) d¼wiêku. Wtyczka ta mo¿e byæ u¿yta, je¿eli masz kartê ze sta³± czêstotliwo¶ci± lub posiadasz kartê, która nie jest w stanie obs³u¿yæ wiêcej ni¿ 44.1 kHz. Ograniczenia Twojego sprzêtu nie s± automatycznie wykrywane, wiêc musisz wyra¼nie podaæ czêstotliwo¶æ. Wtyczka ma jeden prze³±cznik: fout, który u¿ywany jest do ustawiania ¿±danej czêstotliwo¶ci wyj¶ciowej. Domy¶ln± warto¶ci± jest 48 kHz i podawana jest w Hz.

Sposób u¿ycia:

mplayer media.avi -aop list=resample:fout=freq

gdzie freq jest czêstotliwo¶ci± w Hz, jak 44100.

Notatka

Czêstotliwo¶æ wyj¶ciow± nie powinna byæ wy¿sza ni¿ warto¶æ domy¶lna. Spowoduje to odtwarzanie strumieni audio i video w zwolnionym tempie oraz zak³ócenia d¼wiêku.

2.3.2.4.2. Dekodowanie d¼wiêku przestrzennego

MPlayer posiada wtyczkê, która umo¿liwia dekodowanie macierzowo zakodowanego d¼wiêku przestrzennego. Dolby Surround jest przyk³adem takiego formatu. Wiele plików zawieraj±cych 2 kana³y audio w rzeczywisto¶ci zawiera d¼wiêk przestrzenny zakodowany macierzowo. Aby skorzystaæ z tej w³a¶ciwo¶ci potrzebujesz karty z obs³ug± przynajmniej 4 kana³ów.

Sposób u¿ycia:

mplayer media.avi -aop list=surround

2.3.2.4.3. Konwerter formatu próbek (sample format converter)

Je¿eli Twój sterownik do karty d¼wiêkowej nie obs³uguje 16-bitowego typu danych ze znakiem, wtyczka ta mo¿e byæ u¿yta do jego zmiany na format zrozumia³y dla karty. Posiada jeden parametr - format, który mo¿e byæ ustawiony na jedn± z warto¶ci umieszczonych w libao2/afmt.h. Wtyczka ta jest raczej rzadko potrzebna i jest przeznaczona dla zaawansowanych u¿ytkowników. Mniej na uwadze, ¿e zmienia ona tylko format próbki a nie jej czêstotliwo¶æ czy ilo¶æ kana³ów.

Sposób u¿ycia:

mplayer media.avi -aop list=format:format=outfmt

gdzie outfmt to wymagany format próbki.

2.3.2.4.4. Opó¼nianie

Wtyczka opó¼nia d¼wiêk i jest przyk³adem tego, jak tworzyæ nowe wtyczki. Nie ma dla niej ¿adnego sensownego zastosowania z punktu widzenia u¿ytkownika i wspomnia³em tylko o niej ze wzglêdu na kompletno¶æ tej dokumentacji. Nie u¿ywaj tej wtyczki, chyba ¿e jeste¶ deweloperem.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.3.2.4.5. Programowa regulacja g³o¶no¶ci± (software volume control)

Wtyczka jest programowym odpowiednikiem regulacji g³o¶no¶ci± i mo¿e byæ u¿ywana na maszynach z uszkodzonym urz±dzeniem miksuj±cym. Mo¿e byæ równie¿ przydatna, je¿eli kto¶ chce zmieniæ poziom wyj¶ciowy g³o¶no¶ci w MPlayerze bez zmiany ustawieñ PCM w mikserze. Ma jeden parametr - volume, który s³u¿y do ustawienia pocz±tkowej g³o¶no¶ci. Mo¿e przyjmowaæ warto¶ci pomiêdzy 0 a 255. Warto¶ci± domy¶lna jest 101, co odpowiada wzmocnieniu równemu 0dB. U¿ywaj tej wtyczki ostro¿nie, gdy¿ mo¿esz obni¿yæ stosunek sygna³u do szumu. W wiêkszo¶ci wypadków najlepszym rozwi±zaniem jest ustawienie miksera PCM na maksymaln± warto¶æ i, zamiast wtyczk±, regulowaæ g³o¶no¶æ przy pomocy g³o¶ników. Je¿eli do komputera pod³±czony jest zewnêtrzny wzmacniacz (a zazwyczaj jest), poziom ha³asu mo¿e zostaæ zredukowany poprzez dostrojenie g³ównego poziomu g³o¶no¶ci (master level) i pokrêt³a g³o¶no¶ci, dopóki syczenie w tle nie ustanie.

Sposób u¿ycia:

mplayer media.avi -aop list=volume:volume=0-255

Wtyczka ma równie¿ kompresor lub zdolno¶æ do miêkkiego obcinania (soft-clipping). Kompresja mo¿e byæ u¿yta, je¿eli dynamika d¼wiêku jest bardzo wysoka lub je¿eli moc g³o¶ników jest zbyt niska. B±d¼ ostro¿ny, poniewa¿ ta funkcja powoduje zak³ócenia d¼wiêku i powinna byæ u¿yta w ostateczno¶ci.

Sposób u¿ycia:

mplayer media.avi -aop list=volume:softclip

2.3.2.4.6. Extrastereo

Wtyczka (liniowo) zwiêksza ró¿nicê pomiêdzy lewym a prawym kana³em (jak wtyczka extrastereo w XMMS), co dodaje efekt "na ¿ywo" do odtwarzanego d¼wiêku.

Sposób u¿ycia:

mplayer media.avi -aop list=extrastereo
mplayer media.avi -aop list=extrastereo:mul=3.45

Wspó³czynnikiem (mul) jest liczba rzeczywista, której warto¶æ domy¶lna to 2.5. Je¿eli ustawisz go na 0.0, otrzymasz d¼wiêk mono (¶rednia obu kana³ów). Je¶li na 1.0, nic siê nie zmieni, a je¶li na -1.0, lewy i prawy kana³ zostan± zamienione.

2.3.2.4.7. Normalizator g³o¶no¶ci (volume normalizer)

Wtyczka ustawia maksymalny poziom d¼wiêku, bez powodowania zak³óceñ.

Sposób u¿ycia:

mplayer media.avi -aop list=volnorm

2.4. Wej¶cie TV

Sekcja ta opisuje jak ogl±daæ/nagrywaæ obraz za pomoc± tunera TV kompatybilnego z V4L. Zajrzyj do strony man by zobaczyæ opis opcji TV i klawiszy steruj±cych.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.4.1. Kompilacja

Najpierw musisz przekompilowaæ. ./configure wykryje automatycznie nag³ówki j±dra zwi±zane z V4L i obecno¶æ urz±dzeñ /dev/video*. Je¶li istniej±, obs³uga TV zostanie wbudowana (zobacz wynik dzia³ania ./configure). 1.

Upewnij siê, ¿e Twój tuner dzia³a z innymi programami do obs³ugi TV pod Linuksem, na przyk³ad XawTV. 2. 2.4.2. Wskazówki u¿ytkowania

Kompletna lista opcji dostêpna jest na stronie man. Tu jest tylko kilka wskazówek:

U¿ywaj opcji channels. Przyk³ad

-tv channels=26-MTV1,23-TV2

Wyja¶nienie: u¿ywaj±c tej opcji, tylko kana³y 23 i 26 bêd± dostêpne oraz pojawi siê fajny napis na OSD przy zmianie kana³u, wy¶wietlaj±cy jego nazwê. Odstêpy w nazwie kana³u musz± zostaæ zast±pione znakiem "_".

•

U¿ywaj rozs±dnych rozmiarów obrazu. Rozmiary obrazu wynikowego powinny byæ podzielne przez 16. • Je¶li nagrywasz obraz video o pionowej rozdzielczo¶ci wiêkszej ni¿ po³owa rozdzielczo¶ci pe³nej (np. 288 dla PAL lub 240 dla NTSC), upewnij siê, ¿e w³±czy³e¶ usuwanie przeplotu (deinterlacing). W przeciwnym wypadku dostaniesz film, który jest zniekszta³cony w trakcie scen o du¿ej dynamice, a wskazana szybko¶æ prawdopodobnie nie bêdzie nawet mog³a byæ utrzymana przez kontroler szybko¶ci (bitrate controller), gdy¿ artefakty przeplotu tworz± du¿e ilo¶ci szczegó³ów, a co za tym idzie, potrzebuj± du¿ej przepustowo¶ci. Mo¿esz w³±czyæ usuwanie przeplotu za pomoc± opcji -vf

pp=TYP_DEINT. Zwykle pp=lb spisuje siê dobrze, ale to kwestia gustu. Poczytaj o innych

algorytmach usuwania przeplotu na stronie man i zacznij eksperymentowaæ.

•

Usuwaj "martwe miejsca". Kiedy nagrywasz video, s± pewnie miejsca przy brzegach, które s± zazwyczaj czarne lub zawieraj± szum. Jak siê ³atwo domy¶liæ, niepotrzebnie wymagaj± wiêkszej przepustowo¶ci (dok³adniej, to nie same czarne miejsca, lecz ostre przej¶cia pomiêdzy czarnym kolorem i ja¶niejszym obrazem video, ale nie jest to akurat takie wa¿ne). Zanim zaczniesz nagrywaæ, ustaw argumenty opcji crop by wszystkie "¶mieci" na brzegach zosta³y wyciête. Oczywi¶cie nie zapomnij o utrzymaniu prawid³owych wymiarów obrazu.

•

Uwa¿aj na obci±¿enie CPU. Nie powinno ono przekroczyæ granicy 90% przez wiêkszo¶æ czasu. Je¶li masz du¿y bufor nagrywania, MEncoder mo¿e przetrwaæ przeci±¿enie przez najwy¿ej kilka sekund i nic wiêcej. Lepiej wiêc wy³±czyæ wszystkie trójwymiarowe wygaszacze OpenGL i inne tego typu bajery.

•

Nie mieszaj z zegarem systemowym. MEncoder korzysta z niego do synchronizacji A/V. Je¶li zmodyfikujesz zegar systemowy (zw³aszcza wstecz), MEncoder siê pogubi i utraci klatki. Jest to bardzo wa¿na sprawa je¶li jeste¶ podpiêty do sieci i u¿ywasz do synchronizacji czasu ró¿nych programów typu NTP. Musisz wy³±czyæ NTP w trakcie nagrywania, je¶li chcesz, by by³o ono przeprowadzone niezawodnie.

•

Nie zmieniaj opcji outfmt, chyba, ¿e wiesz co robisz lub Twoja karta/sterownik naprawdê nie obs³uguje ustawienia domy¶lnego (przestrzeñ kolorów YV12). W poprzednich wersjach MPlayera/MEncodera konieczne by³o podanie formatu wyj¶cia. Ten problem powinien byæ rozwi±zany w aktualnych wydaniach i opcja outfmt nie jest ju¿ wymagana, a ustawienie domy¶lne powinno pasowaæ ka¿demu. Na przyk³ad, je¶li nagrywasz do formatu DivX u¿ywaj±c libavcodec i podasz opcjê outfmt=RGB24 aby zwiêkszyæ jako¶æ nagrywanego obrazu, zostanie on i tak

•

MPlayer - Odtwarzacz filmów dla LINUKSA

2.4.1. Kompilacja 69 pó¼niej z powrotem przekonwertowany do YV12, wiêc jedyne, co osi±gniesz, to ogromna strata mocy obliczeniowej. By u¿yæ przestrzeni kolorów I420 (outfmt=i420), musisz dodaæ opcjê -vc rawi420 z powodu konfliktu fourcc z kodekiem Intel Indeo. • Jest kilka sposobów na nagrywanie audio. Mo¿esz nagrywaæ d¼wiêk za pomoc± Twojej karty d¼wiêkowej korzystaj±c z zewnêtrznego kabla pomiêdzy kart± video i wej¶ciem liniowym lub korzystaj±c z wbudowanego w uk³ad bt878 przetwornika ADC. W tym drugim przypadku musisz za³adowaæ sterownik btaudio. Przeczytaj plik linux/Documentation/sound/btaudio (w drzewie j±dra, a nie MPlayera) by dowiedzieæ siê jak korzystaæ z tego sterownika.

•

Je¶li MEncoder nie mo¿e otworzyæ urz±dzenia d¼wiêkowego, upewnij siê, ¿e jest ono rzeczywi¶cie dostêpne. Zdarzaj± siê problemy z serwerami d¼wiêku typu aRts (KDE) lub esd (GNOME). Je¶li masz kartê full-duplex (prawie wszystkie przyzwoite karty dostêpne obecnie obs³uguj± tê funkcjê) i korzystasz z KDE, spróbuj zaznaczyæ opcjê "Dzia³anie w pe³ni dupleksowe" ("full duplex") w konfiguracji serwera d¼wiêku.

•

2.4.3. Przyk³ady

Puste wyj¶cie, do AAlib :)

mplayer -tv driver=dummy:width=640:height=480 -vo aa tv://

Wej¶cie ze standardowego V4L:

mplayer -tv driver=v4l:width=640:height=480:outfmt=i420 -vc rawi420 -vo xv tv://

Bardziej skomplikowany przyk³ad. Ka¿e on MEncoderowi nagraæ pe³en obraz PAL, wykadrowaæ go i usun±æ przeplot korzystaj±c z algorytmu liniowego zlewania (linear blend). Audio jest kompresowane ze sta³± szybko¶ci± równ± 64kbps, korzystaj±c z kodeka LAME. To ustawienie jest dobre do nagrywania filmów.

     mencoder -tv driver=v4l:width=768:height=576 \
     -ovc lavc -lavcopts vcodec=mpeg4:vbitrate=900 \
     -oac mp3lame -lameopts cbr:br=64 \
     -vf crop=720:544:24:16,pp=lb -o output.avi tv://

Ten przyk³ad dodatkowo przeskaluje obraz do 384x288 i skompresuje video z szybko¶ci± 350kbps w trybie wysokiej jako¶ci. Opcja vqmax uwalnia kwantyzator i pozwala kompresorowi video na osi±gniêcie tak niskiej szybko¶ci nawet kosztem jako¶ci obrazu. Mo¿e byæ to u¿ywane do nagrywania d³ugich seriali TV, kiedy jako¶æ obrazu nie jest tak wa¿na.

     mencoder -tv driver=v4l:width=768:height=576 \
     -ovc lavc -lavcopts vcodec=mpeg4:vbitrate=350:vhq:vqmax=31:keyint=300 \
     -oac mp3lame -lameopts cbr:br=48 \
     -vf crop=720:540:24:18,pp=tn/lb,scale=384:288 -sws 1 -o output.avi tv://

Jest równie¿ mo¿liwe podanie mniejszych wymiarów obrazu w opcji -tv i pominiêcie programowego skalowania, ale to podej¶cie wykorzystuje maksymaln± ilo¶æ dostêpnych informacji i jest trochê bardziej odporne na szum. Z powodu ograniczeñ sprzêtowych Uk³ady bt878 mog± stosowaæ u¶rednianie pikseli jedynie w kierunku poziomym.

MPlayer - Odtwarzacz filmów dla LINUKSA

2.4.3. Przyk³ady 70

2.5. Edit Decision Lists (EDL)

The edit decision list (EDL) system allows you to automatically skip or mute sections of videos during playback, based on a movie specific EDL configuration file.

This is useful for those who may want to watch a film in "family-friendly" mode. You can cut out any violence, profanity, Jar-Jar Binks .. from a movie according to your own personal preferences. Aside from this, there are other uses, like automatically skipping over commercials in video files you watch.

The EDL file format is pretty bare-bones. Once the EDL system has reached a certain level of maturity, an XML-based file format will probably be implemented (keeping backwards compatibility with previous EDL formats).

The maximum number of EDL entries for the current incarnation of EDL is 1000. If you happen to need more, change the #define MAX_EDL_ENTRIES in the edl.h file.

2.5.1. Using an EDL file

Include the -edl <filename> flag when you run MPlayer, with the name of the EDL file you want applied to the video.

2.5.2. Making an EDL file

The current EDL file format is:

[begin second] [end second] [action]

Where the seconds are floating-point numbers and the action is either 0 for skip or 1 for mute. Example:

5.3   7.1    0
15    16.7   1
420   422    0

This will skip from second 5.3 to second 7.1 of the video, then mute at 15 seconds, unmute at 16.7 seconds and skip from second 420 to second 422 of the video. These actions will be performed when the playback timer reaches the times given in the file.

To create an EDL file to work from, use the -edlout <filename> flag. During playback, when you want to mark the previous two seconds to skip over, hit i. A corresponding entry will be written to the file for that time. You can then go back and fine-tune the generated EDL file.

Rozdzia³ 3. Sposób u¿ycia

Spis tre¶ci

3.1. Linia poleceñ 3.2. Sterowanie

3.2.1. Konfiguracja sterowania 3.2.1.1. Nazwy klawiszy 3.2.1.2. Komendy

MPlayer - Odtwarzacz filmów dla LINUKSA

2.5. Edit Decision Lists (EDL) 71

3.2.2. Sterowanie poprzez LIRC 3.2.3. Tryb s³ugi 3.3. Strumieniowanie z sieci i potoków 3.4. Strumienie zdalne

3.4.1. Kompilacja serwera 3.4.2. U¿ywanie strumieni zdalnych

3.1. Linia poleceñ

MPlayer u¿ywa skomplikowanego drzewa odtwarzania. Sk³ada siê on z opcji globalnych podanych na pocz±tku, na przyk³ad:

mplayer -vfm 5

i opcji podanych po nazwach plików, które stosuj± siê jedynie do podanego pliku/URLa/czegokolwiek, na przyk³ad:

mplayer -vfm 5 film1.avi film2.avi -vfm 4

Mo¿esz pogrupowaæ nazwy plików/URLe za pomoc± { oraz }. Przydaje siê to przy opcji -loop:

mplayer { 1.avi -loop 2 2.avi } -loop 3

Powy¿sze polecenie odtworzy pliki w kolejno¶ci: 1, 1, 2, 1, 1, 2, 1, 1, 2.

Odtwarzanie pliku:

mplayer [opcje] [¶cie¿ka/]nazwa_pliku

Odtwarzanie wiêkszej ilo¶ci plików:

mplayer [opcje domy¶lne] [¶cie¿ka/]nazwa_pliku1 [opcje dla nazwa_pliku1] nazwa_pliku2 [opcje dla nazwa_pliku2] ...

Odtwarzanie VCD:

mplayer [opcje] vcd://numer_¶cie¿ki [-cdrom-device /dev/cdrom]

Odtwarzanie DVD:

mplayer [opcja] dvd://numer_tytu³u [-dvd-device /dev/dvd]

Odtwarzanie z WWW:

mplayer [opcje] http://strona.com/plik.asf

(mo¿na u¿yæ równie¿ playlist)

Odtwarzanie z RTSP:

mplayer [opcje] rtsp://serwer.przyklad.com/nazwa_strumienia

Przyk³ady:

MPlayer - Odtwarzacz filmów dla LINUKSA

3.1. Linia poleceñ 72

mplayer -vo x11 /mnt/Films/Contact/contact2.mpg
mplayer vcd://2 -cd-rom-device /dev/hdc
mplayer -afm 3 /mnt/DVDtrailers/alien4.vob
mplayer dvd://1 -dvd-device /dev/hdc
mplayer -abs 65536 -delay -0.4 -nobps ~/movies/test.avi

3.2. Sterowanie

MPlayer posiada w pe³ni konfigurowaln±, opart± na komendach warstwê sterowania, która pozwala na sterowanie MPlayera za pomoc± klawiatury, myszki, joysticka lub zdalnego sterowania (za pomoc± LIRC). Zajrzyj do strony man w celu przejrzenia pe³nej listy skrótów klawiszowych.

3.2.1. Konfiguracja sterowania

MPlayer pozwala Ci przypisaæ dowolny klawisz/przycisk do ka¿dej komendy za pomoc± prostego pliku konfiguracyjnego. Sk³adnia tego pliku to nazwa klawisza, po której znajduje siê komenda. Domy¶lny plik konfiguracyjny znajduje siê w $HOME/.mplayer/input.conf, ale mo¿na podaæ tak¿e inny za pomoc± opcji -input plik (¶cie¿ki wzglêdne s± wzglêdem $HOME/.mplayer).

Przyk³ad 3.1. Przyk³adowy plik konfiguracji sterowania

##
## Plik konfiguracji sterowania MPlayera
##

RIGHT seek +10
LEFT seek -10
- audio_delay 0.100
+ audio_delay -0.100
q quit
> pt_step 1
< pt_step -1
ENTER pt_step 1 1

3.2.1.1. Nazwy klawiszy

Mo¿esz uzyskaæ pe³n± listê uruchamiaj±c mplayer -input keylist.

Klawiatura

Dowolny znak drukowalny •

SPACE

•

ENTER

•

TAB

•

CTRL

•

BS

•

DEL

•

INS

•

HOME

•

END

•

PGUP

•

PGDWN

•

ESC

•

MPlayer - Odtwarzacz filmów dla LINUKSA

3.2. Sterowanie 73

RIGHT

•

LEFT

•

UP

•

DOWN

• Myszka (obs³ugiwana tylko w Xach)

MOUSE_BTN0 (Lewy przycisk)

•

MOUSE_BTN1 (Prawy przycisk)

•

MOUSE_BTN2 (¦rodkowy przycisk)

•

MOUSE_BTN3 (Rolka)

•

MOUSE_BTN4 (Rolka)

• ...•

MOUSE_BTN9

• Joystick (obs³uga musi byæ w³±czona podczas kompilacji)

JOY_RIGHT or JOY_AXIS0_PLUS

•

JOY_LEFT or JOY_AXIS0_MINUS

•

JOY_UP or JOY_AXIS1_MINUS

•

JOY_DOWN or JOY_AXIS1_PLUS

•

JOY_AXIS2_PLUS

•

JOY_AXIS2_MINUS

• ...•

JOY_AXIS9_PLUS

•

JOY_AXIS9_MINUS

• 3.2.1.2. Komendy

Mo¿esz uzyskaæ pe³n± listê komend uruchamiaj±c mplayer -input cmdlist.

seek (int) warto¶æ [(int) type=0]

Przeskok do pewnego miejsca w pliku. Type=0 to skok wzglêdny o +/- warto¶æ sekund. Type=1 to skok do warto¶æ% w filmie.

•

audio_delay (float) warto¶æ

Zmienia opó¼nienie o warto¶æ sekund. •

quit

Wychodzi z MPlayera •

pause

Wstrzymuje/przywraca odtwarzanie •

grap_frames

Nie mam pojêcia ;) •

pt_step (int) warto¶æ [(int) force=0]

Przejd¼ do nastêpnego/poprzedniego wpisu w drzewie odtwarzania. Znak warto¶ci wskazuje kierunek. Je¶li nie ma ju¿ ¿adnych innych wpisów w danym kierunku, komenda ta nie zrobi nic,

•

MPlayer - Odtwarzacz filmów dla LINUKSA chyba, ¿e argument force nie jest zerem.

pt_up_step (int) warto¶æ [(int) force=0]

Podobnie, jak pt_step, ale skacze do nastêpnego/poprzedniego wpisu w li¶cie elementów nadrzêdnych (parent list). Jest u¿yteczne do przerywania wewnêtrznych pêtli w drzewie odtwarzania.

•

alt_src_step (int) warto¶æ

Gdy dostêpnych jest wiêcej ni¿ jedno ¼ród³o, komenda ta wybiera nastêpne/poprzednie (obs³ugiwane tylko przez playlistê asx).

•

sub_delay (float) warto¶æ [(int) abs=0]

Przesuwa opó¼nienie napisów o +/- warto¶æ sekund lub ustawia je na warto¶æ sekund gdy abs nie jest równe 0.

•

osd [(int) level=-1]

Prze³±cza tryb osd lub ostawia go na poziom level gdy level > 0. •

volume (int) kierunek

Zwiêksza/zmniejsza poziom g³o¶no¶ci •

contrast (int) warto¶æ [(int) abs=0]

•

brightness (int) warto¶æ [(int) abs=0]

•

hue (int) warto¶æ [(int) abs=0]

•

saturation (int) warto¶æ [(int) abs=0]

Ustawia/przestawia parametry video. Zasiêg warto¶ci: od -100 do 100. •

frame_drop [(int) type=-1]

Prze³±cza/ustawia tryb opuszczania klatek. •

sub_visibility

Zmienia widoczno¶æ napisów. •

sub_pos (int) val

Zmienia po³o¿enie napisów. •

vobsub_lang

Zmienia jêzyk napisów VobSub. •

vo_fullscreen

Prze³±cza tryb pe³noekranowy. •

tv_step_channel (int) kierunek

Wybiera nastêpny/poprzedni kana³ TV. •

tv_step_norm

Zmienia normê TV. •

tv_step_chanlist

Zmienia listê kana³ów. •

gui_loadfile

•

gui_loadsubtitle

•

MPlayer - Odtwarzacz filmów dla LINUKSA gui_about

•

gui_play

•

gui_stop

•

gui_playlist

•

gui_preferences

•

gui_skinbrowser

Akcje GUI •

3.2.2. Sterowanie poprzez LIRC

Linux Infrared Remote Control - u¿yj ³atwego do w³asnorêcznego zbudowania odbiornika podczerwieni i (prawie) dowolnego pilota zdalnego sterowania i steruj nim swoim Linuksem! Wiêcej o LIRC: www.lirc.org.

Je¶li zainstalowa³e¶ LIRC, configure automatycznie go wykryje. Je¶li wszystko pójdzie dobrze, MPlayer wypisze komunikat typu "Setting up lirc support..." przy starcie. Je¶li wyst±pi b³±d, powiadomi Ciê o tym. Je¶li nic nie powie Ci na temat LIRC, to znaczy, ¿e jego obs³uga nie zosta³a wkompilowana. To tyle ;)

Nazwa aplikacji dla MPlayer to - hmm... zgadnij ;) - mplayer. Mo¿esz u¿ywaæ dowolnych komend, a nawet podaæ wiêcej ni¿ jedn± komendê na raz oddzielaj±c je za pomoc± \n. Nie zapomnij o w³±czeniu flagi repeat w .lircrc je¶li ma to sens (skoki, g³o¶no¶æ itp). To jest fragment mojego .lircrc:

begin
     button = VOLUME_PLUS
     prog = mplayer
     config = volume 1
     repeat = 1
end

begin
    button = VOLUME_MINUS
    prog = mplayer
    config = volume -1
    repeat = 1
end

begin
    button = CD_PLAY
    prog = mplayer
    config = pause
end

begin
    button = CD_STOP
    prog = mplayer
    config = seek 0 1\npause
end

Je¶li nie lubisz standardowej lokalizacji pliku lirc-config (~/.lircrc), u¿yj opcji -lircconf

nazwa_pliku by podaæ inny plik.

MPlayer - Odtwarzacz filmów dla LINUKSA

3.2.2. Sterowanie poprzez LIRC 76

3.2.3. Tryb s³ugi

Tryb s³ugi pozwala Ci na utworzenie prostej nak³adki na MPlayera. Po jego w³±czeniu (opcja -slave) MPlayer bêdzie czyta³ komendy oddzielone znakami nowej linii (\n) ze standardowego wej¶cia.

3.3. Strumieniowanie z sieci i potoków

MPlayer potrafi odtwarzaæ pliki z sieci, u¿ywaj±c protoko³ów HTTP, FTP, MMS lub RTSP/RTP.

Odtwarzanie nastêpuje po prostu przy podaniu URLa w linii poleceñ. MPlayer równie¿ zwraca uwagê na zmienn± ¶rodowiskow± http_proxy i u¿ywa proxy je¶li jest to mo¿liwe. Korzystanie z proxy mo¿e byæ równie¿ wymuszone za pomoc±:

mplayer http_proxy://proxy.micorsops.com:3128/http://micorsops.com:80/strumien.asf

MPlayer potrafi równie¿ czytaæ ze standardowego wej¶cia (nie z nazwanych potoków). Mo¿e to byæ wykorzystane np. do odtwarzania poprzez FTP:

wget ftp://micorsops.com/cokolwiek.avi -O - | mplayer -

Notatka

Uwaga: zalecane jest równie¿ w³±czenie -cache przy odtwarzaniu z sieci:

wget ftp://micorsops.com/cokolwiek.avi -O - | mplayer -cache 8192 -

3.4. Strumienie zdalne

Strumienie zdalne pozwalaj± na dostêp do wiêkszo¶ci strumieni obs³ugiwanych przez MPlayera ze zdalnego hosta. G³ównym celem tej funkcji jest umo¿liwienie bezpo¶redniego korzystania z napêdu CD lub DVD innego komputera w sieci (pod warunkiem posiadania odpowiedniej przepustowo¶ci). Niestety niektóre typy strumieni (aktualnie TV oraz MF) nie s± dostêpne zdalnie, gdy¿ s± zaimplementowane na poziomie demultipleksera. Jest to przykre w przypadku MF, gdy¿ TV i tak by wymaga³o szalonej przepustowo¶ci.

3.4.1. Kompilacja serwera

Po kompilacji MPlayera wejd¼ do katalogu TOOLS/netstream i wpisz make by zbudowaæ program serwera. Mo¿esz wtedy skopiowaæ program nestream do odpowiedniego miejsca w Twoim systemie (przewa¿nie /usr/local/bin pod Linuksem).

3.4.2. U¿ywanie strumieni zdalnych

Najpierw musisz uruchomiæ serwer na komputerze, do którego masz zamiar mieæ dostêp zdalny. Aktualnie serwer jest bardzo podstawowy i nie posiada ¿adnych argumentów w linii poleceñ, wiêc po prostu wpisz

netstream. Teraz mo¿esz np. odtworzyæ drug± ¶cie¿kê VCD na serwerze za pomoc±:

mplayer -cache 5000 mpst://nazwa_serwera/vcd://2

Masz równie¿ dostêp do plików na tym serwerze:

MPlayer - Odtwarzacz filmów dla LINUKSA

3.2.3. Tryb s³ugi 77

mplayer -cache 5000 mpst://nazwa_serwera//usr/local/movies/lol.avi

Zauwa¿, ¿e ¶cie¿ki, które nie zaczynaj± siê na "/" bêd± wzglêdne do katalogu, w którym uruchomiono serwer. Opcja -cache nie jest wymagana, lecz bardzo zalecana.

Miej na uwadze to, ¿e serwer nie jest aktualnie w ogóle bezpieczny. Nie narzekaj wiêc na liczne nadu¿ycia, które s± przez to mo¿liwe. Zamias tego wy¶lij jak±¶ (dobr±) ³atkê, by sta³ siê lepszy lub napisz swój w³asny serwer.

Rozdzia³ 4. Frequently Asked Questions

4.1. Development

Pyt: How do I create a proper patch for MPlayer? Pyt: How can I support MPlayer development? Pyt: How can I become an MPlayer developer? Pyt: Why don't you use autoconf/automake?

4.2. Compilation

Pyt: Are there binary (RPM/deb) packages of MPlayer? Pyt: Compilation stops with an error message similar to this one: cfft.c: In function`passf2': cfft.c:556: unable to find a register to spill in class `FLOAT_REGS' cfft.c:556: this is the insn: (insn 235 233 246 (set (subreg:SF (reg/v:DI 29 rmm0 [110]) 0) (minus:SF (mem:SF (plus:SI (mult:SI (reg:SI 1 edx [112]) (const_int 8 [0x8])) (reg/v/f:SI 3 ebx [62])) [4 S4 A32]) (reg:SF 8 st(0) [132]))) 533 {*fop_sf_1_nosse} (insn_list 232 (nil)) (expr_list:REG_DEAD (reg:SF 8 st(0) [132]) (nil))) cfft.c:556: confused by earlier errors, bailing out Pyt: Compilation stops with an error message similar to this one: In file included from mplayer.c:34: mw.h: In function `mplMainDraw': mw.h:209: Internal compiler error in print_rtl_and_abort, at flow.c:6458 Please submit a full bug report, with preprocessed source if appropriate. Pyt: Configure ends with this text, and MPlayer won't compile! Your gcc does not support even i386 for '-march' and '-mcpu' Pyt: What's the problem with gcc 2.96? Pyt: Great, I have gcc 3.0.1 from Red Hat/Mandrake, then I'm fine! Pyt: I tried to compile MPlayer, but I got this output: In file included from /usr/include/g++-v3/bits/std_cwchar.h:42, from /usr/include/g++-v3/bits/fpos.h:40, from /usr/include/g++-v3/bits/char_traits.h:40, from /usr/include/g++-v3/bits/std_string.h:41, from /usr/include/g++-v3/string:31, from libwin32.h:36, from DS_AudioDecoder.h:4, from DS_AudioDec.cpp:5: /usr/include/wchar.h: In function Long long int wcstoq(const wchar_t*, wchar_t**, int)': /usr/include/wchar.h:514: cannot convert `const wchar_t* __restrict' to `const Pyt: .. gcc 2.96 ... (Yes, some people are STILL flaming about gcc 2.96!) Pyt: SDL output doesn't work or compile. The problem is ... Pyt: I am still having trouble compiling with SDL support. gcc says something about undefined reference to SDL_EnableKeyRepeat. What now? Pyt: It doesn't compile, and it misses uint64_t, inttypes.h and similar things ... Pyt: I have Linux running on a Pentium III but ./configure doesn't detect SSE ... Pyt: I have a Matrox G200/G400/G450/G550, how do I compile/use the mga_vid driver? Pyt: Hmm, strange. When loading the mga_vid.o kernel module, I found this in the logs: Warning: loading mga_vid.o will taint the kernel: no license Pyt: During 'make', MPlayer complains about X11 libraries. I don't understand, I DO have X installed!? Pyt: I can't compile SVGAlib. I'm using kernel 2.3/2.4 ... Pyt: I compiled MPlayer with libdvdcss/libdivxdecore support, but when I try to start it, it says: error

MPlayer - Odtwarzacz filmów dla LINUKSA while loading shared libraries: lib*.so.0: cannot load shared object file: No such file or directory I checked up on the file and it IS there in /usr/local/lib ... Pyt: When compiling MEncoder, it segfaults at linking! Pyt: MPlayer dies with segmentation fault upon pthread check! Pyt: I'd like to compile MPlayer on Minix!

4.3. General questions Pyt: Are there any mailing lists on MPlayer? Pyt: I've found a nasty bug when I tried to play my favorite video! Who should I inform? Pyt: I have problems playing files with the ... codec. Can I use them? Pyt: When I start playing, I get this message but everything seems fine: Linux RTC init: ioctl (rtc_pie_on): Permission denied Pyt: There is a timer in the upper left corner. How can I get rid of it? Pyt: The -xy or -fs option doesn't work with the x11 driver (-vo x11) ... Pyt: What is the meaning of the numbers on the status line? Pyt: What if I don't want them to appear? Pyt: Why is video_out cpu usage zero (0%) for some files? Pyt: There are error messages about file not found /usr/local/lib/codecs/ ... Pyt: Umm, what is "IdegCounter"? Pyt: And what is "Faszom(C)ounter"? Pyt: LIRC doesn't work, because ... Pyt: Subtitles are very nice, the most beautiful I've ever seen, but they slow down playing! I know it's unlikely ... Pyt: The onscreen display (OSD) is flickering! Pyt: What exactly is this libavcodec thing? Pyt: But configure tells me Checking for libavcodec ... no Pyt: Icewm's taskbar keeps covering the movie in fullscreen mode! Pyt: I can't access the GUI menu. I press right click, but I can't access any menu items! Pyt: How can I run MPlayer in the background?

4.4. Playback problems Pyt: I cannot pinpoint the cause of some strange playback problem. Pyt: ... works with xine/avifile/... but doesn't with MPlayer. Pyt: Audio goes out of sync playing an AVI file. Pyt: MPlayer exits with some error when using l3codeca.acm. Pyt: My computer plays MS DivX AVIs with resolutions ~ 640x300 and stereo mp3 sound too slow. When I use -nosound option, everything is OK (but quiet). Pyt: MPlayer dies with MPlayer interrupted by signal 4 in module: decode_video Pyt: I have problems with [your window manager] and fullscreen xv/xmga/sdl/x11 modes ... Pyt: I got this playing MPEG files: Can't find codec for video format 0x10000001! Pyt: When starting MPlayer under KDE I just get a black screen and nothing happens. After about one minute the video starts playing. Pyt: I have an AVI that produces a gray screen when played with -vc odivx and a green one with -vc divx4. Pyt: When I play this movie I get video-audio desync and/or MPlayer crashes with the following message: DEMUXER: Too many (945 in 8390980 bytes) video packets in the buffer! Pyt: I have an MJPEG file which works with other players but displays only a black image in MPlayer Pyt: When I try to grab from my tuner, it works, but colors are strange. It's OK with other applications. Pyt: I have A/V sync problems. Some of my AVIs play fine, but some play with double speed! Pyt: All the WMV (or other..) files I play create a green/gray window and there is only sound! MPlayer prints: Detected video codec: [null] drv:0 (NULL codec (no decoding))

MPlayer - Odtwarzacz filmów dla LINUKSA

Pyt: I get very strange percentage values (way too big) while playing files on my notebook. Pyt: The audio/video gets totally out of sync when I run MPlayer as root on my notebook. It works normal when i run it as a user. Pyt: While playing a movie it suddenly gets jerky and I get the following message: Badly interleaved AVI file detected - switching to -ni mode... Pyt: How can I play MPEG Layer 2 (mp2) audio files?

4.5. Video/audio driver problems (vo/ao) Pyt: I have no sound when playing a video and get error messages similar to this one: AO: [oss] 44100Hz 2ch Signed 16-bit (Little-Endian) audio_setup: Can't open audio device /dev/dsp: Device or resource busy couldn't open/init audio device -> NOSOUND Audio: no sound!!! Start playing... Pyt: What about the DGA driver? I can't find it! Pyt: OK, -vo help shows DGA driver, but it complains about permissions. Help me! Pyt: When using Xvideo, my Voodoo 3/Banshee says: X Error of failed request: BadAccess (attempt to access private resource denied) Major opcode of failed request: 147 (MIT-SHM) Minor opcode of failed request: 1 (X_ShmAttach) Serial number of failed request: 26 Current serial number in output stream:27 Pyt: OpenGL (-vo gl) output doesn't work (hang/black window/X11 errors/...). Pyt: I have an nVidia TNT/TNT2 card, and I have a band with strange colors, right under the movie! Whose fault is this? Pyt: I have an nVidia XYZ card, and when I click on the GUI's display window to toggle displaying the GUI panel, a black square appears where I clicked. I have the newest driver. Pyt: Oh the world is cruel ...! SDL has only x11 target, but not xv!

4.6. DVD playback

Pyt: What about DVD navigation? Pyt: While playing a DVD, I encountered this error: mplayer: ifo_read.c:1143: ifoRead_C_ADT_internal: Assertion nfo_length / sizeof(cell_adr_t) >= c_adt->nr_of_vobs' failed. Pyt: Can I compile libdvdread and libdvdcss on my sweet SPARC under Solaris? Pyt: What about subtitles? Can MPlayer display them? Pyt: How can I set the region code of my DVD-drive? I don't have Windows! Pyt: Do I need to be (setuid) root/setuid fibmap_mplayer to be able to play a DVD? Pyt: Where can I get libdvdread and libdvdcss packages? Pyt: Is it possible to play/encode only selected chapters? Pyt: My DVD playback is sluggish!

4.7. Feature requests

Pyt: If MPlayer is paused and I try to seek or press any key at all, MPlayer ceases to be paused. I would like to be able to seek in the paused movie. Pyt: I'd like to seek +/- 1 frames instead of 10 seconds. Pyt: How can I make MPlayer remember the options I use for this particular file?

4.8. Encoding

Pyt: How can I encode? Pyt: How can I create VCDs? Pyt: How can I join two video files? Pyt: My tuner works, I can hear the sound and watch the video with MPlayer, but MEncoder doesn't encode audio! Pyt: I can't encode DVD subtitles into the AVI! Pyt: MEncoder segfaults on startup! Pyt: How can I encode only selected chapters from a DVD? Pyt: I'm trying to work with 2GB+ files on a VFAT file system. Does it work? Pyt: Why is the recommended bitrate printed by MEncoder negative? Pyt: I can't encode ASF files to AVI/DivX because it uses 1000 fps? Pyt: How can I put subtitles in the output file?

MPlayer - Odtwarzacz filmów dla LINUKSA

4.1. Development

Pyt: How do I create a proper patch for MPlayer? Odp: We made a short document describing all the necessary details. Please follow the instructions. Pyt: How can I support MPlayer development? Odp: We are more than happy to accept your hardware and software donations. They help us in continuously improving MPlayer. Pyt: How can I become an MPlayer developer? Odp: We always welcome coders and documenters. Read the technical documentation to get a first grasp. Then you should subscribe to the mplayer-dev-eng mailing list and start coding.

Pyt: Why don't you use autoconf/automake? Odp: We have a modular, handwritten build system. It does a reasonably good job, so why change? Besides, we dislike the auto* tools, just like other people.

4.2. Compilation

Pyt: Are there binary (RPM/deb) packages of MPlayer? Odp: See the Debian and RPM section for details. Pyt: Compilation stops with an error message similar to this one:

    cfft.c: In function`passf2':
    cfft.c:556: unable to find a register to spill in class `FLOAT_REGS'
    cfft.c:556: this is the insn:
    (insn 235 233 246 (set (subreg:SF (reg/v:DI 29 rmm0 [110]) 0)
            (minus:SF (mem:SF (plus:SI (mult:SI (reg:SI 1 edx [112])
                            (const_int 8 [0x8]))
                        (reg/v/f:SI 3 ebx [62])) [4 S4 A32])
                (reg:SF 8 st(0) [132]))) 533 {*fop_sf_1_nosse} (insn_list
    232 (nil))    (expr_list:REG_DEAD (reg:SF 8 st(0) [132])
            (nil)))
    cfft.c:556: confused by earlier errors, bailing out

Odp: This is a known problem of gcc 3.2, upgrade to 3.3 to solve the problem. How to install gcc is described in the gcc 2.96 section. Alternatively you can use an external FAAD library as described in the AAC section.

Pyt: Compilation stops with an error message similar to this one:

    In file included from mplayer.c:34:
    mw.h: In function `mplMainDraw':
    mw.h:209: Internal compiler error in print_rtl_and_abort, at flow.c:6458
    Please submit a full bug report,
    with preprocessed source if appropriate.

Odp: This is a known problem of gcc 3.0.4, upgrade to 3.1 to solve the problem. How to install gcc is described in the gcc 2.96 section. Pyt: Configure ends with this text, and MPlayer won't compile!

Your gcc does not support even i386 for '-march' and '-mcpu'

Odp: Your gcc isn't installed correctly, check the config.log file for details. Pyt: What's the problem with gcc 2.96? Odp: We strongly discourage the use of gcc 2.96! Read this document for details about why Red Hat released gcc 2.96 and what the problems are all about. If you still really really want to use it, be sure to get the latest release and give the --disable-gcc-checking option to configure. Remember that you are on your own from this point. Do not report bugs, do not ask for help on the mailing lists. We will not provide any support in case you run into problems.

Pyt: Great, I have gcc 3.0.1 from Red Hat/Mandrake, then I'm fine!

MPlayer - Odtwarzacz filmów dla LINUKSA

Odp: No, since there have been/are issues with these compilers as well. To check the status of current compilers' MPlayer support, see the Installation section.

Pyt: I tried to compile MPlayer, but I got this output:

    In file included from /usr/include/g++-v3/bits/std_cwchar.h:42,
                     from /usr/include/g++-v3/bits/fpos.h:40,
                     from /usr/include/g++-v3/bits/char_traits.h:40,
                     from /usr/include/g++-v3/bits/std_string.h:41,
                     from /usr/include/g++-v3/string:31,
                     from libwin32.h:36,
                     from DS_AudioDecoder.h:4,
                     from DS_AudioDec.cpp:5:
    /usr/include/wchar.h: In function Long long int wcstoq(const wchar_t*,
       wchar_t**, int)':
    /usr/include/wchar.h:514: cannot convert `const wchar_t* __restrict' to
    `const

Odp: Upgrade your glibc to the latest release. On Mandrake, use 2.2.4-8mdk. Pyt: .. gcc 2.96 ... (Yes, some people are STILL flaming about gcc 2.96!) Odp: Quoted from a mail A'rpi sent to the mplayer-users list (the word 'ideg' is described below):

And we have idegs. And our idegcounter overflowed again and again.

Unfortunately MPlayer is out of our control. It's used by lamers, Linux users who can't even use Windows, and never tried to compile a kernel. They installed (with default options) Mandrake or Red Hat or SuSE, and without RTFM'ing they send messages saying 'it doesn't work! help me! please! i'm new to Linux! help! oh! help me!'. We can't stop them, but at least we try to force them to RTFM and to read the messages of ./configure and MPlayer.

And you clever guys come and flame us with gcc 2.96 and binary packages. Instead of helping users or making patches to help solve problems.

Half of our spare/free time is spent by answering silly mails here and making newer tricks and checks to configure to avoid such mails.

And there is a balance. On the one side are you, clever guys, saying we are very bad because we don't like buggy gcc 2.96, and on the other side there are the 'new to Linux' guys who are showing us gcc 2.96 is buggy.

Conclusion: We can't be good. Half the people will always say we are bad.

Maybe we should close the project, make it closed source, commercial, and provide install support for it. then we could leave current work, so development could go faster, and we could earn lots of money with it and buy a big house, etc etc. Do you really want it? It seems.

Pyt: SDL output doesn't work or compile. The problem is ... Odp: It was tested to work with SDL 1.2.x and may run on SDL 1.1.7+. It does not work with any previous version. So if you choose to use such a version, you are on your own.

Pyt: I am still having trouble compiling with SDL support. gcc says something about

undefined reference to SDL_EnableKeyRepeat

. What now? Odp: Where did you install the SDL library? If you installed in /usr/local (the default) then edit the top level config.mak and add

-L/usr/local/lib after X_LIBS=. Now type make. You're done!

MPlayer - Odtwarzacz filmów dla LINUKSA

Pyt: It doesn't compile, and it misses uint64_t, inttypes.h and similar things ... Odp: Copy this inttypes.h to /usr/local/include/ or an equivalent place and try again ... Pyt: I have Linux running on a Pentium III but ./configure doesn't detect SSE ... Odp: Only kernel versions 2.4.x support SSE (or try 2.2.19 or newer, but be prepared for problems). Pyt: I have a Matrox G200/G400/G450/G550, how do I compile/use the mga_vid driver? Odp: Read the mga_vid section. Pyt: Hmm, strange. When loading the mga_vid.o kernel module, I found this in the logs:

Warning: loading mga_vid.o will taint the kernel: no license

Odp: The latest kernel modutils require a flag indicating the license (mainly to avoid kernel hackers debugging closed source drivers). Upgrade your kernel, modutils and MPlayer.

Pyt: During 'make', MPlayer complains about X11 libraries. I don't understand, I DO have X installed!? Odp: ... but you don't have the X development package installed. Or not correctly. It's called XFree86-devel* under Red Hat, and xlibs-dev under Debian. Also check if the /usr/X11 and /usr/include/X11 symlinks exist (this can be a problem on Mandrake systems). They can be created with these commands:

     # ln -sf /usr/X11R6 /usr/X11
     # ln -sf /usr/X11R6/include/X11 /usr/include/X11

Your distribution may differ from the Filesystem Hierarchy Standard. Pyt: I can't compile SVGAlib. I'm using kernel 2.3/2.4 ... Odp: You have to edit SVGAlib's Makefile.cfg and comment BACKGROUND = y out. Pyt: I compiled MPlayer with libdvdcss/libdivxdecore support, but when I try to start it, it says:

error while loading shared libraries: lib*.so.0: cannot load shared object file: No such file or directory

I checked up on the file and it IS there in /usr/local/lib ... Odp: Add /usr/local/lib to /etc/ld.so.conf and run ldconfig. Pyt: When compiling MEncoder, it segfaults at linking! Odp: This is a linker problem. Upgrading binutils should help (2.11.92.* or newer should be good). Since it is not our fault, please do not report! Pyt: MPlayer dies with segmentation fault upon pthread check! Odp: chmod 644 /usr/lib/libc.so Pyt: I'd like to compile MPlayer on Minix! Odp: Me too. :)

4.3. General questions

Pyt: Are there any mailing lists on MPlayer? Odp: Yes. See the mailing lists section. Pyt: I've found a nasty bug when I tried to play my favorite video! Who should I inform? Odp: Please read the bug reporting guidelines and follow the instructions. Pyt: I have problems playing files with the ... codec. Can I use them? Odp: Check the codec status, if it doesn't contain your codec, read the codec documentation, especially the codec importing HOWTO and contact us. Pyt: When I start playing, I get this message but everything seems fine:

Linux RTC init: ioctl (rtc_pie_on): Permission denied

MPlayer - Odtwarzacz filmów dla LINUKSA

Odp: You need root privileges or a specially set up kernel to use the new timing code. For details see the RTC section of the documentation. Pyt: There is a timer in the upper left corner. How can I get rid of it? Odp: Press o and try the -osdlevel option. Pyt: The -xy or -fs option doesn't work with the x11 driver (-vo x11) ... Odp: It does, but you have to explicitly specify software scaling (very slow) with the -zoom option. You better use XF86VidMode support: You must specify the -vm and the -fs option, and you're done. Make sure you have the right modelines in your XF86Config file, and try to make the DGA driver and SDL's DGA driver work for you. It's much faster. If SDL's DGA works, use that, it'll be even faster.

Pyt: What is the meaning of the numbers on the status line? Odp: Example:

A: 2.1 V: 2.2 A-V: -0.167 ct: 0.042 57/57 41% 0% 2.6% 0 4 49%

A: audio position in seconds • V: video position in seconds • A-V: audio-video difference in seconds (delay) • ct: total A-V sync correction done • frames played (counting from last seek) • frames decoded (counting from last seek) • video codec cpu usage in percent (for slices and DR this includes video_out) • video_out cpu usage • audio codec cpu usage in percent • frames needed to drop to maintain A-V sync • current level of image postprocessing (when using -autoq) • current cache size used (around 50% is normal) • Most of them are for debug purposes and will be removed at some point.

Pyt: What if I don't want them to appear? Odp: Use the -quiet option and read the man page. Pyt: Why is video_out cpu usage zero (0%) for some files? Odp: It's not zero, but it's called from the codec and thus cannot be measured separately. You should try to play the file using -vo null and then -vo

... and check the difference to see the video_out speed.

Odp: You are using Direct Rendering, where the codec renders to the video memory itself. In this case, the decoding percentage contains the display percentage, too.

Pyt: There are error messages about file not found /usr/local/lib/codecs/ ... Odp: Download the Win32 codecs from our codecs page (avifile's codec package has a different DLL set) and install it. Pyt: Umm, what is "IdegCounter"? Odp: A combination of a Hungarian and an English word. "Ideg" in Hungarian means the same as "nerve" in English, and is pronounced as something like "ydaegh". It was first used to measure the nervousness of A'rpi, after some (umm) "mysterious" disappearance of CVS code ;)

Pyt: And what is "Faszom(C)ounter"? Odp: "Fasz" is a Hungarian word you don't want to know, the others are connected to the perverted minds of the MPlayer developers. Pyt: LIRC doesn't work, because ... Odp: Are you sure you are using mplayer instead of mplayer_lirc? Note that it was mplayer_lirc for a long time, including the 0.60 release, but it was recently changed back to mplayer.

Pyt: Subtitles are very nice, the most beautiful I've ever seen, but they slow down playing! I know it's unlikely ... Odp: After running ./configure, edit config.h and replace #undef FAST_OSD with #define FAST_OSD. Then recompile. Pyt: The onscreen display (OSD) is flickering!

MPlayer - Odtwarzacz filmów dla LINUKSA

Odp: You use a vo driver with single buffering (x11,xv). With xv, use the -double option. Also try -vf expand. Pyt: What exactly is this libavcodec thing? Odp: See the libavcodec section. Pyt: But configure tells me

Checking for libavcodec ... no

Odp: You need to get libavcodec from FFmpeg's CVS. Read the instructions in the libavcodec section. Pyt: Icewm's taskbar keeps covering the movie in fullscreen mode! Odp: This shouldn't happen anymore, if it still does use the -fstype layer option and report it to the mplayer-users mailing list. Pyt: I can't access the GUI menu. I press right click, but I can't access any menu items! Odp: Are you using FVWM? Try the following:

Start -> Settings -> Configuration -> Base Configuration 1. Set Use Applications position hints to Yes 2. Pyt: How can I run MPlayer in the background? Odp: Use:

mplayer options filename < /dev/null &

4.4. Playback problems

Pyt: I cannot pinpoint the cause of some strange playback problem. Odp: Do you have a stray codecs.conf file in ~/.mplayer/, /etc/, /usr/local/etc/ or a similar location? Remove it, outdated

codecs.conf files can cause obscure problems. MPlayer will use its builtin one instead.

Pyt: ... works with xine/avifile/... but doesn't with MPlayer. Odp: MPlayer is not xine/avifile/.... Although these players have some code in common, the codecs (DLL) set, synchronization, demultiplexing etc is different and should not be compared. If you have a file MPlayer fails to play correctly but works in another player, please read the bug reporting guidelines and upload the file to our FTP server.

Pyt: Audio goes out of sync playing an AVI file. Odp: Try the -bps or -nobps option. If it does not improve, read this and upload the file to FTP. Pyt: MPlayer exits with some error when using l3codeca.acm. Odp: Check ldd /usr/local/bin/mplayer output. If it contains

libc.so.6 => /lib/libc.so.6 (0x4???????)

where "?" is any number then it's OK, the error is not here. If it is:

libc.so.6 => /lib/libc.so.6 (0x00??????)

then there is a problem with your kernel/libc. Maybe you are using some security patches (for example Solar Designer's OpenWall patch) which forces loading libraries to very low addresses. Because l3codeca.acm is a non-relocatable DLL, it must be loaded to 0x00400000, we can't change this. You should use a non-patched kernel, or use MPlayer's -afm 1 option to disable using l3codeca.acm.

Pyt: My computer plays MS DivX AVIs with resolutions ~ 640x300 and stereo mp3 sound too slow. When I use -nosound option, everything is OK (but quiet).

Odp: Your machine is too slow or your soundcard driver is broken. Consult the documentation to see if you can improve performance. Pyt: MPlayer dies with

MPlayer - Odtwarzacz filmów dla LINUKSA

MPlayer interrupted by signal 4 in module: decode_video

Odp: Try running MPlayer on the machine you compiled on. Or recompile with runtime CPU detection (./configure --enable-runtime-cpudetection).

Don't use MPlayer on a CPU different from the one it was compiled on, without using the feature mentioned just now. Pyt: I have problems with [your window manager] and fullscreen xv/xmga/sdl/x11 modes ... Odp: Read the bug reporting guidelines and send us a proper bug report. Pyt: I got this playing MPEG files: Can't find codec for video format 0x10000001! Odp: You have an old version of codecs.conf in ~/.mplayer/, /etc/, /usr/local/etc/ or similar. Remove it, it's not needed anymore. OR you have the vc= option or something similar in your config file(s).

Pyt: When starting MPlayer under KDE I just get a black screen and nothing happens. After about one minute the video starts playing. Odp: The KDE arts sound daemon is blocking the sound device. Either wait until the video starts or disable the arts-daemon in control center. If you want to use arts sound, specify audio output via our native arts audio driver (-ao arts). If it fails or isn't compiled in, try SDL (-ao sdl) and make sure your SDL can handle arts sound. Yet another option is to start MPlayer with artsdsp.

Pyt: I have an AVI that produces a gray screen when played with -vc odivx and a green one with -vc divx4. Odp: It's not a DivX file, but an MS MPEG4v3. If you have an old version of codecs.conf in ~/.mplayer/, /etc/, /usr/local/etc/ or similar, remove it.

Pyt: When I play this movie I get video-audio desync and/or MPlayer crashes with the following message:

DEMUXER: Too many (945 in 8390980 bytes) video packets in the buffer!

Odp: This can have multiple reasons.

Your CPU and/or video card and/or bus is too slow. MPlayer displays a message if this is the case (and the dropped frames counter goes up fast). • If it is an AVI, maybe it has bad interleaving. Try the -ni option. • Your sound driver is buggy, or you use ALSA 0.5 with -ao oss. See the sound card section. • The AVI has a bad header, try the -nobps option, and/or -mc 0. • Pyt: I have an MJPEG file which works with other players but displays only a black image in MPlayer Odp: Use another codec to play the file, try -vc ffmjpeg. Pyt: When I try to grab from my tuner, it works, but colors are strange. It's OK with other applications. Odp: Your card probably misreports its colorspace capacity. Try with YUY2 instead of default YV12 (see the TV section). Pyt: I have A/V sync problems. Some of my AVIs play fine, but some play with double speed! Odp: You have a buggy sound card/driver. Most likely it's fixed at 44100Hz, and you try to play a file which has 22050Hz audio. Try the resample audio plugin.

Pyt: All the WMV (or other..) files I play create a green/gray window and there is only sound! MPlayer prints:

Detected video codec: [null] drv:0 (NULL codec (no decoding))

Odp: If you have an old version of codecs.conf in ~/.mplayer/, /etc/, /usr/local/etc/ or similar, remove it. Pyt: I get very strange percentage values (way too big) while playing files on my notebook. Odp: It's an effect of the power management / power saving system of your notebook (BIOS, not kernel). Plug the external power connector in before you power on your notebook. You can also try whether cpufreq (a SpeedStep interface for Linux) helps you.

Pyt: The audio/video gets totally out of sync when I run MPlayer as root on my notebook. It works normal when i run it as a user. Odp: This is again a power management effect (see above). Plug the external power connector in before you power on your notebook or use the -nortc option.

Pyt: While playing a movie it suddenly gets jerky and I get the following message:

Badly interleaved AVI file detected - switching to -ni mode...

Odp: Badly interleaved files and -cache don't work well together. Try -nocache.

MPlayer - Odtwarzacz filmów dla LINUKSA

Pyt: How can I play MPEG Layer 2 (mp2) audio files? Odp: You have to use -rawaudio on:format=0x50.

4.5. Video/audio driver problems (vo/ao)

Pyt: I have no sound when playing a video and get error messages similar to this one:

    AO: [oss] 44100Hz 2ch Signed 16-bit (Little-Endian)
    audio_setup: Can't open audio device /dev/dsp: Device or resource busy
    couldn't open/init audio device -> NOSOUND
    Audio: no sound!!!
    Start playing...

Odp: Are you running KDE or GNOME with the ARTS or ESD sound daemon? Try disabling the sound daemon or use the -ao arts or -ao esd option to make MPlayer use ARTS or ESD.

Pyt: What about the DGA driver? I can't find it! Odp: ./configure autodetects your DGA driver. If -vo help doesn't show DGA, then there's a problem with your X installation. Try ./configure --enable-dga and read the DGA section. Alternatively, try SDL's DGA driver with the -vo sdl:dga option.

Pyt: OK, -vo help shows DGA driver, but it complains about permissions. Help me! Odp: It works only if running as root! It's a DGA limitation. You should become root (su -), and try again. Another solution is making MPlayer SUID root, but it's not recommended!

     chown root /usr/local/bin/mplayer
     chmod 755 /usr/local/bin/mplayer
     chmod +s /usr/local/bin/mplayer

Ostrze¿enie

This is a big security risk! Never do this on a server or on a computer that you do not control completely because other users can gain root privileges through SUID root MPlayer. You have been warned.

Pyt: When using Xvideo, my Voodoo 3/Banshee says:

X Error of failed request: BadAccess (attempt to access private resource denied)
   Major opcode of failed request: 147 (MIT-SHM)
   Minor opcode of failed request: 1 (X_ShmAttach)
   Serial number of failed request: 26
   Current serial number in output stream:27

Odp: The tdfx driver in XFree86 4.0.2/4.0.3 had this bug. This was solved by bugfix #621 of the XFree86 4.1.0 CVS log. So upgrade to XFree86 4.1.0 or later. Alternatively, either download (at least) DRI version 0.6 from the DRI homepage, or use CVS DRI.

Pyt: OpenGL (-vo gl) output doesn't work (hang/black window/X11 errors/...). Odp: Your OpenGL driver doesn't support dynamic texture changes (glTexSubImage). It's known not to work with nVidia's binary mess. It's known to work with Utah-GLX/DRI and Matrox G400 cards. Also with DRI and Radeon cards. It won't work with DRI and other cards. it will not work with 3DFX cards because of the 256x256 texture size limit.

Pyt: I have an nVidia TNT/TNT2 card, and I have a band with strange colors, right under the movie! Whose fault is this? Odp: This is a bug of nVidia's binary X driver. These bugs appear ONLY with the TNT/TNT2 cards, and we can't do anything about it. To fix the problem, upgrade to the latest nVidia binary driver version. If still bad, complain to nVidia!

Pyt: I have an nVidia XYZ card, and when I click on the GUI's display window to toggle displaying the GUI panel, a black square appears where I clicked. I have the newest driver.

Odp: Yes, nVidia corrected a previous bug (above), and introduced a new one. Let's congratulate them. UPDATE: According to nVidia, this has already been fixed.

MPlayer - Odtwarzacz filmów dla LINUKSA

4.5. Video/audio driver problems (vo/ao) 87

Pyt: Oh the world is cruel ...! SDL has only x11 target, but not xv! Odp: Try that x11 target again. Now try -vo x11 -fs -zoom. See the difference? No?! OK, here comes the enlightenment: SDL's x11 target uses xv when available, you don't have to worry about it ... Note: With SDL you can force/disable Xv using -forcexv and -noxv.

4.6. DVD playback

Pyt: What about DVD navigation? Odp: Support for dvdnav in MPlayer is currently broken, normal playback does work, though. If you want to have fancy menus, you will have to use another player like Xine or Ogle. If you care about DVD navigation, send a patch.

Pyt: While playing a DVD, I encountered this error:

mplayer: ifo_read.c:1143: ifoRead_C_ADT_internal: Assertion nfo_length / sizeof(cell_adr_t) >= c_adt->nr_of_vobs' failed.

Odp: This is a known libdvdread 0.9.1/0.9.2 bug. Use libmpdvdkit2, which is present in MPlayer source, and used by default. Pyt: Can I compile libdvdread and libdvdcss on my sweet SPARC under Solaris? Odp: Who knows ... It's said to work, so please test it and send feedback. Refer to the documentation of libdvdread and its homepage as well. We're not the authors of libdvdread. Use libmpdvdkit2, which is present in MPlayer source, and used by default.

Pyt: What about subtitles? Can MPlayer display them? Odp: Yes. See the DVD chapter. Pyt: How can I set the region code of my DVD-drive? I don't have Windows! Odp: Use the regionset tool. Pyt: Do I need to be (setuid) root/setuid fibmap_mplayer to be able to play a DVD? Odp: No. However you must have the proper rights on the DVD device entry (in /dev/). Pyt: Where can I get libdvdread and libdvdcss packages? Odp: You don't need to. Use libmpdvdkit2, which is present in the MPlayer source, and used by default. You can get the mentioned packages from the Ogle site.

Pyt: Is it possible to play/encode only selected chapters? Odp: Yes, try the -chapter option. Pyt: My DVD playback is sluggish! Odp: Use the -cache option (described in the man page) and try enabling DMA for the DVD drive with the hdparm tool (described in the CD chapter).

4.7. Feature requests

Pyt: If MPlayer is paused and I try to seek or press any key at all, MPlayer ceases to be paused. I would like to be able to seek in the paused movie. Odp: This is very tricky to implement without losing A/V synchronization. All attempts have failed so far, but patches are welcome. Pyt: I'd like to seek +/- 1 frames instead of 10 seconds. Odp: This won't be done. It was, but then it messed up A/V sync. Feel free to implement it, and send a patch. Don't ask for it. Pyt: How can I make MPlayer remember the options I use for this particular file? Odp: Create a file named movie.avi.conf with the file-specific options in it and put it in ~/.mplayer or in the same directory as the file.

4.8. Encoding

Pyt: How can I encode? Odp: Read the MEncoder section. Pyt: How can I create VCDs? Odp: Try the mencvcd script from the TOOLS subdirectory. With it you can encode DVDs or other movies to VCD or SVCD format and even burn them directly to CD.

MPlayer - Odtwarzacz filmów dla LINUKSA

4.6. DVD playback 88

Pyt: How can I join two video files? Odp: This has been discussed to no end on mplayer-users. Go search the archives for a complete answer. This is a complicated topic and your mileage may vary a lot depending on the kind of files you want to merge. MPEGs can be concatenated into a single file with luck. For AVIs there are two tools, avidemux and avimerge (part of the transcode tool set), available that might do the job. You can also try MEncoder if you have two files sharing the same dimensions and codec. Try

     cat file1 file2 > file3
     mencoder -ovc copy -oac copy -o out.avi -forceidx file3.avi

Pyt: My tuner works, I can hear the sound and watch the video with MPlayer, but MEncoder doesn't encode audio! Odp: TV audio encoding for Linux is currently unimplemented, we're working on it. At the moment it works only on BSD. Pyt: I can't encode DVD subtitles into the AVI! Odp: You have to specify the -sid option correctly! Pyt: MEncoder segfaults on startup! Odp: Upgrade DivX4Linux. Pyt: How can I encode only selected chapters from a DVD? Odp: Use the -chapter option correctly, like: -chapter 5-7 Pyt: I'm trying to work with 2GB+ files on a VFAT file system. Does it work? Odp: No, VFAT doesn't support 2GB+ files. Pyt: Why is the recommended bitrate printed by MEncoder negative? Odp: Because the bitrate you encoded the audio with is too large to fit the movie on any CD. Check if you have libmp3lame installed properly. Pyt: I can't encode ASF files to AVI/DivX because it uses 1000 fps? Odp: Because ASF uses variable frame rate but AVI uses a fixed one, you have to set it by hand using -ofps. Pyt: How can I put subtitles in the output file? Odp: Just pass the -sub <filename> (or -sid, -vobsub, respectively) option to MEncoder.

Rozdzia³ 5. U¿ywanie CD/DVD

Spis tre¶ci

5.1. Napêdy CD/DVD 5.2. Odtwarzanie DVD 5.3. Odtwarzanie VCD

5.1. Napêdy CD/DVD

Fragment dokumentacji Linuksa:

Nowoczesne napêdy CD-ROM osi±gaj± bardzo du¿e prêdko¶ci. Niektóre z nich s± dodatkowo zdolne do pracy przy zredukowanych prêdko¶ciach. Oto kilka powodów, dla których powinni¶my zastanowiæ siê czy nie nale¿y zredukowaæ prêdko¶ci naszego napêdu:

Istniej± doniesienia o b³êdach odczytu przy du¿ych prêdko¶ciach, szczególnie podczas u¿ywania uszkodzonych b±d¼ wadliwie wyt³oczonych/nagranych p³yt CD. Redukcja prêdko¶ci odczytu mo¿e uchroniæ nas przed utrat± danych w takich przypadkach. •

Wiele napêdów CD jest dokuczliwie g³o¶nych. Redukcja prêdko¶ci mo¿e zmniejszyæ natê¿enie ha³asu. •

MPlayer - Odtwarzacz filmów dla LINUKSA

Rozdzia³ 5. U¿ywanie CD/DVD 89

Redukcjê prêdko¶ci napêdu CD z interfejsem IDE mo¿emy uzystaæ korzystaj±c z hdparm b±d¼ programu setcd. Dzia³aj± one w nastêpuj±cy sposób:

hdparm -E [prêdko¶æ] [urz±dzenie cdrom]

setcd -x [prêdko¶æ] [urz±dzenie cdrom]

Je¿eli masz uprawnienia roota, to pomóc mo¿e tak¿e nastêpuj±ca komenda:

echo file_readahead:2000000 > /proc/ide/[urz±dzenie cdrom]/settings

Ustawiamy w ten sposób wielko¶æ bufora odczytu na 2MB, co pomaga przy odczycie porysowanych p³yt. Je¿eli ustawimy zbyt du¿± wielko¶æ tego bufora, napêd bêdzie stale rozkrêca³ siê i zwalnia³, co spowoduje bardzo znaczny spadek wydajno¶ci. Zaleca siê równie¿ dostrojenie napêdu CD-ROM przy u¿yciu hdparm:

hdparm -d1 -a8 -u1 [urz±dzenie cdrom]

W³±czamy w ten sposób dostêp DMA do dysku, czytanie z wyprzedzeniem i odmaskowanie IRQ (IRQ unmasking) (wiêcej przeczytasz na stronach man do hdparm)

Proszê sprawdziæ "/proc/ide/urz±dzenie cdrom/settings" dla dostrojenia swojego napêdu CD-ROM.

Dla napêdów SCSI nie istnieje jednolity sposób ustawiawiania tych parametrów (je¿eli znasz jaki¶ to napisz nam o nim). Istnieje narzêdzie które dzia³a z napêdami SCSI Plextor.

FreeBSD:

Prêdko¶æ: cdcontrol [-f device] speed speed

DMA: sysctl hw.ata.atapi_dma=1

5.2. Odtwarzanie DVD

Aby poznaæ pe³n± listê dostêpnych opcji, proszê przeczytaæ odpowiednie strony man. Sk³adnia dla standardowego DVD (Digital Versatile Disc) jest nastêpuj±ca:

mplayer dvd://<¶cie¿ka> [-dvd-device <urz±dzenie>]

Przyk³ad:

mplayer dvd://1 -dvd-device /dev/hdc

Domy¶lnym urz±dzeniem (device) DVD jest /dev/dvd. Je¿eli Twoje ustawienia s± inne, stwórz odpowiedni symlink lub ustaw odpowiednie urz±dzenie (device) w linii polecenia korzystaj±c z opcji

-dvd-device.

Obs³uga DVD - nowy sposób (mpdvdkit2). MPlayer u¿ywa libdvdread oraz libdvdcss do dekodowania i odtwarzania DVD. Te dwie biblioteki s± zawarte w podkatalogu libmpdvdkit2/ w g³ównym drzewie katalogów MPlayera, nie trzeba instalowaæ ich osobno. Wybrali¶my tê opcjê poniewa¿ musieli¶my poprawiæ b³±d libdvdread i zastosowaæ ³atkê (patch), która dodaje obs³ugê buforowania

MPlayer - Odtwarzacz filmów dla LINUKSA

5.2. Odtwarzanie DVD 90 z³amanych kluczy CSS do libdvdcss. Skutkuje to du¿ym wzrostem szybko¶ci poniewa¿ klucze nie musz± byæ ³amane za ka¿dym razem przed odtwarzaniem.

Notatka

Je¶li wystêpuj± problemy z dekodowaniem DVD, spróbuj wy³±czyæ supermount albo inne tego typu us³ugi.

MPlayer potrafi tak¿e u¿ywaæ bibliotek systemowych libdvdread oraz libdvdcss, ale to rozwi±zanie jest nie zalecane, gdy¿ mo¿e powodowaæ b³êdy, niekompatybilno¶ci bibliotek oraz zmniejszenie prêdko¶ci.

Obs³uga DVD - stary sposób - OPCJONALNE. U¿yteczne, je¿eli chcesz odtwarzaæ zakodowane pliki VOB z twardego dysku. W tym celu skompiluj i zainstaluj libcss 0.0.1 (nie nowsze) (Je¿eli MPlayer nie radzi sobie, u¿yj opcji -csslib /¶cie¿ka/do/libcss.so). Aby u¿yæ tej metody musisz mieæ uprawnienia roota, binarka MPlayer musi miec suid lub pozwól MPlayerowi na uruchamianie owijacza (wrapper) fibmap_mplayer z suid-root.

Struktura dysku DVD. Dyski DVD maj± po 2048 bajtów na sektor z ECC/CRC. Zwykle posiadaj± system plików UDF na pojedynczej ¶cie¿ce zawieraj±cej ró¿norakie pliki (ma³e pliki .IFO i .BUK oraz du¿e (1GB) pliki .VOB). S± one rzeczywistymi plikami i mog± byæ kopiowane/odtwarzane z podmontowanego systemu plików niezakodowanego DVD.

Pliki .IFO zawieraj± informacje nawigacyjne filmu (rozdzia³/tytu³/mapa zaczepów/tablica jêzyków, itp) i s± konieczne do odczytu i interpretacji zawarto¶ci pliku .VOB (filmu). Pliki .BUK s± kopiami zapasowymi plików .IFO. U¿ywaj± sektorów wszêdzie, wiêc aby zaimplementowaæ nawigacjê na DVD lub rozszyfrowaæ zawarto¶æ, nale¿y u¿ywaæ adresowania sektorów dysku w trybie raw.

Z tego powodu obs³uga DVD w starym stylu z u¿yciem libcss wymaga podmontowanego systemu plików DVD oraz dostêpu do urz±dzenia w trybie raw bazuj±cym na sektorach. Niestety wymagane jest (pod Linuksem) posiadanie uprawnieñ roota aby móc korzystaæ z sektorowego adresowania pliku. Wybór jest nastêpuj±cy:

Posiadaæ uprawnienia roota lub u¿ywaæ programu wykonywalnego MPlayera posiadaj±cego prawa suid-root. • Pozwoliæ MPlayerowi na uruchamianie owijacza (wrapper) fibmap_mplayer w trybie suid-root w celu uzyskania dostêpu do DVD (u¿ywane przy odtwarzaniu DVD star± metod± poprzez libcss). • Wcale nie u¿ywaæ sterownika systemu plików zawartego w j±drze lecz korzystaæ jedynie z narzêdzi dzia³aj±cych w przestrzeni u¿ytkownika. Zajmuj± siê tym biblioteki libdvdread 0.9.x i

libmpdvdkit (obs³uga DVD nowym sposobem). Sterownik systemu plików UDF zawarty w

j±drze nie jest wymagany poniewa¿ wspomniane biblioteki zawieraj± w³asny, wbudowany sterownik systemu plików UDF. DVD nie musi byæ podmontowany, bowiem u¿ywany jest jedynie dostêp w trybie raw.

•

Czasami /dev/dvd nie mo¿e byæ czytany przez u¿ytkowników, zatem autorzy libdvdread zaimplementowali emulacjê warstwy, która przenosi adresowanie sektorowe na nazwy plików i offsety, aby ju¿ u ¼róde³ podmontowanego systemu plików emulowaæ dostêp w trybie raw, na równi z dostêpem do dysku twardego.

libdvdread równie dobrze akceptuje miejsce podmontowania (mountpoint) jak i nazwê urz±dzenia przy

dostêpie w trybie raw i sprawdza /proc/mounts w celu odnalezienia odpowiedniej nazwy urz±dzenia (device). Zosta³o to napisane z my¶l± o systemie Solaris, gdzie nazwy urz±dzeñ s± przydzielane

MPlayer - Odtwarzacz filmów dla LINUKSA automatycznie.

Domy¶lnym urz±dzeniem (device) DVD jest /dev/dvd. Je¿eli Twoje ustawienia s± inne, stwórz odpowiedni symlink lub ustaw odpowiednie urz±dzenie w linii polecenia korzystaj±c z opcji

-dvd-device.

Autoryzacja DVD. Metoda autoryzacji i rozszyfrowywania u¿ywana gdy korzystamy z DVD przy u¿yciu nowego sposobu polega na korzystaniu ze zmodyfikowanej biblioteki libdvdcss (patrz wy¿ej). Ta metoda mo¿e byæ okre¶lona poprzez zmienna ¶rodowiskow± DVDCSS_METHOD, która mo¿e byæ ustawiona na "key", "disk" albo "title".

Je¿eli ¿adna warto¶æ nie jest ustawiona, próbowane s± nastêpuj±ce metody (domy¶lnie: "key", "title request"):

bus key: Ten klucz jest ustalany podczas autoryzacji (d³uga mieszanina ioctl'i i rozmaite wymiany kluczy, bajery kryptograficzne) oraz jest u¿ywany do szyfrowania tytu³u i kluczy dyskowych przed wys³aniem ich nieszyfrowan± magistral± (by zapobiec pods³uchiwaniu). Bus key jest wymagany do pobrania i wstêpnego rozszyfrowania zaszyfrowanego klucza dyskowego (disk key).

1.

cached key: MPlayer wyszukuje ju¿ z³amane klucze tytu³ów, które s± przechowywane w katalogu

~/.mplayer/DVDKeys (szybkie ;) ).

2. key: Je¿eli ¿aden zbuforowany klucz nie jest dostêpny, MPlayer próbuje rozszyfrowaæ klucz dyskowy korzystaj±c z gar¶ci kluczy zaszytych w odtwarzaczu. 3. disk: Je¿eli metoda "key" zawodzi (np. brak kluczy zaszytych w odtwarzaczu), MPlayer z³amie klucz dyskowy u¿ywaj±c algorytmu ataku brutalnego. Proces ten jest bardzo procesoroch³onny i wymaga 64 MB pamiêci (16777216 (16*2^20) 32-bitowych pól tabeli hash) do przechowywania tymczasowych danych. Ta metoda powinna zadzia³aæ zawsze (niestety jest wolna).

4.

title request: Maj±c klucz dyskowy MPlayer pobiera zaszyfrowane klucze tytu³owe (title key), które s± zawarte w ukrytych sektorach (hidden sectors) u¿ywaj±c ioctl(). Ochrona regionalna w napêdach RPC-2 jest realizowana w tym kroku i mo¿e siê nie udaæ na tych napêdach. Je¶li jednak siê uda, klucze tytu³owe zostaj± rozszyfrowane przy u¿yciu magistrali i klucza dyskowego.

5.

title: Ta metoda jest u¿ywana je¿eli zapytanie o tytu³ zakoñczy³o siê niepowodzeniem i nie mo¿na polegaæ na ¿adnej wymianie kluczy z napêdem DVD. U¿ywa ona ataku kryptograficznego w celu odgadniêcia klucza tytu³owego (title key) wprost (poprzez szukanie powtarzaj±cego siê ci±gu znaków (wzoru) w rozszyfrowanej zawarto¶ci pliku VOB oraz poprzez zgadywanie, ¿e czysty tekst odpowiadaj±cy pierwszym zaszyfrowanym bajtom jest kontynuacj± wzoru). Metoda ta jest tak¿e znana jako "znany czysto-tekstowy atak (known plaintext attack)" b±d¼ "DeCSSPlus". Rzadko zdarza siê, ale siê zdarza, ¿e metoda ta mo¿e zawie¶æ poniewa¿ jest niewystarczaj±co du¿o zaszyfrowanych danych na dysku aby spe³niæ za³o¿enia statystycznego ataku lub poniewa¿ klucz zmienia siê w trakcie tytu³u. Jest to jedyna metoda, aby zdeszyfrowaæ DVD przechowywane na twardym dysku lub DVD ze z³ym regionem na napêdzie RPC2 (powolne).

6.

Napêdy DVD RPC-1 zabezpieczaj± ustawienia regionu jedynie poprzez oprogramowanie. Napêdy RPC-2 maj± sprzêtowe zabezpieczenie, które pozwala na co najwy¿ej 5 zmian. Je¿eli posiadamy napêd DVD RPC-2 wymagana/zalecana jest aktualizacja firmware'u do RPC-1 . Nowe wersje firmware'ów mo¿na znale¼æ na tej stronie z firmware'ami. Je¿eli nie ma tam nowej wersji firmware'u dla naszego urz±dzenia, u¿yj regionset tool (narzêdzia do zmiany regionów) aby ustawiæ kod regionu na swoim napêdzie DVD (pod Linuksem). Ostrze¿enie: Mo¿esz ustawiæ region tylko 5 razy.

MPlayer - Odtwarzacz filmów dla LINUKSA

5.3. Odtwarzanie VCD

Pe³na lista dostêpnych opcji znajduje siê na stronie man. Sk³adnia dla standardowego Video CD (VCD) jest nastêpuj±ca:

mplayer vcd://<¶cie¿ka> [-cdrom-device <urz±dzenie>]

Przyk³ad:

mplayer vcd://2 -cdrom-device /dev/hdc

Domy¶lnym urz±dzeniem VCD jest /dev/cdrom. Je¶li Twoje ustawienia s± inne, utwórz dowi±zanie symboliczne lub podaj prawid³owe urz±dzenie w linii poleceñ za pomoc± opcji -cdrom-device

Notatka

Przynajmniej napêdy CD-ROM SCSI firmy Plextor i niektóre modele Toshiby maj± beznadziejn± wydajno¶æ przy odczycie VCD. Jest to spowodowane niekompletn± implementacj± ioctl'a CDROMREADRAW dla tych urz±dzeñ. Je¶li masz jakie¶ pojêcie o programowaniu SCSI, pomó¿ nam zaimplementowaæ ogóln± obs³ugê SCSI dla VCD.

W miêdzyczasie mo¿esz wyci±gaæ dane z VCD za pomoc± readvcd i odtwarzaæ plik wynikowy za pomoc± MPlayera

Struktura VCD. P³yty VCD sk³adaj± siê z jednej lub wiêcej ¶cie¿ek:

Pierwsza ¶cie¿ka jest ma³± ¶cie¿k± o gêsto¶ci 2048 bajtów/sektor z danymi w systemie plików iso9660, zwykle zawieraj±ca windowsowy odtwarzacz VCD i byæ mo¿e inne informacje (obrazy, tekst, itp.). •

Druga i pozosta³e ¶cie¿ki o gêsto¶ci 2324 bajtów/sektor zawieraj± po jednym pakiecie czystego strumienia MPEG PS na sektor zamiast systemu plików. Podobnie, jak w przypadku ¶cie¿ek audio CD, ¶cie¿ki te nie mog± byæ montowane (Czy kiedykolwiek montowa³e¶ p³ytê audio CD by j± odtworzyæ?). Bior±c pod uwagê, ¿e filmy znajduj± siê na tej ¶cie¿ce, powiniene¶ spróbowaæ na pocz±tek opcji vcd://2.

•

Istniej± równie¿ p³yty VCD bez pierwszej ¶cie¿ki (pojedyncza ¶cie¿ka i brak systemu plików w ogóle). Je równie¿ da siê odtwarzaæ, ale nie da siê ich montowaæ. •

O plikach .DAT. Plik o rozmiarze ok. 600 MB widoczny na pierwszej ¶cie¿ce zamontowanego VCD nie jest prawdziwym plikiem ! Jest on tzw. bramk± ISO, utworzon± by Windows móg³ obs³ugiwaæ takie ¶cie¿ki (Windows w ogóle nie zezwala aplikacjom na dostêp do urz±dzeñ w trybie raw). Pod Linuksem nie mo¿esz kopiowaæ ani odtwarzaæ tych plików (zawieraj± "¶mieci"). Pod Windows jest to mo¿liwe, gdy¿ jego sterownik iso9660 symuluje odczyt ¶cie¿ek w trybie raw za pomoc± tego pliku. By móc odtwarzaæ pliki .DAT, musisz mieæ sterownik do j±dra, który dostarczany jest z linuksow± wersj± PowerDVD. Posiada on zmodyfikowany sterownik systemu plików iso9660 (vcdfs/isofs-2.4.X.o), który jest w stanie symulowaæ odczyt ¶cie¿ek w trybie raw za pomoc± pliku .DAT. Je¶li podmontujesz p³ytê u¿ywaj±c ich sterownika, mo¿esz kopiowaæ, a nawet odtwarzaæ pliki .DAT za pomoc± MPlayera. Ale nie bêdzie to dzia³a³o za pomoc± standardowego sterownika iso9660 dostarczonego z j±drem Linuksa! Zamiast tego u¿yj opcji vcd://. Alternatyw± dla kopiowania VCD jest nowy sterownik: cdfs (nie jest czê¶ci± oficjalnego j±dra), który wy¶wietla sesje CD jako pliki obrazów, oraz cdrdao, program do zgrywania p³yt CD bit po bicie.

MPlayer - Odtwarzacz filmów dla LINUKSA

5.3. Odtwarzanie VCD 93

Rozdzia³ 6. Porty

Spis tre¶ci

6.1. Linux

6.1.1. Pakiety Debiana 6.1.2. Pakiety RPM 6.1.3. ARM 6.2. *BSD

6.2.1. FreeBSD 6.2.2. OpenBSD 6.2.3. Darwin 6.3. Sun Solaris 6.4. Silicon Graphics Irix 6.5. QNX 6.6. Windows

6.6.1. Cygwin 6.6.2. MinGW 6.7. Mac OS 6.8. HP UX 6.9. Amiga/MorphOS (zabawki dla zapaleñców)

6.1. Linux

G³ówn± platform± rozwojow± jest Linux x86, chocia¿ MPlayer pracuje równie¿ na wielu innych portach tego systemu. Pakiety binarne s± dostêpne z kilku ¼róde³, jednak¿e ¿aden z nich nie jest przez nas obs³ugiwany. Zg³aszaj problemy do ich opiekunów, a nie do nas.

6.1.1. Pakiety Debiana

Aby zbudowaæ pakiet dla Debiana, wywo³aj poni¿sz± komendê w katalogu ze ¼ród³ami MPlayera:

fakeroot debian/rules binary

Jako superu¿ytkownik mo¿esz zainstalowaæ pakiet .deb tak, jak zwykle:

dpkg -i ../mplayer_wersja.deb

Christian Marillat buduje dla Debiana nieoficjalne paczki MPlayera, MEncodera i czcionek ju¿ przez jaki¶ czas, mo¿esz je pobraæ (apt-get) z jego strony domowej.

6.1.2. Pakiety RPM

Dominik Mierzejewski tworzy i opiekuje siê oficjalnymi pakietami MPlayera dla Red Hata. S± one dostêpne na jego stronie domowej.

RPMy dla Mandrake s± dostêpne na P.L.F.. SuSE zawiera³ okrojon± wersjê MPlayera w dystrybucji. Usunêli j± w swoich najnowszych wydaniach. W pe³ni funkcjonalne pakiety mo¿esz pobraæ z links2linux.de.

MPlayer - Odtwarzacz filmów dla LINUKSA

Rozdzia³ 6. Porty 94

6.1.3. ARM

MPlayer dzia³a równie¿ na PDA z procesorami ARM dzia³aj±cych pod kontrol± Linuksa, np. Sharp Zaurus, Compaq iPAQ. Najprostszym sposobem, ¿eby uzyskaæ MPlayera, jest pobranie go z odpowiedniego ¼ród³a pakietów (stable, testing, unstable) z witryny OpenZaurus. Je¿eli chcesz go skompilowaæ samodzielnie, powiniene¶ przyjrzeæ siê katalogom MPlayera i biblioteki libavcodec w g³ównym katalogu ¼ród³owym OpenZaurusa. Zawieraj± one naj¶wie¿sze ³atki i pliki Makefile, s³u¿±ce do samodzielnej kompilacji MPlayera z libavcodec. Je¿eli potrzebujesz interfejsu GUI, mo¿esz u¿yæ xmms-embedded.

6.2. *BSD

MPlayer dzia³a na FreeBSD, OpenBSD, NetBSD, BSD/OS i Darwinie. Dostêpne s± wersje portów/pkgsrc/fink/itp., które prawdopodobnie s± ³atwiejsze w instalacji, ni¿ kompilacja ze ¼róde³.

Do zbudowania MPlayera bêdziesz potrzebowa³ GNU make (gmake - rdzenne make BSD nie zadzia³a) i najnowszej wersji binutils.

Je¿eli MPlayer nie mo¿e znale¼æ /dev/cdrom lub /dev/dvd, stwórz odpowiednie dowi±zanie symboliczne:

ln -s /dev/twoje_urz±dzenie_cdrom /dev/cdrom

Aby u¿ywaæ bibliotek Win32 z MPlayerem, bêdziesz potrzebowa³ przekompilowaæ j±dro z opcj± "USER_LDT" (chyba, ¿e u¿ywasz FreeBSD-CURRENT, tam jest domy¶lnie w³±czona).

6.2.1. FreeBSD

Je¿eli Twój procesor ma rozszerzenie SSE, przekompiluj j±dro z opcj± "CPU_ENABLE_SSE" (wymagany FreeBSD-STABLE lub ³aty na j±dro).

6.2.2. OpenBSD

Ze wzglêdu na ograniczenia w ró¿nych wersjach gas (GNU assemblera - przyp. t³umacza) (dotycz±ce relokacji i MMX), bêdziesz musia³ przeprowadziæ kompilacjê w dwóch krokach: Po pierwsze, upewnij siê, ¿e wersja nierdzenna wystêpuje w zmiennej $PATH i wykonaj gmake -k, a nastêpnie upewnij siê, ¿e u¿ywana jest wersja rdzenna i wykonaj gmake.

6.2.3. Darwin

Zobacz rozdzia³ Mac OS.

6.3. Sun Solaris

MPlayer powinien dzia³aæ na Solarisie 2.6 lub nowszym.

Na UltraSPARCach, MPlayer korzysta z rozszerzenia VIS (odpowiednik MMX), obecnie tylko w libmpeg2, libvo i libavcodec, ale nie w mp3lib. Mo¿esz ogl±daæ plik VOB na procesorze z taktowaniem 400MHz. Bêdziesz potrzebowa³ do tego biblioteki mLib.

MPlayer - Odtwarzacz filmów dla LINUKSA

Aby zbudowaæ pakiet, bêdziesz potrzebowa³ GNU make (gmake, /opt/sfw/gmake), rdzenne make Solarisa nie zadzia³a. Typowy b³±d jaki otrzymujesz, buduj±c tym drugim zamiast GNU make, to:

   % /usr/ccs/bin/make
   make: Fatal error in reader: Makefile, line 25: Unexpected end of line seen

W Solarisie przeznaczonym dla SPARC, potrzebujesz kompilatora GNU C/C++; nie ma znaczenia, czy jest on skonfigurowany z, czy bez GNU assemblera.

Na Solarisie x86, potrzebujesz GNU assemblera i kompilatora GNU C/C++, skonfigurowanego do u¿ywania GNU assemblera! Kod MPlayera, na platformie x86, w znacz±cy sposób korzysta z instrukcji MMX, SSE i 3DNOW!, które nie mog± byæ skompilowane przy pomocy assemblera Sun /usr/ccs/bin/as.

Skrypt configure stara siê okre¶liæ, jaki assembler wywo³ywany jest przez komendê "gcc" (je¿eli próba zakoñczy siê fiaskiem, u¿yj opcji --as=/gdziekolwiek/zainstalowa³e¶/gnu-as, ¿eby okre¶liæ gdzie skrypt configure mo¿e znale¼æ GNU "as" w Twoim systemie).

B³±d jaki wy¶wietli configure na Solarisie x86, u¿ywaj±cym GCC bez GNU assemblera:

   % configure
   ...
   Checking assembler (/usr/ccs/bin/as) ... , failed
   Please upgrade(downgrade) binutils to 2.10.1...

(Rozwi±zanie: Zainstaluj i u¿ywaj gcc skonfigurowanego z opcj± --with-as=gas)

Typowy b³±d, jaki otrzymasz przy próbie budowy kompilatorem GNU C, który nie u¿ywa GNU as:

   % gmake
   ...
   gcc -c -Iloader -Ilibvo -O4 -march=i686 -mcpu=i686 -pipe -ffast-math
        -fomit-frame-pointer  -I/usr/local/include   -o mplayer.o mplayer.c
   Assembler: mplayer.c
   "(stdin)", line 3567 : Illegal mnemonic
   "(stdin)", line 3567 : Syntax error
   ... more "Illegal mnemonic" and "Syntax error" errors ...

Ze wzglêdu na b³êdy wystêpuj±ce w Solarisie 8, mo¿esz nie byæ w stanie odtwarzaæ p³yt DVD o pojemno¶ci wiêkszej ni¿ 4 GB:

Sterownik sd(7D) dla Solarisa 8 x86 ma b³±d ujawniaj±cy siê przy próbie dostêpu do bloku dyskowego >4GB urz±dzenia korzystaj±cego z logicznego rozmiaru bloku !=DEV_BSIZE (np. no¶nik CD-ROM i DVD). Ze wzglêdu na przepe³nienie 32bitowych liczb ca³kowitych, odczytywany jest adres dysku modulo 4GB (http://groups.yahoo.com/group/solarisonintel/message/22516). Ten problem nie wystêpuje na Solarisie 8 przeznaczonym dla procesorów SPARC.

•

Podobny b³±d wystêpuje w kodzie systemu plików hsfs(7FS) (znanym jako ISO9660), hsfs mo¿e nie obs³ugiwaæ partycji/dysków wiêkszych ni¿ 4GB, wszystkie dane s± odczytywane z bloku modulo 4GB (http://groups.yahoo.com/group/solarisonintel/message/22592). Problem mo¿e byæ rozwi±zany przy pomocy ³atki 109764-04 (sparc) / 109765-04 (x86).

•

Na Solarisie UltraSPARC, mo¿esz otrzymaæ dodatkow± moc obliczeniow±, u¿ywaj±c instrukcji VIS dla pewnych, czasoch³onnych operacji. Akceleracja VIS mo¿e byæ u¿yta w MPlayerze, odwo³uj±c siê do funkcji zawartych w bibliotece Suna mediaLib.

MPlayer - Odtwarzacz filmów dla LINUKSA

Przyspieszone, przy pomocy VIS, operacje z biblioteki mediaLib s± wykorzystywane przy dekodowaniu video w formacie mpeg2 i konwersji przestrzeni kolorów w sterownikach wyj¶ciowych video.

6.4. Silicon Graphics Irix

Mo¿esz albo spróbowaæ zainstalowaæ program GNU install i (je¿eli nie umie¶ci³e¶ go w globalnej ¶cie¿ce) wskazaæ go przez:

./configure --with-install=
/¶cie¿ka/i/nazwa/programu/instalacyjnego

Albo u¿yæ domy¶lnego programu instalacyjnego dostarczonego z IRIX 6.5, w tym wypadku nale¿y rêcznie zmodyfikowaæ plik Makefile w kilku miejscach. Zmieñ poni¿sze dwie linijki:

  $(INSTALL) -c -m 644 DOCS/mplayer.1 $(MANDIR)/man1/mplayer.1

  $(INSTALL) -c -m 644 etc/codecs.conf $(CONFDIR)/codecs.conf

na:

  $(INSTALL) -m 644 mplayer.1 $(MANDIR)/man1/

  $(INSTALL) -m 644 codecs.conf $(CONFDIR)/

A potem wykonaj (w katalogu ¼ród³owym MPlayera):

cp DOCS/mplayer.1 . ; cp etc/codecs.conf .

i dalej skompiluj i zainstaluj.

6.5. QNX

Dzia³a. Bêdziesz musia³ ¶ci±gn±æ bibliotekê SDL dla QNX i zainstalowaæ j±. Wtedy uruchom MPlayera a opcj± -vo sdl:photon i -ao sdl:nto, powinno dzia³aæ szybko.

Wyj¶cie -vo x11 bêdzie nawet wolniejsze ni¿ na Linuksie, poniewa¿ QNX ma tylko emulacjê Xów, która jest bardzo wolna. U¿ywaj SDL.

6.6. Windows

Tak, MPlayer dzia³a na Windowsie pod Cygwinem i MinGW. Nie ma jeszcze interfejsu GUI, ale wersja dla wiersza poleceñ jest ju¿ prawie w pe³ni funkcjonalna. £atki s± zawsze mile widziane. Powiniene¶ sprawdziæ listê mplayer-cygwin, aby uzyskaæ pomoc albo otrzymaæ najnowsze informacje.

Najlepsze wyniki s± osi±gane ze sterownikami wyj¶ciowymi video DirectX (-vo directx) i rdzennym wyj¶ciem d¼wiêkowym wave Windows (-ao win32), jako ¿e OpenGL nie dzia³a, a SDL mo¿e zak³ócaæ d¼wiêk i obraz albo wywo³aæ b³±d i zamkn±æ siê na niektórych systemach. Je¿eli wystêpuj± zak³ócenia obrazu, spróbuj wy³±czyæ sprzêtow± akceleracjê przez opcjê -vo directx:noaccel. ¦ci±gnij pliki nag³ówkowe DirectX 7, ¿eby skompilowaæ sterownik do wyj¶cia video DirectX.

Mo¿esz wykorzystaæ kodeki Win32 i Real dla Win32 (nie kodeki Real dla Linuksa), je¿eli chcesz. Umie¶æ je gdzie¶ w swojej ¶cie¿ce (zmienna PATH - przyp. t³umacza) albo u¿yj opcji

MPlayer - Odtwarzacz filmów dla LINUKSA

6.4. Silicon Graphics Irix 97

--with-codecsdir=c:/¶cie¿ka/do/twoich/kodeków (lub
--with-codecsdir=/¶cie¿ka/do/twoich/kodeków tylko na Cygwin) dla configure.

Mieli¶my doniesienia, ¿e biblioteki Real musz± byæ zapisywalne dla u¿ytkownika, który korzysta z MPlayera, ale tylko na niektórych systemach. Spróbuj nadaæ im atrybut zapisywalno¶ci, je¿eli napotkasz jakie¶ problemy. Biblioteki DLL QuickTime równie¿ dzia³aj±, ale bêdzisz musia³ je umie¶ciæ w katalogu systemowym Windows (C:\Windows\system\ lub podobnym).

Konsola Cygwin/MinGW jest raczej wolna. Przekierowywanie wyj¶cia albo u¿ywanie opcji -quiet zg³oszono jako poprawiaj±ce wydajno¶æ na niektórych systemach. Bezpo¶rednie renderowanie (-dr) równie¿ mo¿e pomóc. Mo¿esz zapobiec migotaniu OSD, w³±czaj±c podwójne buforowanie opcj± -double. Je¿eli odtwarzanie jest nierówne, spróbuj u¿yæ -autosync 100. Je¿eli którakolwiek z tych opcji Ci pomog³a, mo¿e bêdziesz chcia³ umie¶ciæ j± w swoim pliku konfiguracyjnym.

Sascha Sommer wydaje, od czasu do czasu, oficjalne paczki dla Windowsa, Joey Parrish tworzy nieoficjalne paczki z instalatorem. Poszukaj ich w sekcji Windows na stronie naszych projektów.

6.6.1. Cygwin

Cygwin w wersji wcze¶niejszej ni¿ 1.5.0 nie zawiera inttypes.h. Umie¶æ plik inttypes.h w katalogu

/usr/include/, ¿eby umo¿liwiæ kompilacjê MPlayera.

Pliki nag³ówkowe DirectX musz± byæ rozpakowane do /usr/include/ lub /usr/local/include/.

Instrukcje i pliki potrzebne do kompilacji SDLa dla Cygwin s± dostêpne na stronie libsdl.

Mo¿esz odtwarzaæ VCD, odtwarzaj±c pliki .DAT lub .MPG, które Windows pokazuje na VCD. To dzia³a mniej wiêcej tak (dopasuj literê dysku do Twojego CD-ROMu):

mplayer d:/mpegav/avseq01.dat

mplayer /cygdrive/d/MPEG2/AVSEQ01.MPG

DVD równie¿ dzia³a, podaj literê Twojego DVD-ROMu przez opcjê -dvd-device:

mplayer dvd://<tytu³> -dvd-device '\\.\d:'

6.6.2. MinGW

Zainstalowanie MinGW, który umo¿liwi³by kompilacjê MPlayera by³o zawi³e, ale teraz sk³ada siê tylko z trzech prostych kroków i nied³ugo powinno dzia³aæ "prosto z pude³ka". Zainstaluj MinGW 3.0.0 lub nowszy. Zainstaluj MSYS 1.0.9 lub nowszy i wska¿ systemowi poinstalacyjnemu MSYSa, ¿e MinGW jest zainstalowane.

Je¿eli u¿ywasz MinGW wcze¶niejszego ni¿ 3.1.0, zast±p /mingw/include/sys/types.h tym

types.h.

Rozpakuj pliki nag³ówkowe DirectX do /mingw/include/.

VCD i DVD dzia³aj± prawie tak, jak w Cygwinie (dopasuj literê dysku do Twojego CD-ROMu/DVD-ROMu):

MPlayer - Odtwarzacz filmów dla LINUKSA

6.6.1. Cygwin 98

mplayer d:/mpegav/avseq01.dat

mplayer /d/MPEG2/AVSEQ01.MPG

mplayer dvd://<tytu³> -dvd-device /d/

6.7. Mac OS

"Surowe" ¼ród³a MPlayera obs³uguj± tylko Mac OS X w wersjach 10.2 i wy¿szych. Mo¿esz spróbowaæ umo¿liwiæ obs³ugê starszych wersji Mac OS oraz przys³aæ nam ³aty!

Zmodyfikowane GCC 3.X Apple jest zalecane do kompilacji MPlayera, szczególnie z libavcodec, poniewa¿ ich zmodyfikowane GCC 2.95.x nie obs³uguje poprawnie sk³adni C99.

Mo¿esz pobraæ Aqua GUI dla MPlayera razem z jego skompilowanymi binariami dla Mac OS X ze strony projektu MPlayerOSX.

6.8. HP UX

Martin Gansser opiekuje siê cennym dokumentem HOWTO ("Jak to zrobiæ.." - przypisek t³umacza) na temat budowania MPlayera na HP-UX. Zawiera on nawet dzia³ FAQ!

W ka¿dym b±d¼ razie, nasze "surowe" ¼ród³a MPlayera kompilowa³y siê na HP-UX bez ¿adnych problemów.

6.9. Amiga/MorphOS (zabawki dla zapaleñców)

Nicholas Det at Genesi stworzy³ potê¿ny port MPlayera dla MorphOS. Niestety oparty jest on o seriê 0.90.

Pobierz go z MorphZone:

pakiet binarny MPlayer 0.91 • ¼ród³a MPlayera 0.91 • pakiet binarny MEncodera 0.91 • Rozdzia³ 7. Encoding with MEncoder

Spis tre¶ci

7.1. Encoding 2 or 3-pass MPEG-4 ("DivX") 7.2. Encoding to MPEG format 7.3. Rescaling movies 7.4. Stream copying 7.5. Fixing AVIs with broken index or interleaving

7.5.1. Appending multiple AVI files 7.6. Encoding with the libavcodec codec family 7.7. Encoding from multiple input image files (JPEGs,PNGs or TGAs) 7.8. Extracting DVD subtitles to Vobsub file 7.9. Preserving aspect ratio

MPlayer - Odtwarzacz filmów dla LINUKSA

6.7. Mac OS 99

7.10. Custom inter/intra matrices

For the complete list of available MEncoder options and examples, please see the man page. For a series of hands-on examples and detailed guides on using several encoding parameters, read the encoding-tips that were collected from several mailing list threads on mplayer-users. Search the archives for a wealth of discussions about all aspects of and problems related to encoding with MEncoder.

7.1. Encoding 2 or 3-pass MPEG-4 ("DivX")

2-pass encoding. The name comes from the fact that this method encodes the file twice. The first encoding (dubbed pass) creates some temporary files (*.log) with a size of few megabytes, do not delete them yet (you can delete the AVI). In the second pass, the 2-pass output file is created, using the bitrate data from the temporary files. The resulting file will have much better image quality. If this is the first time you heard about this, you should consult some guides available on the Net.

This example shows how to encode a DVD to a 2-pass MPEG-4 ("DivX") AVI. Just two commands are needed:

rm frameno.avi

remove this file, which can come from a previous 3-pass encoding (it interferes with current one)

mencoder dvd://2 -ovc lavc -lavcopts vcodec=mpeg4:vpass=1 -oac copy -o movie.avi
mencoder dvd://2 -ovc lavc -lavcopts vcodec=mpeg4:vpass=2 -oac copy -o movie.avi

3-pass encoding. This is an extension of 2-pass encoding, where the audio encoding takes place in a separate pass. This method enables estimation of recommended video bitrate in order to fit on a CD. Also, the audio is encoded only once, unlike in 2-pass mode. The schematics:

Remove conflicting temporary file:

rm frameno.avi

1.

First pass:

mencoder file/DVD -ovc frameno -oac mp3lame -lameopts vbr=3 -o frameno.avi

An audio-only avi file will be created, containing only the requested audio stream. Don't forget

-lameopts, if you need to set it. If you were encoding a long movie, MEncoder prints the

recommended bitrate values for 650Mb, 700Mb, and 800Mb destination sizes, after this pass finishes.

2.

Second pass:

mencoder file/DVD -oac copy -ovc lavc -lavcopts vcodec=mpeg4:vpass=1:vbitrate=bitrate

This is the first pass of video encoding. Optionally specify the video bitrate MEncoder printed at the end of the previous pass.

3.

Third pass:

mencoder file/DVD -oac copy -pass 2 \
         -ovc divx4 -divx4opts br=bitrate

This is the second pass of video encoding. Specify the same bitrate as in the previous pass unless you really know what you are doing. In this pass, audio from frameno.avi will be inserted into the

4.

MPlayer - Odtwarzacz filmów dla LINUKSA

7.1. Encoding 2 or 3-pass MPEG-4 ("DivX") 100 destination file...and it's all ready!

Przyk³ad 7.1. Example of 3-pass encoding

rm frameno.avi

remove this file, which can come from a previous 3-pass encoding (it interferes with current one)

mencoder dvd://2 -ovc frameno -o frameno.avi -oac mp3lame -lameopts vbr=3
mencoder dvd://2 -ovc lavc -lavcopts vcodec=mpeg4:vpass=1 -oac copy -o movie.avi
mencoder dvd://2 -ovc lavc -lavcopts vcodec=mpeg4:vpass=2 -oac copy -o movie.avi

7.2. Encoding to MPEG format

MEncoder can create MPEG (MPEG-PS) format output files. It's probably useful only with libavcodec's mpeg1video codec, because players - except MPlayer - expect MPEG1 video, and MPEG1 layer 2 (MP2) audio streams in MPEG files.

This feature is not very useful right now, aside that it probably has many bugs, but the more importantly because MEncoder currently cannot encode MPEG1 layer 2 (MP2) audio, which all other players expect in MPEG files.

To change MEncoder's output file format, use the -of mpeg option.

Example:

mencoder -of mpeg -ovc lavc -lavcopts vcodec=mpeg1video -oac copy other options media.avi -o output.mpg

7.3. Rescaling movies

Often the need to resize movie images' size emerges. Its reasons can be many: decreasing file size, network bandwidth,etc. Most people even do rescaling when converting DVDs or SVCDs to DivX AVI. This is bad. Instead of even you doing so, read the Preserving aspect ratio section.

The scaling process is handled by the scale video filter: -vf scale=width:height. Its quality can be set with the -sws option. If it's not specified, MEncoder will use 0: fast bilinear.

Usage:

mencoder input.mpg -ovc lavc -lavcopts vcodec=mpeg4 -vf scale=640:480-o output.avi

7.4. Stream copying

MEncoder can handle input streams in two ways: encode or copy them. This section is about copying.

Video stream (option -ovc copy): nice stuff can be done :) Like, putting (not converting!) FLI or VIVO or MPEG1 video into an AVI file! Of course only MPlayer can play such files :) And it probably has no real life value at all. Rationally: video stream copying can be useful for example when only the audio stream has to be encoded (like, uncompressed PCM to MP3).

•

MPlayer - Odtwarzacz filmów dla LINUKSA

7.2. Encoding to MPEG format 101

Audio stream (option -oac copy): straightforward. It is possible to take an external audio file (MP3, WAV) and mux it into the output stream. Use the -audiofile filename option for this. • 7.5. Fixing AVIs with broken index or interleaving

Easiest thing. We simply copy the video and audio streams, and MEncoder generates the index. Of course this cannot fix possible bugs in the video and/or audio streams. It also fixes files with broken interleaving, thus the

-ni option won't be needed for them anymore.

Command:

mencoder -idx input.avi -ovc copy -oac copy -o output.avi

7.5.1. Appending multiple AVI files

As a side-effect, the broken AVI fixer function enables MEncoder to append 2 (or more) AVI files:

Command:

cat 1.avi 2.avi | mencoder -noidx -ovc copy -oac copy -o output.avi -

Notatka

This expects 1.avi and 2.avi to use the same codecs, resolution, stream rate etc, and at least 1.avi must not be broken. You may need to fix your input AVI files first, as described above.

7.6. Encoding with the libavcodec codec family

libavcodec provides simple encoding to a lot of interesting video and audio formats (currently its audio codecs are unsupported). You can encode to the following codecs (more or less up to date):

Codec name Description mjpeg Motion JPEG ljpeg Lossless JPEG h263 H263 h263p H263 Plus

mpeg4 ISO standard MPEG-4 (DivX 5, XVID compatible)

msmpeg4 pre-standard MPEG-4 variant by MS, v3 (aka DivX3)

msmpeg4v2 pre-standard MPEG-4 by MS, v2 (used in old asf files) wmv1 Windows Media Video, version 1 (aka WMV7) wmv2 Windows Media Video, version 2 (aka WMV8) rv10 an old RealVideo codec mpeg1video MPEG1 video mpeg2video MPEG2 video

MPlayer - Odtwarzacz filmów dla LINUKSA

7.5. Fixing AVIs with broken index or interleaving 102 huffyuv lossless compression asv1 ASUS Video v1 asv2 ASUS Video v2 ffv1 FFmpeg's lossless video codec The first column contains the codec names that should be passed after the vcodec config, like: -lavcopts

vcodec=msmpeg4

An example, with MJPEG compression:

mencoder dvd://2 -o title2.avi -ovc lavc -lavcopts vcodec=mjpeg -oac copy

7.7. Encoding from multiple input image files (JPEGs,PNGs or TGAs)

MEncoder is capable of creating movies from one or more JPEG, PNG or TGA files. With simple framecopy it can create MJPEG (Motion JPEG), MPNG (Motion PNG) or MTGA (Motion TGA) files.

Explanation of the process:

MEncoder decodes the input image(s) with libjpeg (when decoding PNGs, it will use libpng). 1. MEncoder then feeds the decoded image to the chosen video compressor (DivX4, Xvid, ffmpeg msmpeg4, etc.). 2.

Examples. The explanation of the -mf option can be found below in the man page.

Creating a DivX4 file from all the JPEG files in the current dir:

mencoder -mf on:w=800:h=600:fps=25 -ovc divx4 -o output.avi \*.jpg

Creating a DivX4 file from some JPEG files in the current dir:

mencoder -mf on:w=800:h=600:fps=25 -ovc divx4 -o output.avi frame001.jpg,frame002.jpg

Creating a Motion JPEG (MJPEG) file from all the JPEG files in the current dir:

mencoder -mf on:w=800:h=600:fps=25 -ovc copy -o output.avi \*.jpg

Creating an uncompressed file from all the PNG files in the current dir:

mencoder -mf on:w=800:h=600:fps=25:type=png -ovc raw -o output.avi \*.png

Notatka

Width must be integer multiple of 4, it's a limitation of the RAW RGB AVI format.

Creating a Motion PNG (MPNG) file from all the PNG files in the current dir:

mencoder -mf on:w=800:h=600:fps=25:type=png -ovc copy -o output.avi \*.png

Creating a Motion TGA (MTGA) file from all the TGA files in the current dir:

MPlayer - Odtwarzacz filmów dla LINUKSA

7.7. Encoding from multiple input image files (JPEGs,PNGs or TGAs) 103

mencoder -mf on:w=800:h=600:fps=25:type=tga -ovc copy -o output.avi \*.tga

7.8. Extracting DVD subtitles to Vobsub file

MEncoder is capable of extracting subtitles from a DVD into Vobsub formatted files. They consist of a pair of files ending in .idx and .sub and are usually packaged in a single .rar archive. MPlayer can play these with the -vobsub and -vobsubid options.

You specify the basename (i.e without the .idx or .sub extension) of the output files with -vobsubout and the index for this subtitle in the resulting files with -vobsuboutindex.

If the input is not from a DVD you should use -ifo to indicate the .ifo file needed to construct the resulting .idx file.

If the input is not from a DVD and you do not have the .ifo file you will need to use the -vobsubid option to let it know what language id to put in the .idx file.

Each run will append the running subtitle if the .idx and .sub files already exist. So you should remove any before starting.

Przyk³ad 7.2. Copying two subtitles from a DVD while doing 3-pass encoding

rm subtitles.idx subtitles.sub
mencoder dvd://1 -vobsubout subtitles -vobsuboutindex 0 -sid 2 -o frameno.avi -ovc frameno
mencoder dvd://1 -oac copy -ovc divx4 -pass 1
mencoder dvd://1 -oac copy -ovc divx4 -pass 2 -vobsubout subtitles -vobsuboutindex 1 -sid 5

Przyk³ad 7.3. Copying a french subtitle from an MPEG file

rm subtitles.idx subtitles.sub
mencoder movie.mpg -ifo movie.ifo -vobsubout subtitles -vobsuboutindex 0 -vobsuboutid fr -sid 1

7.9. Preserving aspect ratio

DVDs and SVCDs (i.e. MPEG1/2) files contain an aspect ratio value, which describes how the player should scale the video stream, so humans won't have egg heads (ex.: 480x480 + 4:3 = 640x480). However when encoding to AVI (DivX) files, you have be aware that AVI headers don't store this value. Rescaling the movie is disgusting and time consuming, there has to be a better way!

There is

MPEG4 has an unique feature: the video stream can contain its needed aspect ratio. Yes, just like MPEG1/2 (DVD, SVCD) and H263 files. Regretfully, there are no video players outside which support this attribute of MPEG4, except MPlayer.

This feature can be used only with libavcodec's mpeg4 codec. Keep in mind: although MPlayer will correctly play the created file, other players will use the wrong aspect ratio.

You seriously should crop the black bands over and below the movie image. See the man page for the usage of the cropdetect and crop filters.

MPlayer - Odtwarzacz filmów dla LINUKSA

7.8. Extracting DVD subtitles to Vobsub file 104

Usage

mencoder sample-svcd.mpg -ovc lavc -lavcopts vcodec=mpeg4:autoaspect -vf crop=714:548:0:14 -oac copy -o output.avi

7.10. Custom inter/intra matrices

With this feature of libavcodec you are able to set custom inter (I-frames/key frames) and intra (P-frames/predicted frames) matrices. It is supported by many of the codecs: mpeg1video and

mpeg2video are reported as working.

A typical usage of this feature is to set the matrices preferred by the KVCD specifications.

The KVCD "Notch" Quantization Matrix:

Intra:

 8  9 12 22 26 27 29 34
 9 10 14 26 27 29 34 37
12 14 18 27 29 34 37 38
22 26 27 31 36 37 38 40
26 27 29 36 39 38 40 48
27 29 34 37 38 40 48 58
29 34 37 38 40 48 58 69
34 37 38 40 48 58 69 79

Inter:

16 18 20 22 24 26 28 30
18 20 22 24 26 28 30 32
20 22 24 26 28 30 32 34
22 24 26 30 32 32 34 36
24 26 28 32 34 34 36 38
26 28 30 32 34 36 38 40
28 30 32 34 36 38 42 42
30 32 34 36 38 40 42 44

Usage:

$ mencoder input.avi -o output.avi -oac copy -ovc lavc -lavcopts inter_matrix=...:intra_matrix=...

$ mencoder input.avi -ovc lavc -lavcopts
vcodec=mpeg2video:intra_matrix=8,9,12,22,26,27,29,34,9,10,14,26,27,29,34,37,
12,14,18,27,29,34,37,38,22,26,27,31,36,37,38,40,26,27,29,36,39,38,40,48,27,
29,34,37,38,40,48,58,29,34,37,38,40,48,58,69,34,37,38,40,48,58,69,79
:inter_matrix=16,18,20,22,24,26,28,30,18,20,22,24,26,28,30,32,20,22,24,26,
28,30,32,34,22,24,26,30,32,32,34,36,24,26,28,32,34,34,36,38,26,28,30,32,34,
36,38,40,28,30,32,34,36,38,42,42,30,32,34,36,38,40,42,44 -oac copy -o svcd.mpg

Dodatek A. Listy mailingowe

Istniej± publiczne listy dyskusyjne o MPlayerze. Je¶li nie jest to wyra¼nie zaznaczone, jêzykiem obowi±zuj±cym na nich jest angielski. Proszê nie przysy³aæ wiadomo¶ci w innym jêzyku, ani w formacie HTML! Limit na wielko¶æ wiadomo¶ci wynosi 80KB. Wiêksze dane nale¿y ulokowaæ w miejscu przeznaczonym do publicznego ¶ci±gania. ¯eby siê zapisaæ, nale¿y klikn±æ na poni¿szych odno¶nikach. Na

MPlayer - Odtwarzacz filmów dla LINUKSA

7.10. Custom inter/intra matrices 105 tych listach obowi±zuj± te same zasady pisania i cytowania, co w Usenecie. Prosimy o ich przestrzeganie, u³atwia to ¿ycie tym, którzy czytaj± Wasze maile. Zasady pisania dostêpne s± pod adresami HOWTO edit messages lub (dla niecierpliwych) Quoting HOWTO.

Lista og³oszeñ MPlayera: http://mplayerhq.hu/mailman/listinfo/mplayer-announce Lista na og³oszenia MPlayera. Wysy³ane s± na ni± informacje o nowych mo¿liwo¶ciach. • Lista deweloperów MPlayera: http://mplayerhq.hu/mailman/listinfo/mplayer-dev-eng To lista dotycz±ca rozwoju MPlayera! Jest to miejsce na rozmowy o zmianach interfejsu/API, nowych bibliotekach, optymalizacji kodu i zmianach w konfiguracji. Aby utrzymaæ ma³y ruch na li¶cie, mo¿na przysy³aæ tu ³atki, ale nie zg³oszenia b³êdów, pytania u¿ytkowników, pro¶by o nowe mo¿liwo¶ci czy flame'y.

•

Lista dokumentacji MPlayera: http://mplayerhq.hu/mailman/listinfo/mplayer-docs To lista na dyskusje o dokumentacji MPlayera i jej t³umaczeniu. Przesy³ane s± te¿ na ni± logi CVS dotycz±ce dokumentacji i strony domowej. •

Lista u¿ytkowników MPlayera: http://mplayerhq.hu/mailman/listinfo/mplayer-users Mo¿na tu przesy³aæ zg³oszenia b³êdów po przeczytaniu znanych b³êdów i opisu zg³aszania b³êdów ♦ Mo¿na tu przesy³aæ pro¶by o nowe mo¿liwo¶ci (po przeczytaniu ca³ej dokumentacji). ♦ Mo¿na tu przesy³aæ pytania dotycz±ce u¿ytkowania (po przeczytaniu ca³ej dokumentacji). ♦

•

Lista wêgierskich u¿ytkowników MPlayera:

http://mplayerhq.hu/mailman/listinfo/mplayer-felhasznalok

Lista w jêzyku wêgierskim ♦ Temat? Jeszcze zobaczymy... Na razie g³ównie flame'y i pytania typu RTFM :( ♦

•

Lista u¿ytkowników MPlayera i Matroxa G200/G400/G450/G550:

http://mplayerhq.hu/mailman/listinfo/mplayer-matrox Pytania zwi±zane z Matroxem, takie jak pytania o mga_vid ♦ oficjalne sterowniki beta Matroxa (dla X 4.x.x) ♦ pytania o matroxfb-TVout ♦

•

Lista u¿ytkowników MPlayera i kart DVB: http://mplayerhq.hu/mailman/listinfo/mplayer-dvb Sprawy zwi±zane ze sprzêtowym dekoderem zwanym DVB (nie DXR3!). • Log CVSu MPlayera: http://mplayerhq.hu/mailman/listinfo/mplayer-cvslog Na tê listê wysy³ane s± automatycznie wszystkie zmiany w kodzie MPlayera. Dozwolone s± tu tylko pytania o te zmiany (pro¶by o wyja¶nienie, dlaczego dana zmiana jest konieczna, lepsze rozwi±zania, mo¿liwe problemy zwi±zane z t± zmian±).

•

Lista przenoszenia MPlayera do ¶rodowiska Cygwin:

http://mplayerhq.hu/mailman/listinfo/mplayer-cygwin Lista po¶wiêcona dyskusji o przenoszeniu MPlayera do ¶rodowiska Cygwin i MinGW. •

Lista przenoszenia MPlayera do ¶rodowiska OS/2: http://mplayerhq.hu/mailman/listinfo/mplayer-os2 Lista po¶wiêcona dyskusji o przenoszeniu MPlayera do ¶rodowiska OS/2. • Lista twórców i t³umaczy MPlayer Weekly News:

http://mplayerhq.hu/mailman/listinfo/mplayer-mwn Lista po¶wiêcona dyskusjom o MPlayer Weekly News. •

Notatka

Wyszukiwanie w archiwach list jest dostêpne pod adresem http://www.mplayerhq.hu/cgi-bin/htsearch.

MPlayer - Odtwarzacz filmów dla LINUKSA

Dodatek B. Jak zg³aszaæ b³êdy

Spis tre¶ci

B.1. Jak poprawiaæ b³êdy B.2. Jak zg³aszaæ b³êdy B.3. Gdzie zg³aszaæ b³êdy B.4. Co zg³aszaæ

B.4.1. Informacja o systemie operacyjnym B.4.2. Sprzêt i sterowniki B.4.3. Problemy z konfiguracj± B.4.4. Problemy z kompilacj± B.4.5. Problemy z odtwarzaniem B.4.6. Awarie programu (ang. Crashes) B.4.6.1. Jak otrzymaæ informacjê o awarii B.4.6.2. Jak wyci±gn±æ sensowne informacjê ze zrzutu core (ang. core dump) B.5. Wiem co robiê...

Dobre raporty b³êdów stanowi± bardzo istotny wk³ad w rozwój ka¿dego projektu. Jednak tak jak pisanie dobrych programów wymaga sporo pracy, tak dobre zg³oszenia problemów wymagaj± trochê wysi³ku. Prosimy wzi±æ pod uwagê to, ¿e wiêkszo¶æ deweloperów jest bardzo zajêta i odbiera nieprzyzwoit± wrêcz ilo¶æ listów. Wsparcie ze strony u¿ytkownika jest naprawdê wa¿ne w procesie ulepszania MPlayera. Nale¿y jednak pamiêtaæ, ¿e trzeba dostarczyæ wszystkie informacjê o które poprosimy i postêpowaæ dok³adnie wed³ug instrukcji zawartej w tym dokumencie.

B.1. Jak poprawiaæ b³êdy

Je¿eli uwa¿asz, ¿e posiadasz wystarczaj±ce umiejêtno¶ci, namawiamy Ciê do samodzielnego poprawiania b³êdów. A mo¿e ju¿ to zrobi³e¶? Przeczytaj ten krótki dokument, ¿eby dowiedzieæ siê w jaki sposób dodaæ swoj± ³atê do ¼róde³ MPlayera. Je¿eli bêdziesz mia³ jakie¶ pytania, pomog± Ci ludzie z listy mplayer-dev-eng (tylko w jêzyku angielskim -przyp. t³umacza).

B.2. Jak zg³aszaæ b³êdy

Po pierwsze sprawd¼ najnowsz± wersjê CVS MPlayera, poniewa¿ dany b³±d mo¿e byæ ju¿ w niej naprawiony. Rozwój MPlayera przebiega naprawdê szybko, wiêkszo¶æ problemów wystêpuj±cych w oficjalnych wydaniach jest zg³aszana w ci±gu kilku dni albo nawet godzin. Dlatego te¿ prosimy u¿ywaæ tylko wersji z CVSa do zg³aszania b³êdów. Dotyczy to g³ównie pakietów binarnych MPlayera. Instrukcje dotycz±ce CVSa znajduj± siê na dole tej strony lub w pliku README. Je¿eli problem dalej wystêpuje prosimy sprawdziæ listê znanych b³êdów i resztê dokumentacji. Je¿eli problem nie jest znany lub rozwi±zany przez nasz± dokumentacjê prosimy zg³osiæ b³±d.

Nie nale¿y wysy³aæ zg³oszeñ do deweloperów. MPlayer jest dzie³em du¿ej grupy, wiêc wiêcej osób mo¿e byæ zainteresowanych tym problemem. Czasami inni u¿ytkownicy spotkali siê ju¿ z danym problemem i wiedz± jak go rozwi±zaæ nawet je¿eli jest to b³±d w kodzie MPlayera.

Prosimy opisywaæ problem tak dok³adnie, jak to tylko mo¿liwe. Nale¿y sprawdziæ w jakich dok³adnie okoliczno¶ciach pojawia siê b³±d. Czy wystêpuje on tylko w okre¶lonych sytuacjach? Czy ma zwi±zek z konkretnym plikiem lub typem plików? Czy dotyczy tylko danego kodeka, czy te¿ jest niezale¿ny od

MPlayer - Odtwarzacz filmów dla LINUKSA

Dodatek B. Jak zg³aszaæ b³êdy 107 kodeków? Czy mo¿esz go odtworzyæ z ka¿dym wyj¶ciem video? Im wiêcej informacji dostarczysz, tym wiêksze s± szanse na rozwi±zanie zg³oszonego problemu. Nie nale¿y równie¿ zapominaæ o do³±czeniu warto¶ciowych informacji wymienionych poni¿ej. W przeciwnym wypadku nie bêdziemy w stanie prawid³owo zdiagnozowaæ zg³oszonego problemu.

Doskona³ym i dobrze napisanym przewodnikiem dotycz±cym zadawania pytañ jest dokument "Jak zadawaæ pytania w m±dry sposób" napisany przez Erica S. Raymonda. Istnieje tak¿e inny dokumentem tego typu zatytu³owany Jak efektywnie zg³aszaæ b³êdy stworzony przez Simona Tathama (Polskie t³umaczenie tego dokumentu mo¿na znale¼æ tutaj -przyp. t³um.). Je¶li bêdziesz postêpowa³ zgodnie z tymi przewodnikami, powiniene¶ uzyskaæ pomoc. Prosimy jednak pamiêtaæ, ¿e ¶ledzimy listê jako ochotnicy po¶wiêcaj±c nasz wolny czas. Jeste¶my bardzo zajêci i nie potrafimy zagwarantowaæ, ¿e pomo¿emy rozwi±zaæ zg³oszony problem, ani nawet tego, ¿e odpowiemy na Twoje zg³oszenie.

B.3. Gdzie zg³aszaæ b³êdy

Zapisz siê na listê mplayer-users: http://mplayerhq.hu/mailman/listinfo/mplayer-users i wy¶lij swoje zg³oszenie b³êdu na: mailto:mplayer-users@mplayerhq.hu

Jêzykiem obowi±zuj±cym na tej li¶cie jest angielski. Prosimy trzymaæ siê zasad standardowej Netykiety (Polsk± wersjê netykiety mo¿na przeczytaæ np. tutaj -przyp. t³um.) i nie wysy³aæ listów w HTMLu na ¿adn± z naszych list. W przeciwnym wypadku zostaniesz zignorowany lub wyrzucony z listy. Je¿eli nie wiesz czym jest list w HTMLu albo dlaczego jest on z³y, przeczytaj ten ¶wietny dokument (znów tylko po angielsku -przyp. t³um.). Wyja¶nia on wszystkie szczegó³y i zawiera instrukcje wy³±czania HTMLa. Zauwa¿ równie¿, ¿e nie wysy³amy kopii listów do u¿ytkowników, wiêc dobrym pomys³em jest zapisanie siê na listê w celu uzyskania odpowiedzi.

B.4. Co zg³aszaæ

Mo¿esz potrzebowaæ do³±czyæ log, konfiguracjê lub przyk³adowy plik w twoim zg³oszeniu b³êdu. Je¿eli który¶ z nich ma du¿y rozmiar, lepiej za³adowaæ go na nasz serwer FTP w skompresowanej postaci (gzip i bzip2 s± preferowanymi formatami) i za³±czyæ tylko ¶cie¿kê i nazwê pliku do zg³oszenia b³êdu. Nasza lista ma ustawiony limit rozmiaru ka¿dej wiadomo¶ci na 80k. Je¿eli potrzebujesz wys³aæ co¶ wiêkszego, musisz to skompresowaæ albo za³adowaæ na serwer.

B.4.1. Informacja o systemie operacyjnym

Nazwa Twojej dystrybucji Linuksa albo system operacyjny. Np.:

Red Hat 7.1 ♦ Slackware 7.0 + pakiety rozwojowe z 7.1 ... ♦ •

wersja j±dra (kernela):

uname -a

•

wersja biblioteki libc:

ls -l /lib/libc[.-]*

•

wersja gcc i ld:

gcc -v
ld -v

•

MPlayer - Odtwarzacz filmów dla LINUKSA

B.3. Gdzie zg³aszaæ b³êdy 108 wersja binutils:

as --version

•

Je¿eli masz problem z trybem pe³noekranowym:

Menad¿er okien i wersja ♦ •

Je¿eli masz problem z XVIDIXem:

g³êbia barw Xów (colour depth):

xdpyinfo | grep "depth of root"

♦ •

Je¿eli tylko GUI zawiera b³êdy:

wersja GTK ♦ wersja GLIB ♦ wersja libpng ♦ Sytuacja w której pojawia siê b³±d GUI ♦

•

B.4.2. Sprzêt i sterowniki

informacje o procesorze (CPU) (to dzia³a tylko pod Linuksem):

cat /proc/cpuinfo

•

Producent karty graficznej i model. Np.:

ASUS V3800U chip: nVidia TNT2 Ultra pro 32MB SDRAM ♦ Matrox G400 DH 32MB SGRAM ♦

•

Typ sterownika video i wersja, np:

wbudowane sterowniki X ♦ nVidia 0.9.623 ♦ Utah-GLX CVS 2001-02-17 ♦ DRI z X 4.0.3 ♦

•

Typ karty d¼wiêkowej i sterownik, np:

Creative SBLive! Gold ze sterownikiem OSS z oss.creative.com ♦ Creative SB16 ze sterownikiem OSS z kernela ♦ GUS PnP z emulacj± ALSA OSS ♦

•

Je¿eli masz w±tpliwo¶ci, za³±cz wyj¶cie lspci -vv systemu Linux. • B.4.3. Problemy z konfiguracj±

Je¿eli dostajesz b³±d podczas uruchamiania ./configure albo automatyczne wykrywanie czego¶ zawiedzie, przeczytaj configure.log. Mo¿liwe, ¿e znajdziesz tam odpowied¼, na przyk³ad kilka po³±czonych wersji tej samej biblioteki w Twoim systemie albo ¿e zapomnia³e¶ zainstalowaæ pakietów rozwojowych (tych z przyrostkiem -dev albo -devel). Je¿eli wydaje Ci siê, ¿e istnieje jednak b³±d, za³±cz configure.log w twoim raporcie.

B.4.4. Problemy z kompilacj±

Prosimy za³±czyæ nastêpuj±ce pliki:

MPlayer - Odtwarzacz filmów dla LINUKSA

B.4.2. Sprzêt i sterowniki 109 config.h • config.mak • Tylko je¿eli kompilacja siê nie powiedzie w którym¶ z tych katalogów, za³±cz nastêpuj±ce pliki:

Gui/config.mak • libvo/config.mak • libao2/config.mak • B.4.5. Problemy z odtwarzaniem

Prosimy za³±czyæ wyj¶cie MPlayera w trybie gadatliwym na poziomie pierwszym (opcja -v -przyp. t³um.), ale pamiêtaj±c o nie skracaniu wyniku polecenia podczas kopiowania go do Twojego listu. Developerzy potrzebuj± wszystkich informacji do prawid³owego zdiagnozowania problemu. Mo¿esz przekierowaæ wyj¶cie bezpo¶rednio do pliku w ten sposób:

mplayer -v opcje nazwa_pliku > mplayer.log 2>&1

Je¿eli Twój problem jest specyficzny dla jednego albo wielu plików, za³aduj winowajcê(ów) na: ftp://mplayerhq.hu/MPlayer/incoming/

Za³aduj tak¿e ma³y plik tekstowy nazwany tak samo jak Twój plik, ale z rozszerzeniem .txt. Opisz w nim problem, który masz z zawartym plikiem i za³±cz swój adres email oraz wyj¶cie MPlayera w trybie gadatliwym na poziomie pierwszym. Zazwyczaj pierwsze 1-5 MB pliku jest wystarczaj±ce do odtworzenia problemu, ale ¿eby byæ pewnym prosimy wykonaæ:

dd if=twój_plik of=ma³y_plik bs=1024k count=5

To polecenie we¼mie pierwsze piêæ megabajtów 'twojego_pliku' i zapisze je do 'ma³ego_pliku'. Nastêpnie spróbuj odtworzyæ ma³y plik i je¶li b³±d wci±¿ siê pojawia plik ten jest dla nas wystarczaj±cy. Prosimy w ¿adnym wypadku nie wysy³aæ plików poprzez pocztê elektroniczn±! Za³aduj je na serwer FTP i wy¶lij tylko ¶cie¿kê/nazwê pliku. Je¿eli plik jest dostêpny w sieci, wy¶lij dok³adny adres pod którym jest on dostêpny.

B.4.6. Awarie programu (ang. Crashes)

Musisz uruchomiæ MPlayera wewn±trz gdb i wys³aæ nam kompletne wyj¶cie albo je¿eli posiadasz zrzut

core (ang. core dump) utworzony w wyniku awarii, wyci±gn±æ z niego u¿yteczne informacje. Oto jak to

zrobiæ:

B.4.6.1. Jak otrzymaæ informacjê o awarii

Przekompiluj MPlayera z opcj± debugowania kodu:

./configure --enable-debug=3
make

i uruchom MPlayera u¿ywaj±c gdb:

gdb ./mplayer

Jeste¶ teraz wewn±trz gdb. Wpisz:

MPlayer - Odtwarzacz filmów dla LINUKSA

B.4.5. Problemy z odtwarzaniem 110

run -v opcje-mplayera
nazwa_pliku

i odtwórz swoj± awariê. Gdy tylko to zrobisz, gdb przeniesie ciê z powrotem do linii poleceñ, gdzie nale¿y wpisaæ

bt
disass $pc-32 $pc+32
info all-registers

B.4.6.2. Jak wyci±gn±æ sensowne informacjê ze zrzutu core (ang. core dump)

Utwórz nastêpuj±cy plik poleceñ:

bt
disass $pc-32 $pc+32
info all-registers

A nastêpnie uruchomiæ nastêpuj±ce polecenie:

gdb mplayer --core=core -batch --command=command_file > mplayer.bug

B.5. Wiem co robiê...

Je¿eli utworzy³e¶ w³a¶ciwy raport b³êdu kieruj±c siê powy¿szymi wskazówkami i jeste¶ pewien ¿e to b³±d MPlayera, nie kompilatora albo uszkodzonego pliku, przeczyta³e¶ dokumentacjê i nie mo¿esz znale¼æ rozwi±zania, Twoje sterowniki d¼wiêku s± w porz±dku, mo¿esz chcieæ zapisaæ siê na listê mplayer-advusers (tylko po angielsku -przyp. t³um.) i wys³aæ tam swoje zg³oszenie b³êdu, aby uzyskaæ lepsz± i szybsz± odpowied¼.

Wiedz, ¿e je¶li zadasz trywialne pytanie albo odpowied¼ na nie znajduje siê w podrêczniku (ang. man), zamiast dostaæ odpowied¼ zostaniesz zignorowany albo obrzucony wyzwiskami. Dlatego te¿ nie obra¿aj nas i zapisz siê na listê -advusers tylko je¿eli naprawdê wiesz co robisz i czujesz siê zaawansowanym u¿ytkownikiem lub deweloperem. Je¿eli spe³niasz te kryteria, nie powinno Ci sprawiæ problemu znalezienie sposobu zapisania siê na listê (pamiêtaj, ¿e musisz biegle znaæ j. angielski -przyp. t³um.)

Dodatek C. Znane b³êdy

Spis tre¶ci

C.1. Specjalne systemowe/specyficzne dla procesora b³êdy/problemy C.2. Ró¿ne problemy z synchronizacj± A-V i d¼wiêkiem

C.2.1. Ogólne opó¼nienie audio lub "d³awi±cy siê" d¼wiêk (wystêpuje przy wszystkich lub wielu plikach) C.2.2. Opó¼nienia/desynchronizacja d¼wiêku specyficzne dla jednego lub kilku plików C.2.3. Zupe³ny brak d¼wiêku C.2.4. Zupe³ny brak obrazu (jedynie puste, szare lub zielone okno) C.2.5. Problemy z wyj¶ciem video

MPlayer - Odtwarzacz filmów dla LINUKSA

B.4.6. Awarie programu (ang. Crashes) 111

C.1. Specjalne systemowe/specyficzne dla procesora b³êdy/problemy

SIGILL (sygna³ 4) na P3 przy j±drze 2.2.x:

Problem: j±dro 2.2.x nie ma prawid³owej (dzia³aj±cej) obs³ugi SSE Rozwi±zanie: aktualizacja j±dra do 2.4.x Obej¶cie: ./configure --disable-sse

•

Ogólny SIGILL (sygna³ 4):

Problem: skompilowa³e¶ i próbowa³e¶ uruchomiæ MPlayera na dwóch ró¿nych maszynach (np. skompilowa³e¶ na P3, a próbowa³e¶ uruchomiæ na Celeronie) Rozwi±zanie: kompiluj MPlayera na tej samej maszynie, na której chcesz go u¿ywaæ! Obej¶cie: polecenia ./configure --disable-sse itp.

•

"Niespójno¶æ wewnêtrznego bufora" ("Internal buffer inconsistency") w trakcie dzia³ania MEncodera:

Problem: znany problem przy lame < 3.90 skompilowanym za pomoc± GCC 2.96 lub 3.x. Rozwi±zanie: u¿ywaj lame'a >=3.90.

Obej¶cie: skompiluj lame za pomoc± GCC 2.95.x i usuñ ju¿ zainstalowane pakiety lame'a, gdy¿ mog³y one zostaæ skompilowane za pomoc± GCC 2.96.

•

Zepsuty d¼wiêk MP2/MP3 na PPC:

Problem: znany b³±d z³ej kompilacji kodu przez GCC dla platformy PPC, na razie bez rozwi±zania. Obej¶cie: u¿yj (powolnego) dekodera MP1/MP2/MP3 z FFmpeg (-ac ffmpeg)

•

Sygna³ 11 w libmpeg2, przy skalowaniu i kodowaniu: Problem: znany b³±d MMX w GCC 2.95.2 MMX. Rozwi±zanie: aktualizacja GCC do 2.95.3.

•

C.2. Ró¿ne problemy z synchronizacj± A-V i d¼wiêkiem

C.2.1. Ogólne opó¼nienie audio lub "d³awi±cy siê" d¼wiêk (wystêpuje przy wszystkich lub wielu plikach)

najczê¶ciej: zepsuty sterownik d¼wiêku! - spróbuj u¿yæ innych sterowników, np. emulacji OSS ALSY 0.9 za pomoc± opcji -ao oss. Spróbuj tak¿e -ao sdl. Opcje te czasem pomagaj±. Je¶li Twój plik odtwarza siê bez problemów z opcj± -nosound, to mo¿esz byæ pewien, ¿e to wina karty d¼wiêkowej lub jej sterownika.

•

problemy z buforem audio (¼le wykryty rozmiar bufora) •

MPlayer - Odtwarzacz filmów dla LINUKSA

C.1. Specjalne systemowe/specyficzne dla procesora b³êdy/problemy 112

Obej¶cie: opcja MPlayera -abs problemy z czêstotliwo¶ci± próbkowania - byæ mo¿e Twoja karta nie obs³uguje czêstotliwo¶ci próbkowania u¿ytych w Twoich plikach - spróbuj wtyczki do zmiany rozdzielczo¶ci d¼wiêku (-af

resample=...)

•

powolna maszyna (procesor lub karta graficzna) spróbuj opcji -vo null, je¶li odtwarza dobrze, oznacza to, ¿e masz zbyt woln± kartê graficzn± lub jej sterownik Obej¶cie: kup szybsz± kartê lub poczytaj tê dokumentacjê by dowiedzieæ siê jak przyspieszyæ odtwarzanie Spróbuj równie¿ opcji-framedrop

•

C.2.2. Opó¼nienia/desynchronizacja d¼wiêku specyficzne dla jednego lub kilku plików

z³y plik Obej¶cia:

opcje -ni lub -nobps (dla plików bez przeplotu lub uszkodzonych) i/lub ♦

opcja -mc 0 (wymagana dla plików ze z³ym przeplotem d¼wiêku VBR) i/lub ♦

opcja -delay lub klawisze +/- w trakcie odtwarzania do regulacji opó¼nienia ♦ Je¶li ¿adne z wymienionych rozwi±zañ nie przynosz± efektu, przy¶lij nam plik, a my to sprawdzimy (i naprawimy).

•

Twoja karta d¼wiêkowa nie obs³uguje próbkowania 48kHz Obej¶cie: kup lepsz± kartê... lub spróbuj zmniejszyæ liczbê klatek na sekundê o 10% (u¿ywaj±c opcji

-fps 27 dla filmu o 30 klatkach na sekundê) lub u¿yj wtyczki do zmiany rozdzielczo¶ci d¼wiêku

•

powolna maszyna (je¶li A-V nie jest w okolicach 0 i ostatnia liczba w statusie zwiêksza siê) Obej¶cie: opcja -framedrop •

C.2.3. Zupe³ny brak d¼wiêku

Twój plik u¿ywa nieobs³ugiwanego kodeka audio Obej¶cie: poczytaj dokumentacjê i pomó¿ nam dodaæ jego obs³ugê •

C.2.4. Zupe³ny brak obrazu (jedynie puste, szare lub zielone okno)

Twój plik u¿ywa nieobs³ugiwanego kodeka video •

MPlayer - Odtwarzacz filmów dla LINUKSA

C.2.2. Opó¼nienia/desynchronizacja d¼wiêku specyficzne dla jednego lub kilku plików 113

Obej¶cie: poczytaj dokumentacjê i pomó¿ nam dodaæ jego obs³ugê automatycznie wybrany kodek nie potrafi dekodowaæ pliku, spróbuj u¿yæ innego za pomoc± opcji

-vc lub -vfm

• próbujesz odtwarzaæ plik DivX 3.x za pomoc± kodeka OpenDivX lub XviD (opcja -vc odivx) - zainstaluj Divx4Linux i przekompiluj odtwarzacz • C.2.5. Problemy z wyj¶ciem video

Pierwsza uwaga: opcje -fs -vm i -zoom s± jedynie zaleceniami, nieobs³ugiwanymi (jeszcze) przez wszystkie sterowniki. Nie jest to wiêc b³±d, je¶li nie dzia³aj±. Tylko niektóre sterowniki obs³uguj± skalowanie/powiêkszanie i nie oczekuj tego od x11 lub dga.

Migotanie OSD/napisów.

sterownik x11: przykro nam, ale nie da siê tego teraz naprawiæ • sterownik xv: u¿yj opcji -double • Zielony obraz przy u¿yciu mga_vid (-vo mga / -vo xmga).

mga_vid ¼le wykry³ ilo¶æ pamiêci RAM na Twojej karcie, prze³aduj go u¿ywaj±c opcji

mga_ram_size.

• Dodatek D. Format skórki MPlayera

Spis tre¶ci

D.1. Wstêp

D.1.1. Katalogi D.1.2. Formaty obrazków D.1.3. Sk³adniki skórki D.1.4. Pliki D.2. Plik skin

D.2.1. Okno g³ówne i panel odtwarzania D.2.2. Okno ekranu D.2.3. Menu skórki D.3. Czcionki

D.3.1. Znaki specjalne (symbole) D.4. Sygna³y GUI

Celem tego dokumentu jest opisanie formatu skórki MPlayera. Informacje zawarte tutaj mog± byæ niedok³adne poniewa¿

Nie jestem tym, który pisa³ GUI. 1. GUI nie jest ukoñczone. 2. Mogê siê myliæ. 3. A wiêc nie b±d¼ zaskoczony je¶li co¶ nie bêdzie dzia³aæ tak, jak przedstawiono tutaj.

Podziêkowania Zoltánowi Ponekkerowi za jego pomoc.

MPlayer - Odtwarzacz filmów dla LINUKSA

C.2.5. Problemy z wyj¶ciem video 114

András Mohari <mayday@freemail.hu>

D.1. Wstêp

W zasadzie nie ma to ¿adnego zwi±zku z formatem skórki, ale powiniene¶ wiedzieæ, ¿e MPlayer nie posiada wbudowanej skórki, w zwi±zku z tym co najmniej jedna skórka musi byæ zainstalowana, aby by³a mo¿liwo¶æ u¿ywania GUI.

D.1.1. Katalogi

Skórki s± szukane w nastêpuj±cych katalogach (w kolejno¶ci):

$(DATADIR)/Skin/

1.

$(PREFIX)/share/mplayer/Skin/

2.

~/.mplayer/Skin/

3. Zauwa¿, ¿e pierwsza ¶cie¿ka mo¿e siê ró¿niæ w zale¿no¶ci od sposobu w jaki MPlayer by³ skonfigurowany (zobacz argumenty --prefix oraz --datadir w skrypcie configure).

Ka¿da skórka jest instalowana w swoim w³asnym katalogu, w jednym z katalogów wy¿ej wymienionych, na przyk³ad:

$(PREFIX)/share/mplayer/Skin/default/

D.1.2. Formaty obrazków

Obrazki musz± byæ w formacie PNG truecolor (24 lub 32 bpp).

W g³ównym oknie oraz na panelu odtwarzania (zobacz ni¿ej) mo¿esz u¿yæ obrazków z 'przezroczysto¶ci±': obszary wype³nione kolorem #FF00FF (magenta) s± w pe³ni przezroczyste dla MPlayera. Oznacza to, ¿e mo¿esz mieæ okna o ró¿nych kszta³tach je¶li Twój X Server posiada rozszerzenie XShape.

D.1.3. Sk³adniki skórki

Skórki s± ca³kowicie konfigurowalne (w odró¿nieniu od skórek np. Winampa/XMMS), a wiêc zale¿y to od Ciebie, czy stworzysz co¶ wspania³ego.

W chwili obecnej mamy trzy okna, które mo¿na ozdobiæ: okno g³ówne (main window), okno ekranu (subwindow), panel odtwarzania (playbar), menu skórki (skin menu) (które mo¿e byæ aktywowane prawym przyciskiem myszy).

Okno g³ówne i/lub panel odtwarzania to miejsca, gdzie mo¿na sterowaæ programem MPlayer. T³em tego okna jest obrazek. Ró¿ne elementy mog± (i musz±) byæ umieszczone w tym oknie: przyciski, potencjometry (suwaki) i etykiety. Dla ka¿dego elementu musisz okre¶liæ ich pozycjê oraz rozmiar.

Przycisk ma trzy stany (wci¶niêty, zwolniony, nieaktywny), zatem jego obrazki musz± byæ podzielone na trzy czê¶ci w pionie. Zobacz sekcjê button, by dowiedzieæ siê wiêcej.

•

MPlayer - Odtwarzacz filmów dla LINUKSA

D.1. Wstêp 115

Potencjometr (suwak) (wykorzystywany g³ównie jako pasek przewijania i kontrolka g³o¶no¶ci/balansu) mo¿e sk³adaæ siê z ka¿dej liczby stanów poprzez podzielenie jego obrazka na wiele czê¶ci, z których jedna poprzedza drug±. Zobacz hpotmeter oraz potmeter, by dowiedzieæ siê wiêcej.

Etykiety s± nieco specyficzne: Znaki potrzebne do ich narysowania s± pobierane z pliku graficznego, a znaki umieszczone w pliku graficznym s± opisane przez plik opisu czcionek. Jest to plik, który za pomoc± czystego tekstu okre¶la wspó³rzêdne x, y oraz wielko¶æ ka¿dego znaku umieszczonego na obrazku (plik graficzny i jego plik opisu tworz± razem zestaw czcionek). Zobacz dlabel oraz slabel, by dowiedzieæ siê wiêcej.

Notatka

Wszystkie obrazki mog± byæ ca³kowicie przezroczyste - tak, jak to opisano w sekcji formaty plików graficznych. Je¿eli X Server nie obs³uguje rozszerzenia XShape, to elementy oznaczone jako przezroczyste bêd± czarne. Je¶li chcia³by¶ wykorzystaæ tak± mo¿liwo¶æ, szeroko¶æ obrazka t³a g³ównego okna musi byæ podzielna przez 8. Okno ekranu to miejsce odtwarzania filmu. Mo¿e ono wy¶wietlaæ okre¶lony obrazek je¶li ¿aden film nie jest uruchomiony (to do¶æ nudne mieæ puste okno :-)) Uwaga: przezroczysto¶æ nie jest tutaj dostêpna. •

Menu skórki to po prostu jeden ze sposobów na kontrolowanie MPlayera poprzez wpisy w menu. Dwa obrazki s± wymagane dla tego menu: pierwszy z nich jest obrazkiem podstawowym, który pokazuje zwyk³y stan menu, drugi za¶ s³u¿y do wy¶wietlenia zaznaczonych obszarów. Gdy uaktywnisz menu, zostanie pokazany pierwszy obrazek. Je¶li przesuniesz mysz nad który¶ z jego wpisów, wówczas zaznaczony element jest kopiowany z drugiego obrazka w miejsce, na które wskazuje kursor myszy (drugi obrazek nigdy nie jest wy¶wietlany jako ca³o¶æ).

Wpis w menu jest okre¶lony przez jego pozycjê oraz rozmiar na obrazku (zobacz sekcjê menu skórki by dowiedzieæ siê wiêcej).

•

Jedna wa¿na sprawa, która nie zosta³a jeszcze powiedziana: MPlayer musi wiedzieæ co zrobiæ w momencie klikniêcia na przyciski, potencjometry i wpisy w menu, aby zadzia³a³y. Zosta³o to zrobione za pomoc± sygna³ów (zdarzeñ). Dla tych elementów musisz zdefiniowaæ sygna³y, które maj± byæ generowane podczas ich klikniêcia.

D.1.4. Pliki

Potrzebne s± nastêpuj±ce pliki podczas tworzenia skórki:

Plik konfiguracyjny o nazwie skin, mówi±cy programowi MPlayer jak po³±czyæ ró¿ne czê¶ci skórki razem i co zrobiæ, gdy nast±pi klikniêcie w którym¶ obszarze okna. • Plik graficzny t³a w oknie g³ównym. • Obrazki dla elementów w g³ównym oknie (zawieraj±ce jeden lub wiêcej plików opisu czcionek, potrzebnych do rysowania etykiet). • Obrazek wy¶wietlany w oknie ekranu (opcjonalnie) • Dwa obrazki dla menu skórki (potrzebne s± tylko wtedy, gdy chcesz tworzyæ takie menu). • Za wyj±tkiem pliku konfiguracyjnego skórki mo¿esz nazwaæ wszystkie pliki tak, jak tego chcesz (ale we¼ pod uwagê, ¿e pliki opisu czcionek musz± mieæ rozszerzenie .fnt ).

MPlayer - Odtwarzacz filmów dla LINUKSA

D.2. Plik skin

Jak zosta³o powiedziane wcze¶niej, plik ten jest plikiem konfiguruj±cym skórkê. Obs³uguje ró¿ne rodzaje wierszy; komentarze zaczynaj± wiersz znakiem ';' (tylko spacje i znaki tabulacji s± dopuszczone przed ';').

Plik podzielony jest na sekcje. Ka¿da sekcja opisuje skórkê dla ka¿dej aplikacji i ma nastêpuj±c± formê:

section = nazwa sekcji
.
.
.
end

Obecnie jest tylko jedna aplikacja, a wiêc potrzebujesz tylko jedn± sekcjê 'section': nazwa tej sekcji to movieplayer.

Wewn±trz tej sekcji ka¿de z okien jest opisane przez blok nastêpuj±cej postaci:

window = nazwa okna
.
.
.
end

gdzie nazwa oknamo¿e byæ jednym z poni¿szych ³añcuchów:

main - dla okna g³ównego • sub - dla okna ekranu • menu - dla menu skórki • playbar - dla panelu odtwarzania • (Bloki sub i menu s± opcjonalne - nie musisz tworzyæ menu czy elementów skórki dla okna ekranu)

Wewn±trz bloku 'window' mo¿esz definiowaæ ka¿dy element okna wpisuj±c linijkê tej postaci:

item = parametr

Gdzie item jest ³añcuchem, kóry identyfikuje typ elementu GUI, parametr jest warto¶ci± numeryczn± lub tekstow± (lub list± takich warto¶ci oddzielonych od siebie znakiem przecinka).

Z³o¿enie powy¿szych elementów razem tworzy plik, który wygl±da mniej wiêcej tak:

section = movieplayer
  window = main
  ; ... elementy okna g³ównego ...
  end

  window = sub
  ; ... elementy okna ekranu ...
  end

  window = menu
  ; ... elementy menu skórki ...
  end

MPlayer - Odtwarzacz filmów dla LINUKSA

D.2. Plik skin 117

  window = playbar
  ; ... elementy panelu odtwarzania ...
  end
end

Nazwa pliku graficznego musi zostaæ podana bez ¿adnych nazw katalogów - obrazki s± szukane w katalogu

Skin. Mo¿esz (ale nie musisz) okre¶liæ rozszerzenia tego pliku. Je¶li plik taki nie istnieje, MPlayer próbuje

wczytaæ plik <nazwa pliku>.<rozszerzenie>, gdzie png oraz PNG s± próbowane jako

<rozszerzenie> (w tej w³a¶nie kolejno¶ci). Pierwszy pasuj±cy plik bêdzie u¿yty.

Na koniec kilka s³ów na temat pozycjonowania. Okno g³ówne oraz okno ekranu mo¿e zostaæ umieszczone w ró¿nych naro¿nikach ekranu poprzez ustawienie wspó³rzêdnych X i Y. 0 to góra lub lewa strona, -1 to ¶rodek, -2 to strona prawa lub dó³, tak jak przedstawiono na poni¿szej ilustracji:

(0, 0)----(-1, 0)----(-2, 0)
  |          |          |
  |          |          |
(0,-1)----(-1,-1)----(-2,-1)
  |          |          |
  |          |          |
(0,-2)----(-1,-2)----(-2,-2)

Oto przyk³ad wyja¶niaj±cy to lepiej. Przypu¶æmy, ¿e masz obrazek nazwany main.png, który zosta³ u¿yty dla okna g³ównego:

base = main, -1, -1

MPlayer próbuje wczytaæ pliki main, main.png, main.PNG.

D.2.1. Okno g³ówne i panel odtwarzania

Poni¿ej znajduje siê lista wpisów, które mog± byæ u¿yte w blokach 'window = main'...'end', oraz 'window = playbar' ... 'end'.

base = obrazek, X, Y

Pozwala okre¶liæ obrazek t³a, który bêdzie u¿ywany w oknie g³ównym Okno bêdzie widoczne w pozycji X, Y na ekranie. Okno bêdzie wielko¶ci tego obrazka.

Notatka

Wspó³rzêdne te nie dzia³aj± na razie dla okna ekranu.

Ostrze¿enie

Obszary przezroczysto¶ci obrazka (kolor #FF00FF) bêd± widoczne jako czarne pod X serwerami nieposiadaj±cymi rozszerzenia XShape. Szeroko¶æ obrazka musi byæ podzielna przez 8.

button = obrazek, X, Y, szeroko¶æ, wysoko¶æ, sygna³

Umieszcza przycisk o rozmiarze szeroko¶æ * wysoko¶æ w pozycji X, Y. Okre¶lony sygna³ jest generowany podczas klikniêcia na przycisk. Obrazek ten opisany przez obrazek musi sk³adaæ siê z trzech czê¶ci jedna pod drug± (stosownie do mo¿liwych stanów przycisku), w ten oto sposób:

+---------------+
|  wci¶niêty    |

MPlayer - Odtwarzacz filmów dla LINUKSA

D.2.1. Okno g³ówne i panel odtwarzania 118

       +---------------+
       |  zwolniony    |
       +---------------+
       | nieaktywny    |
       +---------------+

decoration = enable|disable (w³±czona|wy³aczona)

W³±cza lub wy³±cza dekoracjê mened¿era okna w oknie g³ównym. Domy¶lnie jest wy³±czona.

Notatka

Nie dzia³a to w oknie ekranu, gdy¿ nie ma takiej potrzeby.

hpotmeter = przycisk, szer_przycisku, wys_przycisku, faza, liczba_faz,
domy¶lny, X, Y, szeroko¶æ, wysoko¶æ, sygna³
vpotmeter = przycisk, szer_przycisku, wys_przycisku, fazy, liczba_faz,
domy¶lny, X, Y, szeroko¶æ, wysoko¶æ, sygna³

Umieszcza poziomo (hpotmeter) lub pionowo (vpotmeter) suwak o rozmiarze szeroko¶æ *

wysoko¶æ i pozycji X,Y. Obrazek mo¿e byæ podzielony na ró¿ne czê¶ci dla ró¿nych faz suwaka

(np. mo¿esz mieæ suwak g³o¶no¶ci, który w zale¿no¶ci od po³o¿enia zmienia kolor z zielonego (minimum) na czerwony (maksimum)). hpotmeter mo¿e byæ przyciskiem umieszczonym poziomo. Jego parametry to:

przycisk - obrazek u¿yty do przycisku (musi posiadaæ trzy czê¶ci jedna pod drug± tak,

jak w przypadku przycisku) •

szer_przycisku, wys_przycisku - wielko¶æ przycisku

•

fazy - obrazek u¿ywany do okre¶lenie faz dla hpotmeter. Warto¶æ specjalna NULL mo¿e

byæ u¿yta je¶li nie chcesz ¿adnego obrazka. Obrazek musi byæ podzielony w pionie na

fragmenty poszczególnych faz tak, jak poni¿ej:

+------------+
|  faza #1   |
+------------+
|  faza #2   |
+------------+
     ...
+------------+
|  faza #n   |
+------------+

•

liczba_faz - liczba faz znajduj±ca siê na obrazku z fazami

•

domy¶lny - domy¶lne ustawienie dla hpotmeter (zakres od 0 do 100)

•

X, Y - pozycja dla hpotmeter

•

szeroko¶æ, wysoko¶æ - szeroko¶æ i wysoko¶æ dla hpotmeter

•

sygna³ - sygna³ generowany podczas zmiany warto¶ci hpotmeter

•

potmeter = fazy, liczba_faz, domy¶lny, X, Y, szeroko¶æ, wysoko¶æ, sygna³
     hpotmeter bez przycisku. (domy¶lam siê, ¿e chodzi o to, aby nim krêciæ, ale reaguje on tylko na

poziome przesuwanie). Opis parametrów znajdziesz w czê¶ci o hpotmeter. Parametr fazy mo¿e mieæ warto¶æ NULL, ale jest to zupe³nie bezu¿yteczne, gdy¿ nie widaæ wtedy po³o¿enia potencjometru.

font = plik_czcionek, id_czcionki

Definiuje czcionki. plik_czcionek jest nazw± pliku opisu czcionek z rozszerzeniem .fnt (nie podawaj rozszerzenia w tym miejscu). id_czcionki jest u¿ywany do wskazywania konkretnej czcionki (zobacz dlabel oraz slabel). Mo¿na zdefiniowaæ do 25 czcionek.

slabel = X, Y, id_czcionki, "tekst"

MPlayer - Odtwarzacz filmów dla LINUKSA

Umieszcza statyczn± etykietê w pozycji X,Y. tekst jest wy¶wietlany za pomoc± czcionek wskazywanych przez id_czcionki. Tekst jest po prostu zwyk³ym ³añcuchem znaków (zmienne

$x nie dzia³aj±), które musz± byæ umieszczone pomiêdzy podwójnym cudzys³owem (a znak " nie

mo¿e byæ czê¶ci± tekstu). Etykieta wy¶wietlana jest za pomoc± czcionek, na które wskazuje

     id_czcionki.
dlabel = X, Y, d³ugo¶æ, wyrównanie, id_czcionki, "tekst"

Umieszcza dynamiczn± etykietê w pozycji X,Y. Etykieta jest nazywana dynamiczn± poniewa¿ jej tekst jest cyklicznie od¶wie¿any. Maksymalna d³ugo¶æ etykiety okre¶la parametr d³ugo¶æ (jej wysoko¶æ okre¶la wysoko¶æ czcionek). Je¶li tekst jest szerszy ni¿ zdefiniowana d³ugo¶æ, bêdzie on przewijany, w przeciwnym wypadku bêdzie wyrównany w miejscu okre¶lonym przez warto¶æ parametru wyrównanie: 0 oznacza do prawej, 1 to wy¶rodkowanie, 2 to wyrównanie do lewej.

Wy¶wietlany tekst jest okre¶lony przez zmienn± tekst: musi byæ zawarty pomiêdzy podwójnymi cudzys³owami (a znak " nie mo¿e byæ czê¶ci± tekstu). Etykieta wy¶wietlana jest za pomoc± czcionek, na które wskazuje parametr id_czcionki. Mo¿esz u¿yæ nastêpuj±cych zmiennych w tek¶cie:

Zmienna Znaczenie $1 czas odtwarzania w formacie hh:mm:ss $2 czas odtwarzania w formacie mmmm:ss $3 czas odtwarzania w formacie (godziny) hh $4 czas odtwarzania w formacie (minuty) mm $5 czas odtwarzania w formacie (sekundy) ss $6 d³ugo¶æ filmu w formacie hh:mm:ss $7 d³ugo¶æ filmu w formacie mmmm:ss $8 d³ugo¶æ filmu w formacieh:mm:ss $v format g³o¶no¶ci w %xxx.xx $V format g³o¶no¶ci xxx.xx format $b format balansu w %xxx.xx $B format balansu xxx.xx $$ znak $ $a oznaczenie zgodne z rodzajem typu pliku audio (nic: n, mono: m, stereo: t) $t numer ¶cie¿ki (na li¶cie odtwarzania) $o nazwa pliku $f nazwa pliku pisana ma³ymi literami $F nazwa pliku pisana wielkimi literami

$T oznaczenie zgodne z rodzajem strumienia (plik: f, Video CD: v, DVD: d, URL:

u)

$p znak p (gdy film jest odtwarzany i czcionka ma znak p) $s znak s (gdy film jest zatrzymany i czcionka ma znak s) $e znak e (gdy film jest wstrzymany (pauza) i czcionka ma znak e) $x rozdzielczo¶æ filmu (szeroko¶æ) $y rozdzielczo¶æ filmu (wysoko¶æ) $C nazwa u¿ywanego kodeka

MPlayer - Odtwarzacz filmów dla LINUKSA

Notatka

Zmienne $a, $T, $p, $s oraz $e zwracaj± znaki, które powinny byæ wy¶wietlane jako znaki specjalne (na przyk³ad e jest symbolem pauzy, która z regu³y wygl±da mniej wiêcej tak ||). Powiniene¶ mieæ czcionkê dla zwyk³ych znaków oraz osobn± czcionkê dla symboli. Zobacz sekcjê na temat symboli, by dowiedzieæ siê wiêcej.

D.2.2. Okno ekranu

Poni¿sze wpisy mog± byæ u¿yte w bloku 'window = sub' . . . 'end' .

base = obrazek, X, Y, szeroko¶æ, wysoko¶æ

Wy¶wietla obrazek w oknie. Okno bêdzie widoczne na ekranie w miejscu oznaczonym przez wspó³rzêdne X, Y (0,0 to lewy górny naro¿nik). Mo¿esz u¿yæ -1 dla ¶rodka, -2 dla prawej strony (X) i do³u (Y). Okno bêdzie mieæ wielko¶æ obrazka. szeroko¶æ oraz wysoko¶æ oznaczaj± wielko¶æ okna; s± one opcjonalne (je¶li nie s± okre¶lone, okno bêdzie wielko¶ci takiej, jak obrazek).

background = R, G, B

Pozwala ustawiæ kolor t³a. Jest to u¿yteczne je¶li obrazek jest mniejszy ni¿ okno. R, G oraz B okre¶laj± sk³adniki kolorów czerwonego, zielonego i niebieskiego (ka¿dy z nich jest reprezentowany przez liczbê dziesiêtn± w zakresie od 0 do 255).

D.2.3. Menu skórki

Jak wspomniano wcze¶niej, menu jest wy¶wietlane przy u¿yciu dwóch obrazków. Zwyk³e obszary menu s± pobierane z obrazka okre¶lonego przez element base, podczas gdy obszary zaznaczone s± pobierane z obrazka wskazywanego przez element selected. Musisz zdefiniowaæ pozycjê i rozmiar ka¿dego obszaru menu poprzez element menu.

Poni¿sze wpisy mog± byæ u¿yte w bloku: 'window = menu'. . .'end' .

base = obrazek

Obrazek dla zwyk³ych obszarów menu.

selected = obrazek

Obrazek pokazuj±cy w menu wszystkie zaznaczone obszary.

menu = X, Y, szeroko¶æ, wysoko¶æ, sygna³

Definiuje pozycjê i rozmiar obszarów menu na obrazku przy pomocy X,Y. sygna³ to zdarzenie wygenerowane podczas zwolnienia przycisku myszy nad obszarem.

D.3. Czcionki

Jak wspomniano w sekcji na temat fragmentów skórki, czcionka jest definiowana przez obrazek i plik opisuj±cy. Mo¿esz umie¶ciæ znak gdziekolwiek na obrazku, ale miej pewno¶æ, ¿e jego pozycja i rozmiar jest podana w³a¶ciwie w pliku opisuj±cym.

Plik opisuj±cy czcionki (o rozszerzeniu .fnt) mo¿e posiadaæ linie komentarzy zaczynaj±ce siê znakiem ';'. Plik musi zawieraæ linie w postaci:

image = obrazek

MPlayer - Odtwarzacz filmów dla LINUKSA

Gdzie obrazek jest nazw± pliku graficznego, który zawiera czcionki (nie musisz dopisywaæ jego rozszerzenia).

"char" = X, Y, szeroko¶æ, wysoko¶æ

X oraz Y okre¶laj± pozycjê znaku char na obrazku (0,0 to górny lewy naro¿nik). szeroko¶æ i
wysoko¶æ to rozmiar znaku w pikselach.

Przyk³ad: definiujemy znaki A, B, C przy u¿yciu pliku font.png.

; Mo¿e byæ "font" zamiast "font.png".
image = font.png

; Trzy znaki wystarcz± do tej demonstracji :-)
"A" =  0,0, 7,13
"B" =  7,0, 7,13
"C" = 14,0, 7,13

D.3.1. Znaki specjalne (symbole)

Niektóre znaki maj± specjalne znaczenie, gdy s± zwracane przez pewne zmienne u¿ywane w dlabel. Znaki te mog± byæ wy¶wietlane jako symbole w ten sposób, ¿e np. podczas odtwarzania strumienia DVD widoczne jest ³adne logo zamiast znaku 'd'.

Poni¿sza tablica zawiera znaki u¿ywane do wy¶wietlania symboli (wymagaj± one oddzielnych czcionek).

Znak Symbol p odtwarzanie s stop e pauza n bez d¼wiêku m d¼wiêk mono t d¼wiêk stereo f strumieñ z pliku

v strumieñ z Video CD d strumieñ z DVD u strumieñ z URL

D.4. Sygna³y GUI

Tutaj znajduj± siê sygna³y, które mog± byæ generowane przez przyciski, suwaki i elementy menu.

Notatka

Niektóre sygna³y mog± nie dzia³aæ w oczekiwany sposób (lub nie dzia³aæ w ogóle). Jak wiadomo, GUI jest jeszcze w fazie rozwoju.

Kontrola odtwarzania :

MPlayer - Odtwarzacz filmów dla LINUKSA evNext

Przejd¼ do nastêpnej pozycji na li¶cie odtwarzania. evPause

Tworzy prze³±cznik razem z evPlaySwitchToPause. Mog± byæ u¿yte do utworzenia wspólnego przycisku dla odtwarzania/pauzy. Oba sygna³y powinny byæ powi±zane z przyciskami wy¶wietlonymi w tej samej pozycji w oknie. Sygna³ wstrzymuje wtedy odtwarzanie i wy¶wietlanty jest obrazek dla przycisku evPlaySwitchToPause (aby zaznaczyæ, ¿e przycisk ten mo¿e byæ u¿yty do kontynuowania odtwarzania).

evPlay

Rozpoczyna odtwarzanie. evPlaySwitchToPause Przeciwieñstwo evPauseSwitchToPlay. Ten sygna³ zaczyna odtwarzanie oraz wy¶wietlenie obrazka dla przycisku evPauseSwitchToPlay (aby zaznaczyæ, ¿e przycisk ten mo¿e byæ u¿yty ponownie do wstrzymania odtwarzania).

evPrev

Przejd¼ do poprzedniej pozycji na li¶cie odtwarzania. evStop

Zatrzymuje odtwarzanie.

Przewijanie:

evBackward10sec Przewija do ty³u o 10 sekund.

evBackward1min

Przewija do ty³u o 1 minutê. evBackward10min Przewija do ty³u o 10 minut.

evForward10sec

Przewija do przodu o 10 sekund. evForward1min

Przewija do przodu o 1 minutê. evForward10min

Przewija do przodu o 10 minut.. evSetMoviePosition Przewija do pozycji (mo¿e byæ wykorzystane przez suwak; u¿yte s± wzglêdne warto¶ci (0-100%) suwaka).

Kontrola video:

evDoubleSize

Ustawia podwójny rozmiar okna z filmem. evFullScreen

W³±cza/wy³±cza tryb pe³noekranowy. evNormalSize

Ustawia typowy rozmiar okna z filmem.

Kontrola d¼wiêku:

evDecAudioBufDelay Zmniejsza opó¼nienie bufora d¼wiêku.

evDecBalance

MPlayer - Odtwarzacz filmów dla LINUKSA

Zmniejsza balans. evDecVolume

Zmniejsza g³o¶no¶æ evIncAudioBufDelay Zwiêksza opó¼nienie bufora d¼wiêku.

evIncBalance

Zwiêksza balans. evIncVolume

Zwiêksza g³o¶no¶æ. evMute

Wycisza/przywraca d¼wiêk. evSetBalance

Ustawia balans (mo¿e byæ u¿ywane przez suwak; u¿ywana jest warto¶æ wzglêdna (0-100%)). evSetVolume

Ustawia g³o¶no¶æ (mo¿e byæ u¿ywane przez suwak; u¿ywana jest warto¶æ wzglêdna (0-100%)).

Ró¿ne:

evAbout

Otwiera okno "o programie". evDropSubtitle

Wy³±cza aktualnie u¿ywane napisy. evEqualizer

W³±cza/wy³±cza equalizer. evExit

Wy³±cza program. evIconify

Minimalizuje okno. evLoad

Wczytuje plik (poprzez otwarcie okna przegl±darki plików, gdzie mo¿esz wybraæ plik). evLoadPlay

Robi to samo co evLoad, ale zaczyna automatycznie odtwarzaæ zaraz po wyborze pliku. evLoadSubtitle

Wczytuje plik z napisami (z przegl±darki plików). evLoadAudioFile Wczytuje plik d¼wiêkowy (z przegl±darki plików).

evNone

Sygna³ pusty - nic nie robi (mo¿e za wyj±tkiem wersji z CVS:-)). evPlayList

Otwórz/zamknij okno listy odtwarzania. evPlayDVD

Próbuje odczytaæ p³ytê ze wskazanego czytnika DVD. evPlayVCD

Próbuje odczytaæ p³ytê ze wskazanego czytnika CD. evPreferences

Otwiera okno z ustawieniami. evSetAspect

Ustawia proporcje obrazu. evSetURL

Wy¶wietla okienko dialogowe URL. evSkinBrowser

MPlayer - Odtwarzacz filmów dla LINUKSA

Otwiera okno przegl±darki skórek.

Dodatek E. Developer cries

Spis tre¶ci

E.1. GCC 2.96 E.2. Binary distribution E.3. nVidia E.4. Joe Barr

E.1. GCC 2.96

The background: The GCC 2.95 series is an official GNU release and version 2.95.3 of GCC is the most bug-free in that series. We have never noticed compilation problems that we could trace to gcc-2.95.3. Starting with Red Hat Linux 7.0, Red Hat included a heavily patched CVS version of GCC in their distribution and named it 2.96. Red Hat included this version in the distribution because GCC 3.0 was not finished at the time, and they needed a compiler that worked well on all of their supported platforms, including IA64 and s390. The Linux distributor Mandrake also followed Red Hat's example and started shipping GCC 2.96 with their Linux-Mandrake 8.0 series.

The statements: The GCC team disclaimed any link with GCC 2.96 and issued an official response to GCC 2.96. Many developers around the world began having problems with GCC 2.96, and started recommending other compilers. Examples are MySQL, and avifile. Other interesting links are Linux kernel news flash about kernel 2.4.17 and Voy Forum. MPlayer also suffered from intermittent problems that were all solved by switching to a different version of GCC. Several projects started implementing workarounds for some of the 2.96 issues, but we refused to fix other people's bugs, especially since some workarounds may imply a performance penalty.

GCC 2.96 does not allow | (pipe) characters in assembler comments because it supports Intel as well as AT&T Syntax and the | character is a symbol in the Intel variant. The problem is that it silently ignores the whole assembler block. This is supposedly fixed now, GCC prints a warning instead of skipping the block.

The present: Red Hat says that GCC 2.96-85 and above is fixed. The situation has indeed improved, yet we still see problem reports on our mailing lists that disappear with a different compiler. In any case it does not matter any longer. Hopefully a maturing GCC 3.x will solve the issue for good. If you want to compile with 2.96 give the --disable-gcc-checking flag to configure. Remember that you are on your own and do not report any bugs. If you do, you will only get banned from our mailing list because we have had more than enough flame wars over GCC 2.96. Please let the matter rest.

If you have problems with GCC 2.96, you can get 2.96-85 packages from the Red Hat ftp server, or just go for the 3.0.4 packages offered for version 7.2 and later. You can also get gcc-3.2.3-11 packages (unofficial, but working fine) and you can install them along the gcc-2.96 you already have. MPlayer will detect it and use 3.2 instead of 2.96. If you do not want to or cannot use the binary packages, here is how you can compile GCC 3 from source:

Go to the GCC mirrors page page and download gcc-core-XXX.tar.gz where XXX is the version number. This includes the complete C compiler and is sufficient for MPlayer. If you also want C++, Java or some of the other advanced GCC features gcc-XXX.tar.gz may better suit your needs.

1.

MPlayer - Odtwarzacz filmów dla LINUKSA

Dodatek E. Developer cries 125

Extract the archive with

tar -xvzf gcc-core-XXX.tar.gz

2.

GCC is not built inside the source directory itself like most programs, but needs a build directory outside the source directory. Thus you need to create this directory via

mkdir gcc-build

3.

Then you can proceed to configure gcc in the build directory, but you need the configure from the source directory:

cd gcc-build
../gcc-3.XXX/configure

4.

Compile GCC by issuing this command in the build directory:

make bootstrap

5.

Now you can install GCC (as root) by typing

make install

6.

E.2. Binary distribution

MPlayer previously contained source from the OpenDivX project, which disallows binary redistribution.This code has been removed in version 0.90-pre1 and the remaining file divx_vbr.c that is derived from OpenDivX sources has been put under the GPL by its authors as of version 0.90pre9. You are now welcome to create binary packages as you see fit.

Another impediment to binary redistribution was compiletime optimizations for CPU architecture. MPlayer now supports runtime CPU detection (pass the --enable-runtime-cpudetection to configure). It is disabled by default because it implies a small speed sacrifice, but it is now possible to create binaries that run on different members of the Intel compatible CPU family.

E.3. nVidia

We dislike the fact that nVidia only provides binary drivers (for use with XFree86), which are often buggy. We have had many reports on mplayer-users about problems related to these closed-source drivers and their poor quality, instability and poor user and expert support. Many of these problems/issues keep appearing repeatedly. We have been contacted by nVidia lately, and they said these bugs do not exist, instability is caused by bad AGP chips, and they received no reports of driver bugs (like the purple line). So if you have a problem with your nVidia card, you are advised to update the nVidia driver and/or buy a new motherboard or ask nVidia to supply open-source drivers. In any case, if you are using the nVidia binary drivers and facing driver related problems, please be aware that you will receive very little help from our side because we have little power to help in this matter.

E.4. Joe Barr

Joe Barr became infamous in december 2001 by writing a less than favorable MPlayer review called MPlayer: The project from hell. He found MPlayer hard to install, and concluded that the developers were unfriendly and the documentation incomplete and insulting. You be the judge of that. He went on to mention Arpi negatively in his 10 Linux predictions for 2002. In a followup review of xine called A streaming media player for the rest of us he continued stirring up controversy. Ironically at the end of that article he quotes his

MPlayer - Odtwarzacz filmów dla LINUKSA

E.2. Binary distribution 126 exchange with Günter Bartsch, the original author of xine, that perfectly summarizes the whole situation:

However, he also went on to say that he was "surprised" by my column about MPlayer and thought it was unfair, reminding me that it is a free software project. "If you don't like it," Bartsch said, "you're free not to use it."

Almost two years later in october 2003 he wrote another review called Mplayer revisited. In it he came to the following conclusions:

I would have to say that there have been improvements in the number of features, in performance, and in documentation. It's still not the easiest install in the world, especially for newbies, but it's a little better than it used to be. and But more importantly, I didn't notice any recent comments about user abuse. I think I deserve some of the credit for that, even if I do say so myself. Arpi and the rest of the project team must feel that way too, because they have taken care to remember me in a special section of the documentation included in the tarball. Like I said at the start, some things haven't changed at all.

We could not have summarized our feelings towards Joe Barr better: "It's still not the fairest or best researched article in the world, but it's better than it used to be." Hopefully the next time around we will meet each other's expectations. However, the credit for maturity goes to our increasing age only, and maybe to being weary of flame wars.

Dodatek F. Jak przesy³aæ poprawki (patche)

Proszê przeczytaæ ten plik.

MPlayer - Odtwarzacz filmów dla LINUKSA

Dodatek F. Jak przesy³aæ poprawki (patche) 127